Abbreviations and codes presented in the publication entitled 
"Industrial Two-phase Olive Pomace Slurry-Derived Hydrochar Fuel for Energy Applications."

Abbreviations of samples:
OP = Two phase olive pomace slurry
180-2 = Hydrochar produced at 180 °C with 2 min holding time
180-16 = Hydrochar produced at 180 °C with 16 min holding time
180-30 = Hydrochar produced at 180 °C with 30 min holding time
215-2 = Hydrochar produced at 215 °C with 2 min holding time 
215-16 = Hydrochar produced at 215 °C with 16 min holding time
215-30 = Hydrochar produced at 215 °C with 30 min holding time
250-2 = Hydrochar produced at 250 °C with 2 min holding time
250-16 = Hydrochar produced at 250 °C with 16 min holding time
250-30 = Hydrochar produced at 250 °C with 30 min holding time

Abbreviations of properties analysed for raw material and hydrochars samples: 
E = Extractives obtained by hexane solvent extraction
AIL = Acid insoluble lignin
HY = Hydrochar yield
VM = Volatile matter 
FC = Fixed carbon 
FCI = Fixed carbon index
CDF = Carbon densification factor
HHV = Higher heating value 
EDR = Energy densification ratio
EY = Energy yield
AI = Alkali index 
B/A = Base to acid ratio 
SI = Slagging index 
FI = Fouling index 
SVI = Slag viscosity index
BAI = Bed agglomeration index 
STDEV = Standard deviation			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			
			