File 180-bus 20kV Distribution Grid.xlsx contains the networks parameters and the operating condition of the distribution grid as extracted from PowerFactory using PandaPower export. The files can be readily incorporated in Pandapower and run the corresponding Power Flow.

Note that in the above file the Q-V droop characteristic does not exist. This is a limitation of the Pandapower export. In this analysis, the Q-V droop characteristic proposed in IEEE Std 1547 was used assuming default parameters and Category B PV plants.

Inside the False Data Injection Attacks Folder the following can be found:

1) Attack Configuration Map.xlsx providing an overview of the examined scenarios
2) Noiseless_PF-based_measurements.xlsx containing the outputs of the power flow analysis from PowerFactory including also the Q-V droop characteristic
3) Noisy_measurement.xlsx where noise has been added in the output of the power flow analysis to imitate real-field conditions. This file is used as an input to the derivation of false data injection attacks
4) Attack Configuration folder containing the information used/exploited for the derivation of false data injection attacks.
5) Attack Values folder containing the outputs of the above derivation, i.e. a list of network nodes with v,p,q where some of them (or all depending the examined scenario) has false data.

For more details please contact: stdimoulias@gmail.com
