Normalized flux conditionally averaged based on the topography categories for the near surface source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,  -0.0386,   0.3123
       2,  -0.4133,   0.2302
       3,  -0.2499,   0.2106
       4,   0.1414,   0.1829
       5,   0.6041,   0.1805
       6,   5.2942,   3.5168
       7,   2.5135,   1.7322
       8,   0.7509,   1.5978



Normalized flux conditionally averaged based on the topography categories for the lower canopy source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.1565,   0.3352
       2,  -0.2896,   0.2383
       3,  -0.1420,   0.2225
       4,   0.2950,   0.2167
       5,   0.9693,   0.3424
       6,   4.1683,   1.5427
       7,   2.5778,   1.2810
       8,   0.9055,   1.0535



Normalized flux conditionally averaged based on the topography categories for the middle canopy source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.4931,   0.2997
       2,   0.0462,   0.2482
       3,   0.1671,   0.2357
       4,   0.6670,   0.2604
       5,   1.5066,   0.3461
       6,   2.6366,   0.2423
       7,   1.9632,   0.5323
       8,   1.0235,   0.5292



Normalized flux conditionally averaged based on the topography categories for the upper canopy source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.5907,   0.2671
       2,   0.2175,   0.2416
       3,   0.3643,   0.2314
       4,   0.8833,   0.2607
       5,   1.5861,   0.2148
       6,   2.0652,   0.1192
       7,   1.6557,   0.3191
       8,   1.0389,   0.3714



Normalized flux conditionally averaged based on the topography categories for the near surface source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.0713,   0.4946
       2,  -0.6531,   0.2895
       3,  -0.5337,   0.3041
       4,   0.0610,   0.3024
       5,   0.7817,   0.2218
       6,   2.9887,   1.9102
       7,   4.9291,   1.6860
       8,   1.5374,   1.1874



Normalized flux conditionally averaged based on the topography categories for the lower canopy source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.2261,   0.4874
       2,  -0.5348,   0.2875
       3,  -0.4432,   0.3011
       4,   0.1587,   0.3179
       5,   0.9493,   0.2884
       6,   2.9642,   1.1838
       7,   4.0708,   0.9578
       8,   1.5773,   0.9008



Normalized flux conditionally averaged based on the topography categories for the middle canopy source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.4455,   0.4203
       2,  -0.2610,   0.2915
       3,  -0.2162,   0.3002
       4,   0.3965,   0.3488
       5,   1.3235,   0.3635
       6,   2.7139,   0.4597
       7,   2.8011,   0.3921
       8,   1.4780,   0.5664



Normalized flux conditionally averaged based on the topography categories for the upper canopy source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.5050,   0.3913
       2,  -0.1440,   0.2878
       3,  -0.0882,   0.3046
       4,   0.5252,   0.3585
       5,   1.4673,   0.3564
       6,   2.4956,   0.2985
       7,   2.3977,   0.2825
       8,   1.4318,   0.4642



Normalized flux conditionally averaged based on the topography categories for the near surface source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.4350,   0.7313
       2,  -0.7429,   0.3446
       3,  -0.7339,   0.3515
       4,  -0.0260,   0.3892
       5,   0.8708,   0.3096
       6,   1.9398,   0.5928
       7,   4.6946,   0.5571
       8,   2.5816,   1.0309



Normalized flux conditionally averaged based on the topography categories for the lower canopy source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.5151,   0.6632
       2,  -0.6372,   0.3347
       3,  -0.6508,   0.3404
       4,   0.0405,   0.3947
       5,   0.9597,   0.3515
       6,   2.1728,   0.6142
       7,   4.0427,   0.3313
       8,   2.4272,   0.8274



Normalized flux conditionally averaged based on the topography categories for the middle canopy source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.5817,   0.5383
       2,  -0.4275,   0.3283
       3,  -0.4773,   0.3336
       4,   0.1964,   0.4127
       5,   1.1813,   0.4162
       6,   2.4219,   0.5214
       7,   3.1618,   0.2355
       8,   2.0622,   0.5622



Normalized flux conditionally averaged based on the topography categories for the upper canopy source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   0.5962,   0.4957
       2,  -0.3471,   0.3198
       3,  -0.3887,   0.3364
       4,   0.2821,   0.4206
       5,   1.2890,   0.4347
       6,   2.4313,   0.4524
       7,   2.8527,   0.2357
       8,   1.9295,   0.4777
