Normalized flux conditionally averaged based on the topography categories for the near surface source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.2400,   1.4919
       2,  -0.0430,   1.1693
       3,  -0.3537,   1.0954
       4,  -0.3893,   0.9426
       5,   0.3225,   0.9514
       6,   1.8240,   1.7046
       7,   2.6861,   2.3704
       8,   2.4323,   2.3139



Normalized flux conditionally averaged based on the topography categories for the lower canopy source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.3297,   1.2286
       2,   0.0650,   1.1168
       3,  -0.2788,   1.0537
       4,  -0.3143,   0.9529
       5,   0.4190,   0.9204
       6,   1.8367,   1.2780
       7,   2.4136,   1.6759
       8,   2.2488,   1.6728



Normalized flux conditionally averaged based on the topography categories for the middle canopy source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.3475,   0.8612
       2,   0.2285,   0.9609
       3,  -0.0777,   0.9718
       4,  -0.0717,   0.9803
       5,   0.6568,   0.9076
       6,   1.8684,   0.8973
       7,   1.9832,   0.9804
       8,   1.8092,   0.9675



Normalized flux conditionally averaged based on the topography categories for the upper canopy source and the measurement at 1.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.3076,   0.7863
       2,   0.2452,   0.8963
       3,   0.0135,   0.9357
       4,   0.0816,   1.0098
       5,   0.7762,   0.9245
       6,   1.8704,   0.8292
       7,   1.8324,   0.8468
       8,   1.6321,   0.8313



Normalized flux conditionally averaged based on the topography categories for the near surface source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.5592,   1.3977
       2,  -0.0522,   1.2402
       3,  -0.5111,   1.2108
       4,  -0.6223,   1.1629
       5,   0.2711,   1.0343
       6,   1.8158,   1.2609
       7,   2.5718,   1.8277
       8,   2.6149,   1.9236



Normalized flux conditionally averaged based on the topography categories for the lower canopy source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.5755,   1.2420
       2,   0.0057,   1.1970
       3,  -0.4585,   1.1937
       4,  -0.5681,   1.1659
       5,   0.3263,   1.0250
       6,   1.8715,   1.1528
       7,   2.4456,   1.5122
       8,   2.4556,   1.5816



Normalized flux conditionally averaged based on the topography categories for the middle canopy source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.5199,   1.0592
       2,   0.0677,   1.1329
       3,  -0.3556,   1.1687
       4,  -0.4364,   1.1777
       5,   0.4559,   1.0442
       6,   1.9978,   1.1107
       7,   2.2721,   1.2625
       8,   2.1519,   1.2491



Normalized flux conditionally averaged based on the topography categories for the upper canopy source and the measurement at 1.5 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.4829,   1.0369
       2,   0.0636,   1.1198
       3,  -0.3175,   1.1600
       4,  -0.3675,   1.1910
       5,   0.5188,   1.0666
       6,   2.0476,   1.1246
       7,   2.2113,   1.2342
       8,   2.0413,   1.2035



Normalized flux conditionally averaged based on the topography categories for the near surface source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.7465,   1.2724
       2,   0.0430,   1.2374
       3,  -0.5050,   1.2625
       4,  -0.7016,   1.2404
       5,   0.2523,   1.0361
       6,   1.8012,   1.1054
       7,   2.4013,   1.4262
       8,   2.5879,   1.5846



Normalized flux conditionally averaged based on the topography categories for the lower canopy source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.7240,   1.1828
       2,   0.0640,   1.2053
       3,  -0.4750,   1.2479
       4,  -0.6674,   1.2289
       5,   0.2849,   1.0297
       6,   1.8442,   1.0920
       7,   2.3635,   1.3350
       8,   2.4940,   1.4397



Normalized flux conditionally averaged based on the topography categories for the middle canopy source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.6545,   1.1048
       2,   0.0676,   1.1730
       3,  -0.4373,   1.2365
       4,  -0.6029,   1.2280
       5,   0.3459,   1.0405
       6,   1.9386,   1.1192
       7,   2.3356,   1.3035
       8,   2.3424,   1.3369



Normalized flux conditionally averaged based on the topography categories for the upper canopy source and the measurement at 2.0 canopy height:
Category, Mean normalized flux, Standard deviation
       1,   1.6225,   1.0969
       2,   0.0566,   1.1689
       3,  -0.4230,   1.2313
       4,  -0.5718,   1.2266
       5,   0.3752,   1.0516
       6,   1.9776,   1.1408
       7,   2.3268,   1.3157
       8,   2.2847,   1.3268
