Here are the HR-GNSS data we used in Kheirdast et al. (2021) to derive the source kinematics of Mw6.2, 24/August/2016, Amatrice Earthquake
The manuscript is submitted to JGR: solid-earth
"Neuro-Fuzzy Kinematic Finite-Fault Inversion: 2. Application to the Mw6.2, 24/August/2016, Amatrice Earthquake"

The data is originally processed by Antonio Avallone and located on "ftp://gpsfree.gm.ingv.it/amatrice2016/". 
We upload this data on zenodo to comply with AGU Fair data policy.

To use this data please refer to:

Avallone, A., Latorre, D., Serpelloni, E., Cavaliere, A., Herrero, A., Cecere, G., ... & Selvaggi, G. (2016). Coseismic displacement waveforms for the 2016 August 24 Mw 6.0 Amatrice earthquake (central Italy) carried out from High-Rate GPS data. Annals of Geophysics, 59.

In addition, please cite the following article for RING stations:

Avallone, A., Selvaggi, G., D'Anastasio, E., D'Agostino, N., Pietrantonio, G., Riguzzi, F., ... & Zarrilli, L. (2010). The RING network: improvement of a GPS velocity field in the central Mediterranean. Annals of Geophysics, 53(2), 39-54.

