Upgrades:

Basement Walls (2x4 R12 Frost Wall)

ACH (from 9.26 to 6)

Added code compliance ventilation

Heat Pump

Slab Insulation

U 1.5 SHGC 0.3 Windows

R28 Batts to exposed floors