Three calibration files are provided, covering the data taken during each period of data collection and each including a list of calibrated wavelengths. Where the experimental spectrum is already calibrated, the .csv filename will end with _cubcal, _calibrated, _calib or similar. When this is not present, the correct calibrated wavelengths must be used. The calibrations are assigned as follows:

AliceHoltLower_Autumn18  - 14thFeb

AliceHoltUpper_Autumn18  - 14thFeb
AliceHoltUpper_Spring19  - 14thFeb
AliceHoltUpper_Summer 18 - 14thFeb

AliceHolt_Nov18Blank     - 10thMar
RHULRoof_Nov18Blank      - 10thMar
Sable_19Blank            - 10thMar

RHULRoof_Autumn19        - 10thMar
RHULRoof_Spring19        - 6thJul
RHULRoof_Summer19        - 6thJul
RHULRoof_Winter19        - 14thFeb

SableIsland_Autumn       - 10thMar
SableIsland_Spring       - 10thMar
SableIsland_Winter1819   - 14thFeb
