Case label: SM-35-119. Kosugi model with evaporation. All SWRC parameters fixed. alpha and saturated K log-fitted.                  
Matric potential at air-entry:             -8.2, at the junction point:         -30925.1, and at the corrected oven-dryness point:       -6309758.6.

Matric potential at which the film flow conductivity starts to decrease (h-sub-a):           -200.0.


Number of flexible fitting parameters: 3
Number of complexes: 2, complex size: 7, sub-complex size: 4, nr. of evolution steps: 7.
Trapezoidal probabilities:  0.250      0.214      0.179      0.143      0.107      0.714E-01  0.357E-01

SCEfitting about to be called for run 1.

SCEfitting about to be called for run 2.

SCEfitting about to be called for run 3.

SCEfitting about to be called for run 4.

SCEfitting about to be called for run 5.

SCEfitting about to be called for run 6.

SCEfitting about to be called for run 7.

SCEfitting about to be called for run 8.

SCEfitting about to be called for run 9.

SCEfitting about to be called for run 10.

SCEfitting about to be called for run 11.

SCEfitting about to be called for run 12.

SCEfitting about to be called for run 13.

SCEfitting about to be called for run 14.

SCEfitting about to be called for run 15.

SCEfitting about to be called for run 16.

SCEfitting about to be called for run 17.

SCEfitting about to be called for run 18.

SCEfitting about to be called for run 19.

SCEfitting about to be called for run 20.

SCEfitting about to be called for run 21.

SCEfitting about to be called for run 22.

SCEfitting about to be called for run 23.

SCEfitting about to be called for run 24.

SCEfitting about to be called for run 25.

SCEfitting about to be called for run 26.

SCEfitting about to be called for run 27.

SCEfitting about to be called for run 28.

SCEfitting about to be called for run 29.

SCEfitting about to be called for run 30.

SCEfitting about to be called for run 31.

SCEfitting about to be called for run 32.

SCEfitting about to be called for run 33.

SCEfitting about to be called for run 34.

SCEfitting about to be called for run 35.

SCEfitting about to be called for run 36.

SCEfitting about to be called for run 37.

SCEfitting about to be called for run 38.

SCEfitting about to be called for run 39.

SCEfitting about to be called for run 40.

SCEfitting about to be called for run 41.

SCEfitting about to be called for run 42.

SCEfitting about to be called for run 43.

SCEfitting about to be called for run 44.

SCEfitting about to be called for run 45.

SCEfitting about to be called for run 46.

SCEfitting about to be called for run 47.

SCEfitting about to be called for run 48.

SCEfitting about to be called for run 49.

SCEfitting about to be called for run 50.

Air-entry suction  End of narrow interval    Junction suction  Oven-dry suction (uncorrected)  Correction factor for oven-dry suction
              8.2                    28.2             30925.1                       6303225.2                            1.036520E-03

The number of plotting points of the unsaturated hydraulic conductivity curve is 100.
