{"text_format":"3","workbook":"xlsx","n_sheets":7,"sheets":["Information","Data_Fig2","Data_Fig3","Data_Fig4","Data_Fig5","Data_Fig6","Data_Fig6Breakevenpoints"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Information","index":0,"n_rows":24,"n_cols":14,"rows_kept":24}
[null,"Exploring techno-economic landscapes of abatement options for hard-to-electrify sectors"]
[null,"Data for Figures 2, 4, 5, 6"]
[]
[null,"Clara Bachorz, Philipp C. Verpoort, Gunnar Luderer, Falko Ueckerdt"]
[]
[null,"Annotations",{"$nulls":10},"Case labels (Data for Figure 3)"]
[]
[null,"LCOP","Levelized cost of a product",{"$nulls":9},"normal","No conditions (first figure row)"]
[null,"CAPEX","Capital expenditure",{"$nulls":9},"ccu","CCU coupling is enforced - CCU user requires a CCU source sector (second figure row)"]
[null,"OPEX","Operational expenditure",{"$nulls":9},"comp","Full climate neutrality, compensation only of residual CO2 emissions"]
[null,"FSCP","Fuel-switching CO2 price"]
[null,"NG","Natural gas"]
[null,"H2","Hydrogen (low-emission)"]
[null,"PCI","Pulvarized coal injection"]
[null,"BF-BOF","Blast furnace with a basic oxygen furnace"]
[null,"BF-BOF-CCS","BF-BOF with carbon capture and storage"]
[null,"DRI-EAF-H2","Direct reduction of iron with hydrogen, with an electric arc furnace"]
[null,"HRC","Hot-rolled coil"]
[null,"PAX","person"]
[null,"CCU","Carbon capture and utilization"]
[null,"CDR","Carbon dioxide removal"]
[null,"CaL","Calcium looping (CO2 capture)"]
[null,"MtJ","Methanol-to-jet fuel synthesis"]
[null,"CF","Chemical feedstocks"]

{"sheet":"Data_Fig2","index":1,"n_rows":9,"n_cols":16,"rows_kept":9}
["Technology type","Technology","LCOP \n(EUR/tHRC)","CO2 emissions \n(tCO2/tHRC)","Fuel-switching CO2 price \n(EUR/tCO2)","CAPEX \n(EUR/tHRC)","OPEX \n(EUR/tHRC)","Other OPEX \n(EUR/tHRC)","Iron ore \n(EUR/tHRC)","Scrap steel \n(EUR/tHRC)","Electricy \n(EUR/tHRC)","Fossil NG \n(EUR/tHRC)","H2 \n(EUR/tHRC)","Coking coal \n(EUR/tHRC)","PCI coal \n(EUR/tHRC)","CO2 transport and storage \n(EUR/tHRC)"]
["BF-BOF","Fossil reference",475.66,2,"-",83.78,31.18,70.9,158,30.6,"-",4.28,"-",77.66,19.27,"-"]
["BF-BOF-CCS"," Low CCS-CAPEX assumption",523.76,0.76,38.83,91.64,37.18,78.1,158,30.6,"-",21.6,"-",68.76,19.27,18.6]
[null,"Medium CCS-CAPEX assumption",539.91,0.76,51.87,107.79,37.18,78.1,158,30.6,"-",21.6,"-",68.76,19.27,18.6]
[null," High CCS-CAPEX assumption",556.06,0.76,64.91,123.94,37.18,78.1,158,30.6,"-",21.6,"-",68.76,19.27,18.6]
["DRI-EAF-H2","Hydrogen levelized cost of 50 EUR/MWh",440.28,0.12,-18.74,75.33,18.53,50.7,141,23.4,27.2,11.62,92.5,"-","-","-"]
[null,"Hydrogen levelized cost of 100 EUR/MWh",532.78,0.12,30.25,75.33,18.53,50.7,141,23.4,27.2,11.62,185,"-","-","-"]
[null,"Hydrogen levelized cost of 150 EUR/MWh",625.28,0.12,79.24,75.33,18.53,50.7,141,23.4,27.2,11.62,277.5,"-","-","-"]
[null,"Hydrogen levelized cost of 200 EUR/MWh",717.78,0.12,128.23,75.33,18.53,50.7,141,23.4,27.2,11.62,370,"-","-","-"]

{"sheet":"Data_Fig3","index":2,"n_rows":88936,"n_cols":13,"rows_kept":4500,"cut":true,"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["Sector","Cheapest mitigation option name","Cheapest mitigation option category","LCOP\n(EUR/product-specific unit)","CO2 emissions \n(tCO2/product-specific unit)","H2 cost assumption \n(EUR/MWh)","Non-fossil CO2 cost\nassumption (EUR/tCO2)","CO2 transport and storage assumption (EUR/tCO2)","LCOP of fossil reference\n(EUR/product-specific unit)","CO2 emissions of fossil reference (tCO2/product-specific unit)","Fuel-switching CO2 price\n(EUR/tCO2)","Difference between cheapest and second cheapest FSCP \n(EUR/tCO2) (if not available, given as 1000)","Case (see Information sheet)"]
["Cement","comp","Compensation",75.147303,0,0,0,15,62.166303,0.8654,15,59.54509,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,0,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,0,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,0,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","comp","Compensation",75.147303,0,0,0,15,62.166303,0.8654,15,59.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",492.224697,-0.314,0,0,15,898.391809,4.8184,-79.13785,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.043632,0,0,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-25.27848,1000,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",51.797634,0,0,0,15,126.00477,0.61911,-119.86099,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,0,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",123.202572,0,0,0,15,62.166303,0.8654,70.52955,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",487.514697,0,0,0,15,898.391809,4.8184,-85.27252,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.043632,0,0,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-25.27848,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",51.797634,0,0,0,15,126.00477,0.61911,-119.86099,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",349.502815,0,0,0,15,475.659121,2.00321,-62.97707,1000,"comp"]
["Cement","comp","Compensation",96.782303,0,0,25,15,62.166303,0.8654,40,34.54509,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,25,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,25,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,25,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","comp","Compensation",96.782303,0,0,25,15,62.166303,0.8654,40,34.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",602.992197,-0.314,0,25,15,898.391809,4.8184,-57.55584,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.045761,0,0,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1.67089,38.35443,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",66.797619,0,0,25,15,126.00477,0.61911,-95.63268,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,25,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",124.661572,0,0,25,15,62.166303,0.8654,72.21547,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",590.432197,0,0,25,15,898.391809,4.8184,-63.91325,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.045761,0,0,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1.67089,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",66.797619,0,0,25,15,126.00477,0.61911,-95.63268,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",352.381315,0,0,25,15,475.659121,2.00321,-61.54013,1000,"comp"]
["Cement","comp","Compensation",118.417303,0,0,50,15,62.166303,0.8654,65,9.54509,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,50,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,50,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,50,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","comp","Compensation",118.417303,0,0,50,15,62.166303,0.8654,65,9.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",713.759697,-0.314,0,50,15,898.391809,4.8184,-35.97384,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.04789,0,0,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},28.62025,36.41772,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",81.797604,0,0,50,15,126.00477,0.61911,-71.40438,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,50,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",126.120572,0,0,50,15,62.166303,0.8654,73.9014,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",693.349697,0,0,50,15,898.391809,4.8184,-42.55398,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.04789,0,0,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},28.62025,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",81.797604,0,0,50,15,126.00477,0.61911,-71.40438,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",355.259815,0,0,50,15,475.659121,2.00321,-60.10319,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,75,15,62.166303,0.8654,74.54509,15.4549099999999,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,75,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,75,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,75,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,75,15,62.166303,0.8654,74.54509,15.4549099999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",824.527197,-0.314,0,75,15,898.391809,4.8184,-14.39183,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.050019,0,0,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},55.56962,34.48101,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,75,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,75,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",127.579572,0,0,75,15,62.166303,0.8654,75.58732,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",796.267197,0,0,75,15,898.391809,4.8184,-21.19471,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.050019,0,0,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},55.56962,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,75,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",358.138315,0,0,75,15,475.659121,2.00321,-58.66624,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,100,15,62.166303,0.8654,74.54509,40.45491,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,100,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,100,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,100,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",935.294697,-0.314,0,100,15,898.391809,4.8184,7.19018,107.80982,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.052148,0,0,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},82.51899,32.5442999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,100,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,100,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",129.038572,0,0,100,15,62.166303,0.8654,77.27325,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",899.184697,0,0,100,15,898.391809,4.8184,0.16455,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.052148,0,0,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},82.51899,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,100,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",361.016815,0,0,100,15,475.659121,2.00321,-57.2293,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,125,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,125,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,125,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,125,15,62.166303,0.8654,74.54509,65.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1046.062197,-0.314,0,125,15,898.391809,4.8184,28.77219,111.22781,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.054278,0,0,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},109.48101,30.59494,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,125,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,125,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",130.497572,0,0,125,15,62.166303,0.8654,78.95917,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1002.102197,0,0,125,15,898.391809,4.8184,21.52382,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.054278,0,0,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},109.48101,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,125,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",363.895315,0,0,125,15,475.659121,2.00321,-55.79236,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,150,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,150,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,150,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,150,15,62.166303,0.8654,74.54509,90.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1156.829697,-0.314,0,150,15,898.391809,4.8184,50.3542,114.6458,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.056407,0,0,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},136.43038,28.6582299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,150,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,150,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",131.956572,0,0,150,15,62.166303,0.8654,80.6451,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1105.019697,0,0,150,15,898.391809,4.8184,42.88309,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.056407,0,0,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},136.43038,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,150,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",366.773815,0,0,150,15,475.659121,2.00321,-54.35541,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,175,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,175,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,175,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,175,15,62.166303,0.8654,74.54509,115.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1267.597197,-0.314,0,175,15,898.391809,4.8184,71.93621,118.06379,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.058536,0,0,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},163.37975,26.7215199999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,175,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,175,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",133.415572,0,0,175,15,62.166303,0.8654,82.33102,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1207.937197,0,0,175,15,898.391809,4.8184,64.24236,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.058536,0,0,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},163.37975,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,175,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",369.652315,0,0,175,15,475.659121,2.00321,-52.91847,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,200,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,200,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,200,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,200,15,62.166303,0.8654,74.54509,140.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1378.364697,-0.314,0,200,15,898.391809,4.8184,93.51822,121.48178,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.060665,0,0,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.32911,24.78481,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,200,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,200,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",134.874572,0,0,200,15,62.166303,0.8654,84.01695,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1310.854697,0,0,200,15,898.391809,4.8184,85.60163,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.060665,0,0,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.32911,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,200,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",372.530815,0,0,200,15,475.659121,2.00321,-51.48153,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,225,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,225,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,225,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,225,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,225,15,62.166303,0.8654,74.54509,165.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1489.132197,-0.314,0,225,15,898.391809,4.8184,115.10022,124.89978,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.062794,0,0,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},217.27848,22.8480999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,225,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,225,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",136.333572,0,0,225,15,62.166303,0.8654,85.70288,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1413.772197,0,0,225,15,898.391809,4.8184,106.9609,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.062794,0,0,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},217.27848,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,225,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",375.409315,0,0,225,15,475.659121,2.00321,-50.04458,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,250,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,250,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,250,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,250,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,250,15,62.166303,0.8654,74.54509,190.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1599.899697,-0.314,0,250,15,898.391809,4.8184,136.68223,128.31777,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.064923,0,0,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},244.22785,20.9113899999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,250,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,250,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",137.792572,0,0,250,15,62.166303,0.8654,87.3888,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1516.689697,0,0,250,15,898.391809,4.8184,128.32017,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.064923,0,0,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},244.22785,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,250,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",378.287815,0,0,250,15,475.659121,2.00321,-48.60764,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,275,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,275,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,275,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,275,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,275,15,62.166303,0.8654,74.54509,215.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1710.667197,-0.314,0,275,15,898.391809,4.8184,158.26424,131.73576,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.067052,0,0,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},271.17722,18.97468,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,275,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,275,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",139.251572,0,0,275,15,62.166303,0.8654,89.07473,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1619.607197,0,0,275,15,898.391809,4.8184,149.67943,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.067052,0,0,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},271.17722,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,275,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",381.166315,0,0,275,15,475.659121,2.00321,-47.17069,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,300,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,300,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,300,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,300,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,300,15,62.166303,0.8654,74.54509,240.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1821.434697,-0.314,0,300,15,898.391809,4.8184,179.84625,135.15375,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.069181,0,0,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},298.12658,17.03798,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,300,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,300,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",140.710572,0,0,300,15,62.166303,0.8654,90.76065,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1722.524697,0,0,300,15,898.391809,4.8184,171.0387,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.069181,0,0,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},298.12658,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,300,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",384.044815,0,0,300,15,475.659121,2.00321,-45.73375,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,325,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,325,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,325,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,325,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1932.202197,-0.314,0,325,15,898.391809,4.8184,201.42826,138.57174,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.07131,0,0,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},325.07595,15.10127,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,325,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,325,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",142.169572,0,0,325,15,62.166303,0.8654,92.44658,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1825.442197,0,0,325,15,898.391809,4.8184,192.39797,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.07131,0,0,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},325.07595,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,325,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",386.923315,0,0,325,15,475.659121,2.00321,-44.29681,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,350,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,350,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,350,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,350,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,350,15,62.166303,0.8654,74.54509,290.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2042.969697,-0.314,0,350,15,898.391809,4.8184,223.01027,141.98973,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.073439,0,0,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},352.02532,13.1645499999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,350,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,350,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",143.628572,0,0,350,15,62.166303,0.8654,94.1325,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1928.359697,0,0,350,15,898.391809,4.8184,213.75724,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.073439,0,0,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},352.02532,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,350,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",389.801815,0,0,350,15,475.659121,2.00321,-42.85986,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,375,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,375,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,375,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,375,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,375,15,62.166303,0.8654,74.54509,315.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2153.737197,-0.314,0,375,15,898.391809,4.8184,244.59227,145.40773,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.075568,0,0,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},378.97468,11.22785,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,375,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,375,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",145.087572,0,0,375,15,62.166303,0.8654,95.81843,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2031.277197,0,0,375,15,898.391809,4.8184,235.11651,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.075568,0,0,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},378.97468,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,375,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",392.680315,0,0,375,15,475.659121,2.00321,-41.42292,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,400,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,400,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,400,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,400,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,400,15,62.166303,0.8654,74.54509,340.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2264.504697,-0.314,0,400,15,898.391809,4.8184,266.17428,148.82572,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.077697,0,0,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},405.92405,9.29113999999998,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,400,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,400,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",146.546572,0,0,400,15,62.166303,0.8654,97.50436,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2134.194697,0,0,400,15,898.391809,4.8184,256.47578,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.077697,0,0,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},405.92405,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,400,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",395.558815,0,0,400,15,475.659121,2.00321,-39.98598,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,425,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,425,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,425,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,425,15,62.166303,0.8654,74.54509,365.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2375.272197,-0.314,0,425,15,898.391809,4.8184,287.75629,152.24371,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.079826,0,0,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},432.87342,7.35442999999997,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,425,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,425,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",148.005572,0,0,425,15,62.166303,0.8654,99.19028,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2237.112197,0,0,425,15,898.391809,4.8184,277.83505,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.079826,0,0,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},432.87342,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,425,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",398.437315,0,0,425,15,475.659121,2.00321,-38.54903,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,450,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,450,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,450,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,450,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,450,15,62.166303,0.8654,74.54509,390.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2486.039697,-0.314,0,450,15,898.391809,4.8184,309.3383,155.6617,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.081956,0,0,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},459.83544,5.40506999999996,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,450,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,450,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",149.464572,0,0,450,15,62.166303,0.8654,100.87621,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2340.029697,0,0,450,15,898.391809,4.8184,299.19432,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.081956,0,0,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},459.83544,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,450,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",401.315815,0,0,450,15,475.659121,2.00321,-37.11209,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,475,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,475,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,475,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,475,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2596.807197,-0.314,0,475,15,898.391809,4.8184,330.92031,159.07969,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.084085,0,0,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},486.78481,3.46834999999998,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,475,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,475,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",150.923572,0,0,475,15,62.166303,0.8654,102.56213,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2442.947197,0,0,475,15,898.391809,4.8184,320.55358,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.084085,0,0,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},486.78481,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,475,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",404.194315,0,0,475,15,475.659121,2.00321,-35.67514,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,500,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,500,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,500,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,500,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,500,15,62.166303,0.8654,74.54509,440.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2707.574697,-0.314,0,500,15,898.391809,4.8184,352.50232,162.49768,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.086214,0,0,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},513.73418,1.53163999999992,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,500,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,500,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",152.382572,0,0,500,15,62.166303,0.8654,104.24806,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2545.864697,0,0,500,15,898.391809,4.8184,341.91285,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.086214,0,0,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},513.73418,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,500,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",407.072815,0,0,500,15,475.659121,2.00321,-34.2382,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,525,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,525,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,525,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,525,15,62.166303,0.8654,74.54509,465.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2818.342197,-0.314,0,525,15,898.391809,4.8184,374.08432,165.91568,"ccu"]
["Aviation","comp","Compensation",0.088311,0,0,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,0.405060000000048,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,525,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,525,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",153.841572,0,0,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2648.782197,0,0,525,15,898.391809,4.8184,363.27212,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.088343,0,0,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.68354,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,525,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",409.951315,0,0,525,15,475.659121,2.00321,-32.80126,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,550,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,550,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,550,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,550,15,62.166303,0.8654,74.54509,490.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2929.109697,-0.314,0,550,15,898.391809,4.8184,395.66633,169.333669999999,"ccu"]
["Aviation","comp","Compensation",0.090287,0,0,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,2.34176999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,550,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,550,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",155.300572,0,0,550,15,62.166303,0.8654,107.61991,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2751.699697,0,0,550,15,898.391809,4.8184,384.63139,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.090472,0,0,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},567.63291,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,550,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",412.829815,0,0,550,15,475.659121,2.00321,-31.36431,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,575,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,575,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,575,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,575,15,62.166303,0.8654,74.54509,515.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3039.877197,-0.314,0,575,15,898.391809,4.8184,417.24834,172.75166,"ccu"]
["Aviation","comp","Compensation",0.092263,0,0,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,4.27847999999994,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,575,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,575,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",156.759572,0,0,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2854.617197,0,0,575,15,898.391809,4.8184,405.99066,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.092601,0,0,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},594.58228,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,575,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",415.708315,0,0,575,15,475.659121,2.00321,-29.92737,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,600,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,600,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,600,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,600,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,600,15,62.166303,0.8654,74.54509,540.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3150.644697,-0.314,0,600,15,898.391809,4.8184,438.83035,176.16965,"ccu"]
["Aviation","comp","Compensation",0.094239,0,0,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,6.21519,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,600,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,600,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",158.218572,0,0,600,15,62.166303,0.8654,110.99176,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2957.534697,0,0,600,15,898.391809,4.8184,427.34993,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.09473,0,0,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},621.53165,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,600,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",418.586815,0,0,600,15,475.659121,2.00321,-28.49043,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,625,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,625,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,625,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,625,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3261.412197,-0.314,0,625,15,898.391809,4.8184,460.41236,179.58764,"ccu"]
["Aviation","comp","Compensation",0.096215,0,0,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,8.15189999999995,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,625,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,625,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",159.677572,0,0,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3060.452197,0,0,625,15,898.391809,4.8184,448.7092,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.096859,0,0,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},648.48101,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,625,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",421.465315,0,0,625,15,475.659121,2.00321,-27.05348,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,650,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,650,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,650,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,650,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,650,15,62.166303,0.8654,74.54509,590.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3372.179697,-0.314,0,650,15,898.391809,4.8184,481.99437,183.00563,"ccu"]
["Aviation","comp","Compensation",0.098191,0,0,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,10.08861,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,650,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,650,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",161.136572,0,0,650,15,62.166303,0.8654,114.36361,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3163.369697,0,0,650,15,898.391809,4.8184,470.06846,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.098988,0,0,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},675.43038,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,650,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",424.343815,0,0,650,15,475.659121,2.00321,-25.61654,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,675,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,675,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,675,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,675,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,675,15,62.166303,0.8654,74.54509,615.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3482.947197,-0.314,0,675,15,898.391809,4.8184,503.57638,186.42362,"ccu"]
["Aviation","comp","Compensation",0.100167,0,0,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,12.0253199999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,675,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,675,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",162.595572,0,0,675,15,62.166303,0.8654,116.04954,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3266.287197,0,0,675,15,898.391809,4.8184,491.42773,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.101117,0,0,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},702.37975,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,675,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",427.222315,0,0,675,15,475.659121,2.00321,-24.17959,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,700,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,700,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,700,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,700,15,62.166303,0.8654,74.54509,640.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3593.714697,-0.314,0,700,15,898.391809,4.8184,525.15838,189.84162,"ccu"]
["Aviation","comp","Compensation",0.102143,0,0,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,13.96202,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,700,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,700,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",164.054572,0,0,700,15,62.166303,0.8654,117.73546,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3369.204697,0,0,700,15,898.391809,4.8184,512.787,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.103246,0,0,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},729.32911,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,700,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",430.100815,0,0,700,15,475.659121,2.00321,-22.74265,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,725,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,725,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,725,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,725,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,725,15,62.166303,0.8654,74.54509,665.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3704.482197,-0.314,0,725,15,898.391809,4.8184,546.74039,193.259609999999,"ccu"]
["Aviation","comp","Compensation",0.104119,0,0,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,15.89873,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,725,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,725,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",165.513572,0,0,725,15,62.166303,0.8654,119.42139,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3472.122197,0,0,725,15,898.391809,4.8184,534.14627,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.105375,0,0,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},756.27848,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,725,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",432.979315,0,0,725,15,475.659121,2.00321,-21.30571,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,750,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,750,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,750,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3815.249697,-0.314,0,750,15,898.391809,4.8184,568.3224,196.677599999999,"ccu"]
["Aviation","comp","Compensation",0.106095,0,0,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,17.8354399999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,750,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,750,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",166.972572,0,0,750,15,62.166303,0.8654,121.10731,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3575.039697,0,0,750,15,898.391809,4.8184,555.50554,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.107504,0,0,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},783.22785,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,750,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",435.857815,0,0,750,15,475.659121,2.00321,-19.86876,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,775,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,775,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,775,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3926.017197,-0.314,0,775,15,898.391809,4.8184,589.90441,200.09559,"ccu"]
["Aviation","comp","Compensation",0.108071,0,0,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,19.7848099999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,775,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,775,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",168.431572,0,0,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3677.957197,0,0,775,15,898.391809,4.8184,576.86481,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.109634,0,0,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},810.18987,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,775,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",438.736315,0,0,775,15,475.659121,2.00321,-18.43182,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,800,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,800,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,800,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,800,15,62.166303,0.8654,74.54509,740.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4036.784697,-0.314,0,800,15,898.391809,4.8184,611.48642,203.51358,"ccu"]
["Aviation","comp","Compensation",0.110047,0,0,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,21.7215199999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,800,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,800,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",169.890572,0,0,800,15,62.166303,0.8654,124.47916,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3780.874697,0,0,800,15,898.391809,4.8184,598.22408,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.111763,0,0,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},837.13924,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,800,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",441.614815,0,0,800,15,475.659121,2.00321,-16.99488,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,825,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,825,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,825,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,825,15,62.166303,0.8654,74.54509,765.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4147.552197,-0.314,0,825,15,898.391809,4.8184,633.06843,206.931569999999,"ccu"]
["Aviation","comp","Compensation",0.112023,0,0,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,23.65823,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,825,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,825,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",171.349572,0,0,825,15,62.166303,0.8654,126.16509,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3883.792197,0,0,825,15,898.391809,4.8184,619.58334,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.113892,0,0,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},864.08861,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,825,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",444.493315,0,0,825,15,475.659121,2.00321,-15.55793,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,850,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,850,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,850,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,850,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,850,15,62.166303,0.8654,74.54509,790.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4258.319697,-0.314,0,850,15,898.391809,4.8184,654.65043,210.349569999999,"ccu"]
["Aviation","comp","Compensation",0.113999,0,0,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,25.5949299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,850,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,850,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",172.808572,0,0,850,15,62.166303,0.8654,127.85102,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3986.709697,0,0,850,15,898.391809,4.8184,640.94261,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.116021,0,0,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},891.03797,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,850,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",447.371815,0,0,850,15,475.659121,2.00321,-14.12099,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,875,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,875,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,875,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,875,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,875,15,62.166303,0.8654,74.54509,815.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4369.087197,-0.314,0,875,15,898.391809,4.8184,676.23244,213.76756,"ccu"]
["Aviation","comp","Compensation",0.115975,0,0,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,27.53164,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,875,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,875,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",174.267572,0,0,875,15,62.166303,0.8654,129.53694,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4089.627197,0,0,875,15,898.391809,4.8184,662.30188,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.11815,0,0,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},917.98734,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,875,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",450.250315,0,0,875,15,475.659121,2.00321,-12.68405,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,900,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,900,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,900,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,900,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,900,15,62.166303,0.8654,74.54509,840.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4479.854697,-0.314,0,900,15,898.391809,4.8184,697.81445,217.18555,"ccu"]
["Aviation","comp","Compensation",0.117951,0,0,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,29.4683599999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,900,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,900,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",175.726572,0,0,900,15,62.166303,0.8654,131.22287,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4192.544697,0,0,900,15,898.391809,4.8184,683.66115,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.120279,0,0,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},944.93671,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,900,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",453.128815,0,0,900,15,475.659121,2.00321,-11.2471,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,925,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,925,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,925,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,925,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,925,15,62.166303,0.8654,74.54509,865.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4590.622197,-0.314,0,925,15,898.391809,4.8184,719.39646,220.603539999999,"ccu"]
["Aviation","comp","Compensation",0.119927,0,0,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},940.48101,31.40507,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,925,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,925,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",177.185572,0,0,925,15,62.166303,0.8654,132.90879,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4295.462197,0,0,925,15,898.391809,4.8184,705.02042,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.122408,0,0,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},971.88608,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,925,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",456.007315,0,0,925,15,475.659121,2.00321,-9.81016,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,950,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,950,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,950,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,950,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,950,15,62.166303,0.8654,74.54509,890.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4701.389697,-0.314,0,950,15,898.391809,4.8184,740.97847,224.021529999999,"ccu"]
["Aviation","comp","Compensation",0.121903,0,0,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},965.49367,33.34177,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,950,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,950,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",178.644572,0,0,950,15,62.166303,0.8654,134.59472,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4398.379697,0,0,950,15,898.391809,4.8184,726.37969,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.124537,0,0,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},998.83544,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,950,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",458.885815,0,0,950,15,475.659121,2.00321,-8.37321,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,975,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,975,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,975,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,975,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,975,15,62.166303,0.8654,74.54509,915.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4812.157197,-0.314,0,975,15,898.391809,4.8184,762.56048,227.43952,"ccu"]
["Aviation","comp","Compensation",0.123879,0,0,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},990.50633,35.27848,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,975,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,975,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",180.103572,0,0,975,15,62.166303,0.8654,136.28064,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4501.297197,0,0,975,15,898.391809,4.8184,747.73896,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.126666,0,0,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1025.78481,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,975,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",461.764315,0,0,975,15,475.659121,2.00321,-6.93627,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1000,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1000,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1000,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1000,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1000,15,62.166303,0.8654,74.54509,940.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4922.924697,-0.314,0,1000,15,898.391809,4.8184,784.14248,230.85752,"ccu"]
["Aviation","comp","Compensation",0.125855,0,0,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,37.2151899999998,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1000,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1000,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",181.562572,0,0,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4604.214697,0,0,1000,15,898.391809,4.8184,769.09823,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.128795,0,0,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1052.73418,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1000,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",464.642815,0,0,1000,15,475.659121,2.00321,-5.49933,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1025,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1025,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1025,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1025,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1025,15,62.166303,0.8654,74.54509,965.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5033.692197,-0.314,0,1025,15,898.391809,4.8184,805.72449,234.27551,"ccu"]
["Aviation","comp","Compensation",0.127831,0,0,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,39.15189,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1025,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1025,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",183.021572,0,0,1025,15,62.166303,0.8654,139.65249,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4707.132197,0,0,1025,15,898.391809,4.8184,790.45749,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.130924,0,0,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1079.68354,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1025,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",467.521315,0,0,1025,15,475.659121,2.00321,-4.06238,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1050,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1050,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1050,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1050,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1050,15,62.166303,0.8654,74.54509,990.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5144.459697,-0.314,0,1050,15,898.391809,4.8184,827.3065,237.693499999999,"ccu"]
["Aviation","comp","Compensation",0.129807,0,0,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,41.08861,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1050,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1050,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",184.480572,0,0,1050,15,62.166303,0.8654,141.33842,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4810.049697,0,0,1050,15,898.391809,4.8184,811.81676,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.133053,0,0,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1106.63291,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1050,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",470.399815,0,0,1050,15,475.659121,2.00321,-2.62544,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1075,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1075,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1075,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1075,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1075,15,62.166303,0.8654,74.54509,1015.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5255.227197,-0.314,0,1075,15,898.391809,4.8184,848.88851,241.11149,"ccu"]
["Aviation","comp","Compensation",0.131783,0,0,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,43.0253200000001,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1075,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1075,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",185.939572,0,0,1075,15,62.166303,0.8654,143.02435,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4912.967197,0,0,1075,15,898.391809,4.8184,833.17603,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.135182,0,0,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1133.58228,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1075,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",473.278315,0,0,1075,15,475.659121,2.00321,-1.1885,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1100,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1100,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1100,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1100,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1100,15,62.166303,0.8654,74.54509,1040.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5365.994697,-0.314,0,1100,15,898.391809,4.8184,870.47052,244.52948,"ccu"]
["Aviation","comp","Compensation",0.133759,0,0,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,44.97468,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1100,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1100,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",187.398572,0,0,1100,15,62.166303,0.8654,144.71027,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5015.884697,0,0,1100,15,898.391809,4.8184,854.5353,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.137312,0,0,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1160.5443,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1100,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",476.156815,0,0,1100,15,475.659121,2.00321,0.24845,457.35657,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1125,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1125,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1125,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1125,15,62.166303,0.8654,74.54509,1065.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5476.762197,-0.314,0,1125,15,898.391809,4.8184,892.05253,247.947469999999,"ccu"]
["Aviation","comp","Compensation",0.135735,0,0,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1140.58228,46.9113899999999,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1125,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1125,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",188.857572,0,0,1125,15,62.166303,0.8654,146.3962,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5118.802197,0,0,1125,15,898.391809,4.8184,875.89457,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.139441,0,0,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1187.49367,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1125,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",479.035315,0,0,1125,15,475.659121,2.00321,1.68539,465.46069,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1150,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1150,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1150,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1150,15,62.166303,0.8654,74.54509,1090.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5587.529697,-0.314,0,1150,15,898.391809,4.8184,913.63454,251.365459999999,"ccu"]
["Aviation","comp","Compensation",0.137711,0,0,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1165.59494,48.8481000000001,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1150,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1150,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",190.316572,0,0,1150,15,62.166303,0.8654,148.08212,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5221.719697,0,0,1150,15,898.391809,4.8184,897.25384,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.14157,0,0,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1214.44304,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1150,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",481.913815,0,0,1150,15,475.659121,2.00321,3.12234,473.564809999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1175,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1175,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1175,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1175,15,62.166303,0.8654,74.54509,1115.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5698.297197,-0.314,0,1175,15,898.391809,4.8184,935.21654,254.78346,"ccu"]
["Aviation","comp","Compensation",0.139687,0,0,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,50.7848199999998,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1175,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1175,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",191.775572,0,0,1175,15,62.166303,0.8654,149.76805,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5324.637197,0,0,1175,15,898.391809,4.8184,918.61311,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.143699,0,0,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1241.39241,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1175,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",484.792315,0,0,1175,15,475.659121,2.00321,4.55928,481.66893,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,0,1200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",492.224697,1.90135,0,1200,15,898.391809,4.8184,-139.239,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.043632,{"v":4.3e-05,"d":"4.30E-05"},0,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-55.47222,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",51.797634,0.3,0,1200,15,126.00477,0.61911,-232.54406,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1200,15,475.659121,2.00321,-67.73234,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,0,1200,15,62.166303,0.8654,74.54509,1140.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5809.064697,-0.314,0,1200,15,898.391809,4.8184,956.79855,258.20145,"ccu"]
["Aviation","comp","Compensation",0.141663,0,0,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,52.72152,"ccu"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1200,15,126.00477,0.61911,-58.54283,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",347.775715,0.11514,0,1200,15,475.659121,2.00321,-67.73234,1000,"ccu"]
["Cement","ccs","CCS",193.23457200000001,0,0,1200,15,62.166303,0.8654,151.45397,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5427.554697,0,0,1200,15,898.391809,4.8184,939.97237,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.145828,0,0,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1268.34177,1000,"comp"]
["Maritime","h2","Low-emission ammonia",89.760317,0,0,1200,15,126.00477,0.61911,-58.54283,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",487.670815,0,0,1200,15,475.659121,2.00321,5.99622,489.77305,"comp"]
["Cement","comp","Compensation",75.147303,0,2,0,15,62.166303,0.8654,15,59.54509,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,0,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,0,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,0,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","comp","Compensation",75.147303,0,2,0,15,62.166303,0.8654,15,59.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",532.593297,-0.314,2,0,15,898.391809,4.8184,-71.27241,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.044454,0,2,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-14.87342,1000,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",57.264295,0,2,0,15,126.00477,0.61911,-111.03112,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,0,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",123.202572,0,2,0,15,62.166303,0.8654,70.52955,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",527.883297,0,2,0,15,898.391809,4.8184,-76.89451,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.044454,0,2,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-14.87342,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",57.264295,0,2,0,15,126.00477,0.61911,-111.03112,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",353.202815,0,2,0,15,475.659121,2.00321,-61.13004,1000,"comp"]
["Cement","comp","Compensation",96.782303,0,2,25,15,62.166303,0.8654,40,34.54509,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,25,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,25,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,25,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","comp","Compensation",96.782303,0,2,25,15,62.166303,0.8654,40,34.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",643.360797,-0.314,2,25,15,898.391809,4.8184,-49.6904,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.046583,0,2,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},12.07595,27.94937,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",72.26428,0,2,25,15,126.00477,0.61911,-86.80281,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,25,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",124.661572,0,2,25,15,62.166303,0.8654,72.21547,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",630.800797,0,2,25,15,898.391809,4.8184,-55.53524,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.046583,0,2,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},12.07595,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",72.26428,0,2,25,15,126.00477,0.61911,-86.80281,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",356.081315,0,2,25,15,475.659121,2.00321,-59.6931,1000,"comp"]
["Cement","comp","Compensation",118.417303,0,2,50,15,62.166303,0.8654,65,9.54509,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,50,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,50,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,50,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","comp","Compensation",118.417303,0,2,50,15,62.166303,0.8654,65,9.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",754.128297,-0.314,2,50,15,898.391809,4.8184,-28.10839,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.048712,0,2,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},39.02532,26.01265,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",87.264265,0,2,50,15,126.00477,0.61911,-62.57451,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,50,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",126.120572,0,2,50,15,62.166303,0.8654,73.9014,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",733.718297,0,2,50,15,898.391809,4.8184,-34.17597,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.048712,0,2,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},39.02532,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",87.264265,0,2,50,15,126.00477,0.61911,-62.57451,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",358.959815,0,2,50,15,475.659121,2.00321,-58.25615,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,75,15,62.166303,0.8654,74.54509,15.4549099999999,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,75,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,75,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,75,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,75,15,62.166303,0.8654,74.54509,15.4549099999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",864.895797,-0.314,2,75,15,898.391809,4.8184,-6.52638,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.050841,0,2,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},65.97468,24.0759499999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,75,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,75,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",127.579572,0,2,75,15,62.166303,0.8654,75.58732,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",836.635797,0,2,75,15,898.391809,4.8184,-12.81671,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.050841,0,2,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},65.97468,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,75,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",361.838315,0,2,75,15,475.659121,2.00321,-56.81921,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,100,15,62.166303,0.8654,74.54509,40.45491,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,100,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,100,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,100,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",975.6632970000001,-0.314,2,100,15,898.391809,4.8184,15.05562,99.94438,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.05297,0,2,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},92.92405,22.13924,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,100,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,100,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",129.038572,0,2,100,15,62.166303,0.8654,77.27325,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",939.553297,0,2,100,15,898.391809,4.8184,8.54256,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.05297,0,2,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},92.92405,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,100,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",364.716815,0,2,100,15,475.659121,2.00321,-55.38226,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,125,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,125,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,125,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,125,15,62.166303,0.8654,74.54509,65.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1086.430797,-0.314,2,125,15,898.391809,4.8184,36.63763,103.36237,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.055099,0,2,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},119.87342,20.20253,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,125,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,125,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",130.497572,0,2,125,15,62.166303,0.8654,78.95917,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1042.470797,0,2,125,15,898.391809,4.8184,29.90183,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.055099,0,2,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},119.87342,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,125,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",367.595315,0,2,125,15,475.659121,2.00321,-53.94532,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,150,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,150,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,150,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,150,15,62.166303,0.8654,74.54509,90.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1197.198297,-0.314,2,150,15,898.391809,4.8184,58.21964,106.78036,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.057228,0,2,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},146.82278,18.2658299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,150,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,150,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",131.956572,0,2,150,15,62.166303,0.8654,80.6451,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1145.388297,0,2,150,15,898.391809,4.8184,51.2611,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.057228,0,2,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},146.82278,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,150,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",370.473815,0,2,150,15,475.659121,2.00321,-52.50838,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,175,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,175,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,175,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,175,15,62.166303,0.8654,74.54509,115.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1307.965797,-0.314,2,175,15,898.391809,4.8184,79.80165,110.19835,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.059357,0,2,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},173.77215,16.3291199999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,175,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,175,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",133.415572,0,2,175,15,62.166303,0.8654,82.33102,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1248.305797,0,2,175,15,898.391809,4.8184,72.62037,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.059357,0,2,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},173.77215,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,175,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",373.352315,0,2,175,15,475.659121,2.00321,-51.07143,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,200,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,200,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,200,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,200,15,62.166303,0.8654,74.54509,140.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1418.733297,-0.314,2,200,15,898.391809,4.8184,101.38366,113.61634,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.061486,0,2,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},200.72152,14.3924,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,200,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,200,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",134.874572,0,2,200,15,62.166303,0.8654,84.01695,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1351.223297,0,2,200,15,898.391809,4.8184,93.97964,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.061486,0,2,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},200.72152,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,200,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",376.230815,0,2,200,15,475.659121,2.00321,-49.63449,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,225,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,225,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,225,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,225,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,225,15,62.166303,0.8654,74.54509,165.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1529.500797,-0.314,2,225,15,898.391809,4.8184,122.96567,117.03433,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.063615,0,2,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},227.67089,12.4556899999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,225,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,225,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",136.333572,0,2,225,15,62.166303,0.8654,85.70288,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1454.140797,0,2,225,15,898.391809,4.8184,115.33891,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.063615,0,2,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},227.67089,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,225,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",379.109315,0,2,225,15,475.659121,2.00321,-48.19755,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,250,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,250,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,250,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,250,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,250,15,62.166303,0.8654,74.54509,190.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1640.268297,-0.314,2,250,15,898.391809,4.8184,144.54768,120.452319999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.065744,0,2,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},254.62025,10.5189899999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,250,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,250,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",137.792572,0,2,250,15,62.166303,0.8654,87.3888,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1557.058297,0,2,250,15,898.391809,4.8184,136.69818,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.065744,0,2,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},254.62025,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,250,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",381.987815,0,2,250,15,475.659121,2.00321,-46.7606,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,275,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,275,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,275,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,275,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,275,15,62.166303,0.8654,74.54509,215.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1751.035797,-0.314,2,275,15,898.391809,4.8184,166.12968,123.870319999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.067873,0,2,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},281.56962,8.58228000000002,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,275,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,275,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",139.251572,0,2,275,15,62.166303,0.8654,89.07473,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1659.975797,0,2,275,15,898.391809,4.8184,158.05744,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.067873,0,2,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},281.56962,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,275,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",384.866315,0,2,275,15,475.659121,2.00321,-45.32366,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,300,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,300,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,300,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,300,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,300,15,62.166303,0.8654,74.54509,240.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1861.803297,-0.314,2,300,15,898.391809,4.8184,187.71169,127.28831,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.070002,0,2,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},308.51899,6.64557000000002,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,300,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,300,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",140.710572,0,2,300,15,62.166303,0.8654,90.76065,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1762.893297,0,2,300,15,898.391809,4.8184,179.41671,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.070002,0,2,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},308.51899,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,300,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",387.744815,0,2,300,15,475.659121,2.00321,-43.88671,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,325,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,325,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,325,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,325,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1972.570797,-0.314,2,325,15,898.391809,4.8184,209.2937,130.7063,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.072132,0,2,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},335.48101,4.69620999999995,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,325,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,325,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",142.169572,0,2,325,15,62.166303,0.8654,92.44658,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1865.810797,0,2,325,15,898.391809,4.8184,200.77598,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.072132,0,2,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},335.48101,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,325,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",390.623315,0,2,325,15,475.659121,2.00321,-42.44977,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,350,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,350,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,350,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,350,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,350,15,62.166303,0.8654,74.54509,290.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2083.338297,-0.314,2,350,15,898.391809,4.8184,230.87571,134.12429,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.074261,0,2,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},362.43038,2.75948999999997,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,350,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,350,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",143.628572,0,2,350,15,62.166303,0.8654,94.1325,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1968.728297,0,2,350,15,898.391809,4.8184,222.13525,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.074261,0,2,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},362.43038,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,350,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",393.501815,0,2,350,15,475.659121,2.00321,-41.01283,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,375,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,375,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,375,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,375,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,375,15,62.166303,0.8654,74.54509,315.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2194.105797,-0.314,2,375,15,898.391809,4.8184,252.45772,137.54228,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.07639,0,2,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},389.37975,0.822780000000022,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,375,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,375,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",145.087572,0,2,375,15,62.166303,0.8654,95.81843,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2071.645797,0,2,375,15,898.391809,4.8184,243.49452,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.07639,0,2,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},389.37975,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,375,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",396.380315,0,2,375,15,475.659121,2.00321,-39.57588,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,400,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,400,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,400,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,400,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,400,15,62.166303,0.8654,74.54509,340.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2304.873297,-0.314,2,400,15,898.391809,4.8184,274.03973,140.960269999999,"ccu"]
["Aviation","comp","Compensation",0.078431,0,2,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,1.11392,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,400,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,400,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",146.546572,0,2,400,15,62.166303,0.8654,97.50436,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2174.563297,0,2,400,15,898.391809,4.8184,264.85379,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.078519,0,2,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},416.32911,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,400,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",399.258815,0,2,400,15,475.659121,2.00321,-38.13894,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,425,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,425,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,425,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,425,15,62.166303,0.8654,74.54509,365.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2415.640797,-0.314,2,425,15,898.391809,4.8184,295.62173,144.37827,"ccu"]
["Aviation","comp","Compensation",0.080407,0,2,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,3.05063000000001,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,425,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,425,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",148.005572,0,2,425,15,62.166303,0.8654,99.19028,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2277.480797,0,2,425,15,898.391809,4.8184,286.21306,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.080648,0,2,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},443.27848,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,425,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",402.137315,0,2,425,15,475.659121,2.00321,-36.702,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,450,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,450,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,450,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,450,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,450,15,62.166303,0.8654,74.54509,390.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2526.408297,-0.314,2,450,15,898.391809,4.8184,317.20374,147.79626,"ccu"]
["Aviation","comp","Compensation",0.082383,0,2,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,4.98734000000001,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,450,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,450,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",149.464572,0,2,450,15,62.166303,0.8654,100.87621,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2380.398297,0,2,450,15,898.391809,4.8184,307.57232,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.082777,0,2,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},470.22785,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,450,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",405.015815,0,2,450,15,475.659121,2.00321,-35.26505,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,475,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,475,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,475,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,475,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2637.175797,-0.314,2,475,15,898.391809,4.8184,338.78575,151.21425,"ccu"]
["Aviation","comp","Compensation",0.084359,0,2,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},490.25316,6.92405999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,475,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,475,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",150.923572,0,2,475,15,62.166303,0.8654,102.56213,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2483.315797,0,2,475,15,898.391809,4.8184,328.93159,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.084906,0,2,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},497.17722,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,475,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",407.894315,0,2,475,15,475.659121,2.00321,-33.82811,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,500,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,500,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,500,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,500,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,500,15,62.166303,0.8654,74.54509,440.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2747.943297,-0.314,2,500,15,898.391809,4.8184,360.36776,154.63224,"ccu"]
["Aviation","comp","Compensation",0.086335,0,2,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,8.86076000000002,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,500,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,500,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",152.382572,0,2,500,15,62.166303,0.8654,104.24806,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2586.233297,0,2,500,15,898.391809,4.8184,350.29086,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.087035,0,2,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},524.12658,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,500,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",410.772815,0,2,500,15,475.659121,2.00321,-32.39117,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,525,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,525,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,525,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,525,15,62.166303,0.8654,74.54509,465.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2858.710797,-0.314,2,525,15,898.391809,4.8184,381.94977,158.05023,"ccu"]
["Aviation","comp","Compensation",0.088311,0,2,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,10.79747,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,525,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,525,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",153.841572,0,2,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2689.150797,0,2,525,15,898.391809,4.8184,371.65013,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.089164,0,2,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},551.07595,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,525,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",413.651315,0,2,525,15,475.659121,2.00321,-30.95422,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,550,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,550,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,550,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,550,15,62.166303,0.8654,74.54509,490.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2969.478297,-0.314,2,550,15,898.391809,4.8184,403.53178,161.468219999999,"ccu"]
["Aviation","comp","Compensation",0.090287,0,2,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,12.7341799999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,550,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,550,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",155.300572,0,2,550,15,62.166303,0.8654,107.61991,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2792.068297,0,2,550,15,898.391809,4.8184,393.0094,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.091293,0,2,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},578.02532,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,550,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",416.529815,0,2,550,15,475.659121,2.00321,-29.51728,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,575,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,575,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,575,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,575,15,62.166303,0.8654,74.54509,515.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3080.245797,-0.314,2,575,15,898.391809,4.8184,425.11378,164.886219999999,"ccu"]
["Aviation","comp","Compensation",0.092263,0,2,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,14.67088,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,575,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,575,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",156.759572,0,2,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2894.985797,0,2,575,15,898.391809,4.8184,414.36867,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.093422,0,2,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},604.97468,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,575,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",419.408315,0,2,575,15,475.659121,2.00321,-28.08033,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,600,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,600,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,600,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,600,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,600,15,62.166303,0.8654,74.54509,540.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3191.013297,-0.314,2,600,15,898.391809,4.8184,446.69579,168.30421,"ccu"]
["Aviation","comp","Compensation",0.094239,0,2,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,16.6075899999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,600,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,600,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",158.218572,0,2,600,15,62.166303,0.8654,110.99176,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2997.903297,0,2,600,15,898.391809,4.8184,435.72794,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.095551,0,2,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},631.92405,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,600,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",422.286815,0,2,600,15,475.659121,2.00321,-26.64339,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,625,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,625,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,625,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,625,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3301.780797,-0.314,2,625,15,898.391809,4.8184,468.2778,171.7222,"ccu"]
["Aviation","comp","Compensation",0.096215,0,2,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,18.5443099999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,625,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,625,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",159.677572,0,2,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3100.820797,0,2,625,15,898.391809,4.8184,457.0872,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.09768,0,2,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},658.87342,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,625,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",425.165315,0,2,625,15,475.659121,2.00321,-25.20645,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,650,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,650,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,650,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,650,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,650,15,62.166303,0.8654,74.54509,590.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3412.548297,-0.314,2,650,15,898.391809,4.8184,489.85981,175.14019,"ccu"]
["Aviation","comp","Compensation",0.098191,0,2,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,20.4936699999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,650,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,650,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",161.136572,0,2,650,15,62.166303,0.8654,114.36361,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3203.738297,0,2,650,15,898.391809,4.8184,478.44647,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.09981,0,2,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},685.83544,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,650,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",428.043815,0,2,650,15,475.659121,2.00321,-23.7695,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,675,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,675,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,675,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,675,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,675,15,62.166303,0.8654,74.54509,615.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3523.315797,-0.314,2,675,15,898.391809,4.8184,511.44182,178.55818,"ccu"]
["Aviation","comp","Compensation",0.100167,0,2,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,22.43038,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,675,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,675,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",162.595572,0,2,675,15,62.166303,0.8654,116.04954,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3306.655797,0,2,675,15,898.391809,4.8184,499.80574,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.101939,0,2,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},712.78481,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,675,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",430.922315,0,2,675,15,475.659121,2.00321,-22.33256,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,700,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,700,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,700,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,700,15,62.166303,0.8654,74.54509,640.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3634.083297,-0.314,2,700,15,898.391809,4.8184,533.02383,181.97617,"ccu"]
["Aviation","comp","Compensation",0.102143,0,2,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,24.36709,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,700,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,700,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",164.054572,0,2,700,15,62.166303,0.8654,117.73546,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3409.573297,0,2,700,15,898.391809,4.8184,521.16501,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.104068,0,2,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},739.73418,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,700,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",433.800815,0,2,700,15,475.659121,2.00321,-20.89562,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,725,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,725,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,725,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,725,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,725,15,62.166303,0.8654,74.54509,665.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3744.850797,-0.314,2,725,15,898.391809,4.8184,554.60584,185.39416,"ccu"]
["Aviation","comp","Compensation",0.104119,0,2,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,26.30379,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,725,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,725,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",165.513572,0,2,725,15,62.166303,0.8654,119.42139,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3512.490797,0,2,725,15,898.391809,4.8184,542.52428,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.106197,0,2,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},766.68354,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,725,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",436.679315,0,2,725,15,475.659121,2.00321,-19.45867,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,750,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,750,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,750,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3855.618297,-0.314,2,750,15,898.391809,4.8184,576.18784,188.812159999999,"ccu"]
["Aviation","comp","Compensation",0.106095,0,2,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,28.2404999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,750,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,750,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",166.972572,0,2,750,15,62.166303,0.8654,121.10731,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3615.408297,0,2,750,15,898.391809,4.8184,563.88355,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.108326,0,2,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},793.63291,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,750,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",439.557815,0,2,750,15,475.659121,2.00321,-18.02173,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,775,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,775,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,775,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3966.385797,-0.314,2,775,15,898.391809,4.8184,597.76985,192.230149999999,"ccu"]
["Aviation","comp","Compensation",0.108071,0,2,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,30.1772199999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,775,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,775,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",168.431572,0,2,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3718.325797,0,2,775,15,898.391809,4.8184,585.24282,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.110455,0,2,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},820.58228,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,775,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",442.436315,0,2,775,15,475.659121,2.00321,-16.58478,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,800,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,800,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,800,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,800,15,62.166303,0.8654,74.54509,740.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4077.153297,-0.314,2,800,15,898.391809,4.8184,619.35186,195.64814,"ccu"]
["Aviation","comp","Compensation",0.110047,0,2,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,32.1139299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,800,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,800,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",169.890572,0,2,800,15,62.166303,0.8654,124.47916,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3821.243297,0,2,800,15,898.391809,4.8184,606.60209,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.112584,0,2,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},847.53165,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,800,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",445.314815,0,2,800,15,475.659121,2.00321,-15.14784,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,825,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,825,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,825,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,825,15,62.166303,0.8654,74.54509,765.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4187.920797,-0.314,2,825,15,898.391809,4.8184,640.93387,199.06613,"ccu"]
["Aviation","comp","Compensation",0.112023,0,2,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,34.0506299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,825,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,825,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",171.349572,0,2,825,15,62.166303,0.8654,126.16509,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3924.160797,0,2,825,15,898.391809,4.8184,627.96135,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.114713,0,2,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},874.48101,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,825,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",448.193315,0,2,825,15,475.659121,2.00321,-13.7109,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,850,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,850,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,850,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,850,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,850,15,62.166303,0.8654,74.54509,790.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4298.688297,-0.314,2,850,15,898.391809,4.8184,662.51588,202.484119999999,"ccu"]
["Aviation","comp","Compensation",0.113999,0,2,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,35.98734,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,850,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,850,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",172.808572,0,2,850,15,62.166303,0.8654,127.85102,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4027.078297,0,2,850,15,898.391809,4.8184,649.32062,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.116842,0,2,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},901.43038,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,850,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",451.071815,0,2,850,15,475.659121,2.00321,-12.27395,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,875,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,875,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,875,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,875,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,875,15,62.166303,0.8654,74.54509,815.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4409.455797,-0.314,2,875,15,898.391809,4.8184,684.09789,205.90211,"ccu"]
["Aviation","comp","Compensation",0.115975,0,2,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,37.9240499999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,875,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,875,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",174.267572,0,2,875,15,62.166303,0.8654,129.53694,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4129.995797,0,2,875,15,898.391809,4.8184,670.67989,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.118971,0,2,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},928.37975,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,875,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",453.950315,0,2,875,15,475.659121,2.00321,-10.83701,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,900,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,900,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,900,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,900,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,900,15,62.166303,0.8654,74.54509,840.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4520.223297,-0.314,2,900,15,898.391809,4.8184,705.67989,209.32011,"ccu"]
["Aviation","comp","Compensation",0.117951,0,2,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,39.86076,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,900,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,900,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",175.726572,0,2,900,15,62.166303,0.8654,131.22287,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4232.913297,0,2,900,15,898.391809,4.8184,692.03916,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.1211,0,2,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},955.32911,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,900,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",456.828815,0,2,900,15,475.659121,2.00321,-9.40007,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,925,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,925,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,925,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,925,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,925,15,62.166303,0.8654,74.54509,865.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4630.990797,-0.314,2,925,15,898.391809,4.8184,727.2619,212.7381,"ccu"]
["Aviation","comp","Compensation",0.119927,0,2,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},940.48101,41.7974699999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,925,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,925,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",177.185572,0,2,925,15,62.166303,0.8654,132.90879,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4335.830797,0,2,925,15,898.391809,4.8184,713.39843,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.123229,0,2,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},982.27848,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,925,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",459.707315,0,2,925,15,475.659121,2.00321,-7.96312,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,950,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,950,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,950,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,950,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,950,15,62.166303,0.8654,74.54509,890.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4741.758297,-0.314,2,950,15,898.391809,4.8184,748.84391,216.156089999999,"ccu"]
["Aviation","comp","Compensation",0.121903,0,2,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},965.49367,43.73418,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,950,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,950,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",178.644572,0,2,950,15,62.166303,0.8654,134.59472,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4438.748297,0,2,950,15,898.391809,4.8184,734.7577,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.125358,0,2,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1009.22785,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,950,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",462.585815,0,2,950,15,475.659121,2.00321,-6.52618,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,975,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,975,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,975,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,975,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,975,15,62.166303,0.8654,74.54509,915.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4852.525797,-0.314,2,975,15,898.391809,4.8184,770.42592,219.574079999999,"ccu"]
["Aviation","comp","Compensation",0.123879,0,2,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},990.50633,45.6835399999998,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,975,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,975,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",180.103572,0,2,975,15,62.166303,0.8654,136.28064,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4541.665797,0,2,975,15,898.391809,4.8184,756.11697,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.127488,0,2,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1036.18987,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,975,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",465.464315,0,2,975,15,475.659121,2.00321,-5.08923,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1000,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1000,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1000,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1000,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1000,15,62.166303,0.8654,74.54509,940.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4963.293297,-0.314,2,1000,15,898.391809,4.8184,792.00793,222.99207,"ccu"]
["Aviation","comp","Compensation",0.125855,0,2,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,47.6202499999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1000,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1000,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",181.562572,0,2,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4644.583297,0,2,1000,15,898.391809,4.8184,777.47623,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.129617,0,2,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1063.13924,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1000,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",468.342815,0,2,1000,15,475.659121,2.00321,-3.65229,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1025,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1025,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1025,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1025,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1025,15,62.166303,0.8654,74.54509,965.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5074.060797,-0.314,2,1025,15,898.391809,4.8184,813.58994,226.41006,"ccu"]
["Aviation","comp","Compensation",0.127831,0,2,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,49.5569600000001,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1025,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1025,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",183.021572,0,2,1025,15,62.166303,0.8654,139.65249,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4747.500797,0,2,1025,15,898.391809,4.8184,798.8355,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.131746,0,2,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.08861,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1025,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",471.221315,0,2,1025,15,475.659121,2.00321,-2.21535,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1050,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1050,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1050,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1050,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1050,15,62.166303,0.8654,74.54509,990.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5184.828297,-0.314,2,1050,15,898.391809,4.8184,835.17194,229.82806,"ccu"]
["Aviation","comp","Compensation",0.129807,0,2,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,51.49367,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1050,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1050,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",184.480572,0,2,1050,15,62.166303,0.8654,141.33842,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4850.418297,0,2,1050,15,898.391809,4.8184,820.19477,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.133875,0,2,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1117.03797,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1050,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",474.099815,0,2,1050,15,475.659121,2.00321,-0.7784,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1075,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1075,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1075,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1075,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1075,15,62.166303,0.8654,74.54509,1015.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5295.595797,-0.314,2,1075,15,898.391809,4.8184,856.75395,233.246049999999,"ccu"]
["Aviation","comp","Compensation",0.131783,0,2,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,53.43038,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1075,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1075,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",185.939572,0,2,1075,15,62.166303,0.8654,143.02435,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4953.335797,0,2,1075,15,898.391809,4.8184,841.55404,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.136004,0,2,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1143.98734,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1075,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",476.978315,0,2,1075,15,475.659121,2.00321,0.65854,447.40542,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1100,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1100,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1100,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1100,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1100,15,62.166303,0.8654,74.54509,1040.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5406.363297,-0.314,2,1100,15,898.391809,4.8184,878.33596,236.66404,"ccu"]
["Aviation","comp","Compensation",0.133759,0,2,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,55.3670899999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1100,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1100,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",187.398572,0,2,1100,15,62.166303,0.8654,144.71027,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5056.253297,0,2,1100,15,898.391809,4.8184,862.91331,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.138133,0,2,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1170.93671,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1100,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",479.856815,0,2,1100,15,475.659121,2.00321,2.09548,455.50954,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1125,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1125,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1125,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1125,15,62.166303,0.8654,74.54509,1065.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5517.130797,-0.314,2,1125,15,898.391809,4.8184,899.91797,240.08203,"ccu"]
["Aviation","comp","Compensation",0.135735,0,2,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1140.58228,57.3037999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1125,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1125,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",188.857572,0,2,1125,15,62.166303,0.8654,146.3962,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5159.170797,0,2,1125,15,898.391809,4.8184,884.27258,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.140262,0,2,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1197.88608,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1125,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",482.735315,0,2,1125,15,475.659121,2.00321,3.53243,463.61365,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1150,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1150,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1150,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1150,15,62.166303,0.8654,74.54509,1090.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5627.898297,-0.314,2,1150,15,898.391809,4.8184,921.49998,243.500019999999,"ccu"]
["Aviation","comp","Compensation",0.137711,0,2,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1165.59494,59.2405000000001,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1150,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1150,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",190.316572,0,2,1150,15,62.166303,0.8654,148.08212,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5262.088297,0,2,1150,15,898.391809,4.8184,905.63185,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.142391,0,2,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1224.83544,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1150,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",485.613815,0,2,1150,15,475.659121,2.00321,4.96937,471.717779999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1175,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1175,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1175,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1175,15,62.166303,0.8654,74.54509,1115.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5738.665797,-0.314,2,1175,15,898.391809,4.8184,943.08199,246.918009999999,"ccu"]
["Aviation","comp","Compensation",0.139687,0,2,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,61.17722,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1175,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1175,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",191.775572,0,2,1175,15,62.166303,0.8654,149.76805,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5365.005797,0,2,1175,15,898.391809,4.8184,926.99111,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.14452,0,2,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1251.78481,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1175,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",488.492315,0,2,1175,15,475.659121,2.00321,6.40631,479.821899999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,2,1200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",532.593297,1.90135,2,1200,15,898.391809,4.8184,-125.40015,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.044454,{"v":4.3e-05,"d":"4.30E-05"},2,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-32.63889,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",57.264295,0.3,2,1200,15,126.00477,0.61911,-215.4131,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1200,15,475.659121,2.00321,-65.77267,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,2,1200,15,62.166303,0.8654,74.54509,1140.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5849.433297,-0.314,2,1200,15,898.391809,4.8184,964.664,250.336,"ccu"]
["Aviation","comp","Compensation",0.141663,0,2,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,63.1139299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1200,15,126.00477,0.61911,-50.5931,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",351.475715,0.11514,2,1200,15,475.659121,2.00321,-65.77267,1000,"ccu"]
["Cement","ccs","CCS",193.23457200000001,0,2,1200,15,62.166303,0.8654,151.45397,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",5467.923297,0,2,1200,15,898.391809,4.8184,948.35038,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.146649,0,2,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1278.73418,1000,"comp"]
["Maritime","h2","Low-emission ammonia",94.682077,0,2,1200,15,126.00477,0.61911,-50.5931,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",491.370815,0,2,1200,15,475.659121,2.00321,7.84326,487.92601,"comp"]
["Cement","comp","Compensation",75.147303,0,4,0,15,62.166303,0.8654,15,59.54509,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,0,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,0,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,0,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","comp","Compensation",75.147303,0,4,0,15,62.166303,0.8654,15,59.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",572.961897,-0.314,4,0,15,898.391809,4.8184,-63.40697,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.045275,0,4,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-4.48101,1000,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",62.730956,0,4,0,15,126.00477,0.61911,-102.20125,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,0,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",123.202572,0,4,0,15,62.166303,0.8654,70.52955,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",568.251897,0,4,0,15,898.391809,4.8184,-68.5165,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.045275,0,4,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-4.48101,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",62.730956,0,4,0,15,126.00477,0.61911,-102.20125,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",356.902815,0,4,0,15,475.659121,2.00321,-59.283,1000,"comp"]
["Cement","comp","Compensation",96.782303,0,4,25,15,62.166303,0.8654,40,34.54509,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,25,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,25,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,25,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","comp","Compensation",96.782303,0,4,25,15,62.166303,0.8654,40,34.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",683.729397,-0.314,4,25,15,898.391809,4.8184,-41.82496,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.047404,0,4,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},22.46835,17.55697,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",77.730941,0,4,25,15,126.00477,0.61911,-77.97294,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,25,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",124.661572,0,4,25,15,62.166303,0.8654,72.21547,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",671.169397,0,4,25,15,898.391809,4.8184,-47.15723,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.047404,0,4,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},22.46835,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",77.730941,0,4,25,15,126.00477,0.61911,-77.97294,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",359.781315,0,4,25,15,475.659121,2.00321,-57.84606,1000,"comp"]
["Cement","comp","Compensation",118.417303,0,4,50,15,62.166303,0.8654,65,9.54509,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,50,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,50,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,50,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","comp","Compensation",118.417303,0,4,50,15,62.166303,0.8654,65,9.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",794.496897,-0.314,4,50,15,898.391809,4.8184,-20.24295,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.049533,0,4,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},49.41772,15.6202499999999,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",92.730926,0,4,50,15,126.00477,0.61911,-53.74464,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,50,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",126.120572,0,4,50,15,62.166303,0.8654,73.9014,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",774.086897,0,4,50,15,898.391809,4.8184,-25.79796,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.049533,0,4,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},49.41772,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",92.730926,0,4,50,15,126.00477,0.61911,-53.74464,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",362.659815,0,4,50,15,475.659121,2.00321,-56.40912,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,75,15,62.166303,0.8654,74.54509,15.4549099999999,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,75,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,75,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,75,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,75,15,62.166303,0.8654,74.54509,15.4549099999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",905.264397,-0.314,4,75,15,898.391809,4.8184,1.33906,88.66094,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.051662,0,4,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},76.36709,13.6835399999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,75,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,75,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",127.579572,0,4,75,15,62.166303,0.8654,75.58732,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",877.004397,0,4,75,15,898.391809,4.8184,-4.4387,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.051662,0,4,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},76.36709,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,75,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",365.538315,0,4,75,15,475.659121,2.00321,-54.97217,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,100,15,62.166303,0.8654,74.54509,40.45491,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,100,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,100,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,100,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1016.031897,-0.314,4,100,15,898.391809,4.8184,22.92107,92.07893,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.053791,0,4,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},103.31646,11.7468299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,100,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,100,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",129.038572,0,4,100,15,62.166303,0.8654,77.27325,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",979.921897,0,4,100,15,898.391809,4.8184,16.92057,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.053791,0,4,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},103.31646,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,100,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",368.416815,0,4,100,15,475.659121,2.00321,-53.53523,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,125,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,125,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,125,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,125,15,62.166303,0.8654,74.54509,65.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1126.799397,-0.314,4,125,15,898.391809,4.8184,44.50308,95.49692,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.05592,0,4,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},130.26582,9.81013000000001,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,125,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,125,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",130.497572,0,4,125,15,62.166303,0.8654,78.95917,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1082.839397,0,4,125,15,898.391809,4.8184,38.27984,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.05592,0,4,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},130.26582,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,125,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",371.295315,0,4,125,15,475.659121,2.00321,-52.09829,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,150,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,150,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,150,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,150,15,62.166303,0.8654,74.54509,90.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1237.566897,-0.314,4,150,15,898.391809,4.8184,66.08508,98.91492,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.058049,0,4,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},157.21519,7.87341999999998,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,150,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,150,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",131.956572,0,4,150,15,62.166303,0.8654,80.6451,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1185.756897,0,4,150,15,898.391809,4.8184,59.63911,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.058049,0,4,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},157.21519,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,150,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",374.173815,0,4,150,15,475.659121,2.00321,-50.66134,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,175,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,175,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,175,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,175,15,62.166303,0.8654,74.54509,115.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1348.334397,-0.314,4,175,15,898.391809,4.8184,87.66709,102.33291,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.060178,0,4,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},184.16456,5.93671,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,175,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,175,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",133.415572,0,4,175,15,62.166303,0.8654,82.33102,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1288.674397,0,4,175,15,898.391809,4.8184,80.99838,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.060178,0,4,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},184.16456,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,175,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",377.052315,0,4,175,15,475.659121,2.00321,-49.2244,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,200,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,200,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,200,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,200,15,62.166303,0.8654,74.54509,140.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1459.101897,-0.314,4,200,15,898.391809,4.8184,109.2491,105.7509,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.062308,0,4,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},211.12658,3.98734000000001,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,200,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,200,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",134.874572,0,4,200,15,62.166303,0.8654,84.01695,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1391.591897,0,4,200,15,898.391809,4.8184,102.35765,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.062308,0,4,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},211.12658,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,200,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",379.930815,0,4,200,15,475.659121,2.00321,-47.78745,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,225,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,225,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,225,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,225,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,225,15,62.166303,0.8654,74.54509,165.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1569.869397,-0.314,4,225,15,898.391809,4.8184,130.83111,109.16889,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.064437,0,4,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},238.07595,2.05062999999998,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,225,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,225,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",136.333572,0,4,225,15,62.166303,0.8654,85.70288,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1494.509397,0,4,225,15,898.391809,4.8184,123.71692,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.064437,0,4,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},238.07595,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,225,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",382.809315,0,4,225,15,475.659121,2.00321,-46.35051,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,250,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,250,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,250,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,250,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,250,15,62.166303,0.8654,74.54509,190.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1680.636897,-0.314,4,250,15,898.391809,4.8184,152.41312,112.58688,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.066566,0,4,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},265.02532,0.11391999999995,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,250,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,250,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",137.792572,0,4,250,15,62.166303,0.8654,87.3888,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1597.426897,0,4,250,15,898.391809,4.8184,145.07618,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.066566,0,4,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},265.02532,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,250,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",385.687815,0,4,250,15,475.659121,2.00321,-44.91357,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,275,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,275,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,275,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,275,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,275,15,62.166303,0.8654,74.54509,215.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1791.404397,-0.314,4,275,15,898.391809,4.8184,173.99513,116.00487,"ccu"]
["Aviation","comp","Compensation",0.068551,0,4,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},290.1519,1.82277999999996,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,275,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,275,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",139.251572,0,4,275,15,62.166303,0.8654,89.07473,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1700.344397,0,4,275,15,898.391809,4.8184,166.43545,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.068695,0,4,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},291.97468,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,275,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",388.566315,0,4,275,15,475.659121,2.00321,-43.47662,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,300,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,300,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,300,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,300,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,300,15,62.166303,0.8654,74.54509,240.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1902.171897,-0.314,4,300,15,898.391809,4.8184,195.57714,119.422859999999,"ccu"]
["Aviation","comp","Compensation",0.070527,0,4,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},315.16456,3.75949000000002,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,300,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,300,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",140.710572,0,4,300,15,62.166303,0.8654,90.76065,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1803.261897,0,4,300,15,898.391809,4.8184,187.79472,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.070824,0,4,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},318.92405,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,300,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",391.444815,0,4,300,15,475.659121,2.00321,-42.03968,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,325,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,325,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,325,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,325,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2012.939397,-0.314,4,325,15,898.391809,4.8184,217.15914,122.840859999999,"ccu"]
["Aviation","comp","Compensation",0.072503,0,4,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},340.17722,5.69620000000003,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,325,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,325,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",142.169572,0,4,325,15,62.166303,0.8654,92.44658,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1906.179397,0,4,325,15,898.391809,4.8184,209.15399,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.072953,0,4,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},345.87342,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,325,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",394.323315,0,4,325,15,475.659121,2.00321,-40.60274,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,350,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,350,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,350,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,350,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,350,15,62.166303,0.8654,74.54509,290.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2123.706897,-0.314,4,350,15,898.391809,4.8184,238.74115,126.25885,"ccu"]
["Aviation","comp","Compensation",0.074479,0,4,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},365.18987,7.63291000000003,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,350,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,350,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",143.628572,0,4,350,15,62.166303,0.8654,94.1325,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2009.096897,0,4,350,15,898.391809,4.8184,230.51326,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.075082,0,4,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},372.82278,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,350,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",397.201815,0,4,350,15,475.659121,2.00321,-39.16579,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,375,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,375,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,375,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,375,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,375,15,62.166303,0.8654,74.54509,315.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2234.474397,-0.314,4,375,15,898.391809,4.8184,260.32316,129.67684,"ccu"]
["Aviation","comp","Compensation",0.076455,0,4,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},390.20253,9.56961999999998,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,375,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,375,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",145.087572,0,4,375,15,62.166303,0.8654,95.81843,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2112.014397,0,4,375,15,898.391809,4.8184,251.87253,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.077211,0,4,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},399.77215,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,375,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",400.080315,0,4,375,15,475.659121,2.00321,-37.72885,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,400,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,400,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,400,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,400,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,400,15,62.166303,0.8654,74.54509,340.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2345.241897,-0.314,4,400,15,898.391809,4.8184,281.90517,133.09483,"ccu"]
["Aviation","comp","Compensation",0.078431,0,4,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,11.5063299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,400,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,400,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",146.546572,0,4,400,15,62.166303,0.8654,97.50436,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2214.931897,0,4,400,15,898.391809,4.8184,273.2318,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.07934,0,4,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},426.72152,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,400,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",402.958815,0,4,400,15,475.659121,2.00321,-36.2919,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,425,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,425,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,425,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,425,15,62.166303,0.8654,74.54509,365.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2456.009397,-0.314,4,425,15,898.391809,4.8184,303.48718,136.512819999999,"ccu"]
["Aviation","comp","Compensation",0.080407,0,4,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,13.4430399999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,425,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,425,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",148.005572,0,4,425,15,62.166303,0.8654,99.19028,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2317.849397,0,4,425,15,898.391809,4.8184,294.59107,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.081469,0,4,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},453.67089,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,425,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",405.837315,0,4,425,15,475.659121,2.00321,-34.85496,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,450,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,450,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,450,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,450,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,450,15,62.166303,0.8654,74.54509,390.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2566.776897,-0.314,4,450,15,898.391809,4.8184,325.06919,139.93081,"ccu"]
["Aviation","comp","Compensation",0.082383,0,4,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,15.37974,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,450,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,450,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",149.464572,0,4,450,15,62.166303,0.8654,100.87621,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2420.766897,0,4,450,15,898.391809,4.8184,315.95033,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.083598,0,4,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},480.62025,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,450,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",408.715815,0,4,450,15,475.659121,2.00321,-33.41802,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,475,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,475,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,475,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,475,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2677.544397,-0.314,4,475,15,898.391809,4.8184,346.65119,143.34881,"ccu"]
["Aviation","comp","Compensation",0.084359,0,4,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},490.25316,17.31646,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,475,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,475,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",150.923572,0,4,475,15,62.166303,0.8654,102.56213,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2523.684397,0,4,475,15,898.391809,4.8184,337.3096,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.085727,0,4,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},507.56962,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,475,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",411.594315,0,4,475,15,475.659121,2.00321,-31.98107,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,500,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,500,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,500,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,500,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,500,15,62.166303,0.8654,74.54509,440.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2788.311897,-0.314,4,500,15,898.391809,4.8184,368.2332,146.7668,"ccu"]
["Aviation","comp","Compensation",0.086335,0,4,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,19.25317,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,500,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,500,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",152.382572,0,4,500,15,62.166303,0.8654,104.24806,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2626.601897,0,4,500,15,898.391809,4.8184,358.66887,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.087856,0,4,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},534.51899,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,500,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",414.472815,0,4,500,15,475.659121,2.00321,-30.54413,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,525,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,525,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,525,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,525,15,62.166303,0.8654,74.54509,465.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2899.079397,-0.314,4,525,15,898.391809,4.8184,389.81521,150.18479,"ccu"]
["Aviation","comp","Compensation",0.088311,0,4,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,21.20253,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,525,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,525,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",153.841572,0,4,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2729.519397,0,4,525,15,898.391809,4.8184,380.02814,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.089986,0,4,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},561.48101,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,525,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",417.351315,0,4,525,15,475.659121,2.00321,-29.10719,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,550,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,550,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,550,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,550,15,62.166303,0.8654,74.54509,490.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3009.846897,-0.314,4,550,15,898.391809,4.8184,411.39722,153.60278,"ccu"]
["Aviation","comp","Compensation",0.090287,0,4,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,23.1392399999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,550,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,550,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",155.300572,0,4,550,15,62.166303,0.8654,107.61991,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2832.436897,0,4,550,15,898.391809,4.8184,401.38741,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.092115,0,4,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},588.43038,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,550,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",420.229815,0,4,550,15,475.659121,2.00321,-27.67024,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,575,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,575,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,575,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,575,15,62.166303,0.8654,74.54509,515.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3120.614397,-0.314,4,575,15,898.391809,4.8184,432.97923,157.02077,"ccu"]
["Aviation","comp","Compensation",0.092263,0,4,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,25.0759499999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,575,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,575,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",156.759572,0,4,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2935.354397,0,4,575,15,898.391809,4.8184,422.74668,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.094244,0,4,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.37975,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,575,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",423.108315,0,4,575,15,475.659121,2.00321,-26.2333,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,600,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,600,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,600,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,600,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,600,15,62.166303,0.8654,74.54509,540.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3231.381897,-0.314,4,600,15,898.391809,4.8184,454.56124,160.43876,"ccu"]
["Aviation","comp","Compensation",0.094239,0,4,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,27.01265,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,600,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,600,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",158.218572,0,4,600,15,62.166303,0.8654,110.99176,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3038.271897,0,4,600,15,898.391809,4.8184,444.10595,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.096373,0,4,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},642.32911,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,600,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",425.986815,0,4,600,15,475.659121,2.00321,-24.79635,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,625,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,625,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,625,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,625,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3342.149397,-0.314,4,625,15,898.391809,4.8184,476.14324,163.85676,"ccu"]
["Aviation","comp","Compensation",0.096215,0,4,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,28.9493699999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,625,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,625,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",159.677572,0,4,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3141.189397,0,4,625,15,898.391809,4.8184,465.46521,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.098502,0,4,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},669.27848,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,625,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",428.865315,0,4,625,15,475.659121,2.00321,-23.35941,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,650,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,650,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,650,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,650,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,650,15,62.166303,0.8654,74.54509,590.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3452.916897,-0.314,4,650,15,898.391809,4.8184,497.72525,167.274749999999,"ccu"]
["Aviation","comp","Compensation",0.098191,0,4,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,30.8860799999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,650,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,650,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",161.136572,0,4,650,15,62.166303,0.8654,114.36361,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3244.106897,0,4,650,15,898.391809,4.8184,486.82448,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.100631,0,4,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},696.22785,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,650,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",431.743815,0,4,650,15,475.659121,2.00321,-21.92247,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,675,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,675,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,675,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,675,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,675,15,62.166303,0.8654,74.54509,615.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3563.684397,-0.314,4,675,15,898.391809,4.8184,519.30726,170.692739999999,"ccu"]
["Aviation","comp","Compensation",0.100167,0,4,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,32.82279,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,675,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,675,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",162.595572,0,4,675,15,62.166303,0.8654,116.04954,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3347.024397,0,4,675,15,898.391809,4.8184,508.18375,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.10276,0,4,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},723.17722,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,675,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",434.622315,0,4,675,15,475.659121,2.00321,-20.48552,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,700,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,700,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,700,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,700,15,62.166303,0.8654,74.54509,640.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3674.451897,-0.314,4,700,15,898.391809,4.8184,540.88927,174.11073,"ccu"]
["Aviation","comp","Compensation",0.102143,0,4,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,34.75949,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,700,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,700,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",164.054572,0,4,700,15,62.166303,0.8654,117.73546,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3449.941897,0,4,700,15,898.391809,4.8184,529.54302,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.104889,0,4,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},750.12658,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,700,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",437.500815,0,4,700,15,475.659121,2.00321,-19.04858,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,725,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,725,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,725,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,725,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,725,15,62.166303,0.8654,74.54509,665.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3785.219397,-0.314,4,725,15,898.391809,4.8184,562.47128,177.52872,"ccu"]
["Aviation","comp","Compensation",0.104119,0,4,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,36.6962,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,725,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,725,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",165.513572,0,4,725,15,62.166303,0.8654,119.42139,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3552.859397,0,4,725,15,898.391809,4.8184,550.90229,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.107018,0,4,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},777.07595,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,725,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",440.379315,0,4,725,15,475.659121,2.00321,-17.61164,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,750,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,750,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,750,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3895.986897,-0.314,4,750,15,898.391809,4.8184,584.05329,180.94671,"ccu"]
["Aviation","comp","Compensation",0.106095,0,4,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,38.6329099999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,750,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,750,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",166.972572,0,4,750,15,62.166303,0.8654,121.10731,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3655.776897,0,4,750,15,898.391809,4.8184,572.26156,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.109147,0,4,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},804.02532,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,750,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",443.257815,0,4,750,15,475.659121,2.00321,-16.17469,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,775,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,775,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,775,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4006.754397,-0.314,4,775,15,898.391809,4.8184,605.63529,184.364709999999,"ccu"]
["Aviation","comp","Compensation",0.108071,0,4,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,40.5696199999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,775,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,775,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",168.431572,0,4,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3758.694397,0,4,775,15,898.391809,4.8184,593.62083,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.111276,0,4,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},830.97468,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,775,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",446.136315,0,4,775,15,475.659121,2.00321,-14.73775,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,800,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,800,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,800,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,800,15,62.166303,0.8654,74.54509,740.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4117.521897,-0.314,4,800,15,898.391809,4.8184,627.2173,187.782699999999,"ccu"]
["Aviation","comp","Compensation",0.110047,0,4,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,42.5063299999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,800,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,800,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",169.890572,0,4,800,15,62.166303,0.8654,124.47916,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3861.611897,0,4,800,15,898.391809,4.8184,614.98009,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.113405,0,4,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},857.92405,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,800,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",449.014815,0,4,800,15,475.659121,2.00321,-13.30081,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,825,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,825,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,825,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,825,15,62.166303,0.8654,74.54509,765.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4228.289397,-0.314,4,825,15,898.391809,4.8184,648.79931,191.20069,"ccu"]
["Aviation","comp","Compensation",0.112023,0,4,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,44.4430399999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,825,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,825,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",171.349572,0,4,825,15,62.166303,0.8654,126.16509,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3964.529397,0,4,825,15,898.391809,4.8184,636.33936,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.115534,0,4,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},884.87342,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,825,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",451.893315,0,4,825,15,475.659121,2.00321,-11.86386,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,850,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,850,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,850,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,850,15,475.659121,2.00321,-63.813,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,4,850,15,62.166303,0.8654,74.54509,790.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4339.056897,-0.314,4,850,15,898.391809,4.8184,670.38132,194.61868,"ccu"]
["Aviation","comp","Compensation",0.113999,0,4,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,46.3923999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,850,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,850,15,475.659121,2.00321,-63.813,1000,"ccu"]
["Cement","ccs","CCS",172.808572,0,4,850,15,62.166303,0.8654,127.85102,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4067.446897,0,4,850,15,898.391809,4.8184,657.69863,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.117664,0,4,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},911.83544,1000,"comp"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,850,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",454.771815,0,4,850,15,475.659121,2.00321,-10.42692,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,4,875,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",572.961897,1.90135,4,875,15,898.391809,4.8184,-111.56131,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.045275,{"v":4.3e-05,"d":"4.30E-05"},4,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},-9.83333,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",62.730956,0.3,4,875,15,126.00477,0.61911,-198.28214,1000,"normal"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,875,15,126.00477,0.61911,-42.64336,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,4,975,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",5114.429397,-0.314,4,1025,15,898.391809,4.8184,821.45538,218.54462,"ccu"]
["Maritime","h2","Low-emission ammonia",99.603837,0,4,1100,15,126.00477,0.61911,-42.64336,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",355.175715,0.11514,4,1175,15,475.659121,2.00321,-63.813,1000,"ccu"]
["CF","efuel","MTO using non-fossil CO2",608.620497,0,6,0,15,898.391809,4.8184,-60.13849,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",68.197617,0.3,6,100,15,126.00477,0.61911,-181.15118,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",358.875715,0.11514,6,150,15,475.659121,2.00321,-61.85332,1000,"ccu"]
["CF","ccu","MTO using fossil CCU",613.330497,1.90135,6,250,15,898.391809,4.8184,-97.72246,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,6,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.082291,0,6,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},464.07595,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2607.145497,-0.314,6,450,15,898.391809,4.8184,332.93463,132.065369999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.088678,0,6,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},544.92405,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.095065,0,6,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},625.77215,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",3284.475497,0,6,650,15,898.391809,4.8184,495.20249,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,6,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",358.875715,0.11514,6,800,15,475.659121,2.00321,-61.85332,1000,"ccu"]
["Maritime","h2","Low-emission ammonia",104.525597,0,6,925,15,126.00477,0.61911,-34.69363,1000,"comp"]
["Maritime","h2","Low-emission ammonia",104.525597,0,6,950,15,126.00477,0.61911,-34.69363,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.137647,0,6,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1164.78481,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",68.197617,0.3,6,1150,15,126.00477,0.61911,-181.15118,1000,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.144034,0,6,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1245.63291,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",73.664278,0.3,8,75,15,126.00477,0.61911,-164.02022,1000,"normal"]
["Maritime","h2","Low-emission ammonia",109.447357,0,8,125,15,126.00477,0.61911,-26.7439,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,8,225,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",1872.141597,-0.314,8,275,15,898.391809,4.8184,189.72601,100.27399,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.074596,0,8,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},366.67089,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,8,375,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",2604.421597,0,8,475,15,898.391809,4.8184,354.06562,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",73.664278,0.3,8,575,15,126.00477,0.61911,-164.02022,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",362.575715,0.11514,8,625,15,475.659121,2.00321,-59.89365,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,8,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",3633.596597,0,8,725,15,898.391809,4.8184,567.65831,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",459.293315,0,8,825,15,475.659121,2.00321,-8.16979,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,8,900,15,62.166303,0.8654,74.54509,840.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.129952,0,8,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1067.37975,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.046918,{"v":4.3e-05,"d":"4.30E-05"},8,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},35.80556,1054.75139999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",5280.276597,0,8,1125,15,898.391809,4.8184,909.40661,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.046918,{"v":4.3e-05,"d":"4.30E-05"},8,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},35.80556,1179.81469,"normal"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",94.130925,0,10,25,15,126.00477,0.61911,-51.48333,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,10,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["Maritime","h2","Low-emission ammonia",114.369117,0,10,200,15,126.00477,0.61911,-18.79416,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",396.787815,0,10,250,15,475.659121,2.00321,-39.37246,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,10,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2233.120197,0,10,375,15,898.391809,4.8184,277.00656,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",366.275715,0.11514,10,475,15,475.659121,2.00321,-57.93398,1000,"ccu"]
["Cement","ccs","CCS",153.841572,0,10,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["CF","ccu","MTO using fossil CCU",694.067697,1.90135,10,600,15,898.391809,4.8184,-70.04478,1000,"normal"]
["Maritime","h2","Low-emission ammonia",114.369117,0,10,675,15,126.00477,0.61911,-18.79416,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",451.479315,0,10,725,15,475.659121,2.00321,-12.07053,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,10,850,15,62.166303,0.8654,74.54509,790.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",114.369117,0,10,875,15,126.00477,0.61911,-18.79416,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",366.275715,0.11514,10,950,15,475.659121,2.00321,-57.93398,1000,"normal"]
["CF","efuel","MTO using non-fossil CO2",4908.975197,0,10,1025,15,898.391809,4.8184,832.34754,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.047739,{"v":4.3e-05,"d":"4.30E-05"},10,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},58.61111,1056.95851,"normal"]
["CF","ccu","MTO using fossil CCU",734.436297,1.90135,12,0,15,898.391809,4.8184,-56.20593,1000,"normal"]
["CF","ccu","MTO using fossil CCU",734.436297,1.90135,12,25,15,898.391809,4.8184,-56.20593,1000,"normal"]
["Aviation","comp","Compensation",0.052743,0,12,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},90.05063,27.9114,"ccu"]
["Primary steel","h2","DRI-EAF with H2",388.973815,0,12,150,15,475.659121,2.00321,-43.2732,1000,"comp"]
["Maritime","h2","Low-emission ammonia",119.290877,0,12,250,15,126.00477,0.61911,-10.84443,1000,"ccu"]
["Cement","ccs","CCS",143.628572,0,12,350,15,62.166303,0.8654,94.1325,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",369.975715,0.11514,12,375,15,475.659121,2.00321,-55.9743,1000,"normal"]
["Maritime","h2","Low-emission ammonia",119.290877,0,12,500,15,126.00477,0.61911,-10.84443,1000,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.04856,{"v":4.3e-05,"d":"4.30E-05"},12,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},81.41667,458.861809999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",369.975715,0.11514,12,625,15,475.659121,2.00321,-55.9743,1000,"normal"]
["Maritime","h2","Low-emission ammonia",119.290877,0,12,700,15,126.00477,0.61911,-10.84443,1000,"comp"]
["Aviation","comp","Compensation",0.104119,0,12,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,78.29114,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4228.921297,0,12,850,15,898.391809,4.8184,691.21067,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4331.838797,0,12,875,15,898.391809,4.8184,712.56994,1000,"comp"]
["Cement","ccs","CCS",181.562572,0,12,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["CF","ccu","MTO using fossil CCU",734.436297,1.90135,12,1075,15,898.391809,4.8184,-56.20593,1000,"normal"]
["Maritime","h2","Low-emission ammonia",119.290877,0,12,1150,15,126.00477,0.61911,-10.84443,1000,"ccu"]
["Primary steel","h2","DRI-EAF with H2",509.870815,0,12,1200,15,475.659121,2.00321,17.07844,478.69083,"comp"]
["Aviation","comp","Compensation",0.048791,0,14,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,34.4303799999999,"ccu"]
["Maritime","h2","Low-emission ammonia",124.212637,0,14,125,15,126.00477,0.61911,-2.89469,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",373.675715,0.11514,14,200,15,475.659121,2.00321,-54.01463,1000,"normal"]
["CF","efuel","MTO using non-fossil CO2",1902.187397,0,14,275,15,898.391809,4.8184,208.3255,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",90.064262,0.3,14,300,15,126.00477,0.61911,-112.62733,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",373.675715,0.11514,14,400,15,475.659121,2.00321,-54.01463,1000,"ccu"]
["CF","ccu","MTO using fossil CCU",774.804897,1.90135,14,500,15,898.391809,4.8184,-42.36709,1000,"normal"]
["Aviation","comp","Compensation",0.090287,0,14,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,75.1265799999999,"ccu"]
["Maritime","h2","Low-emission ammonia",124.212637,0,14,600,15,126.00477,0.61911,-2.89469,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",450.243815,0,14,650,15,475.659121,2.00321,-12.68729,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.113254,0,14,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},856.01266,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",373.675715,0.11514,14,850,15,475.659121,2.00321,-54.01463,1000,"normal"]
["Cement","ccs","CCS",175.726572,0,14,900,15,62.166303,0.8654,131.22287,1000,"comp"]
["CF","ccu","MTO using fossil CCU",774.804897,1.90135,14,975,15,898.391809,4.8184,-42.36709,1000,"normal"]
["Cement","ccs","CCS",183.021572,0,14,1025,15,62.166303,0.8654,139.65249,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,14,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",5980.877397,-0.314,14,1175,15,898.391809,4.8184,990.27465,199.72535,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",110.530908,0,16,25,15,126.00477,0.61911,-24.99372,1000,"comp"]
["CF","ccu","MTO using fossil CCU",815.173497,1.90135,16,150,15,898.391809,4.8184,-28.52824,1000,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.065107,0,16,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},246.55696,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",95.530923,0.3,16,250,15,126.00477,0.61911,-95.49637,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",377.375715,0.11514,16,300,15,475.659121,2.00321,-52.05496,1000,"ccu"]
["CF","ccu","MTO using fossil CCU",815.173497,1.90135,16,400,15,898.391809,4.8184,-28.52824,1000,"normal"]
["Maritime","h2","Low-emission ammonia",129.134397,0,16,425,15,126.00477,0.61911,5.05504,357.604099999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,16,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",3473.593497,-0.314,16,600,15,898.391809,4.8184,501.75389,113.246109999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.105559,0,16,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},758.60759,1000,"comp"]
["Maritime","h2","Low-emission ammonia",129.134397,0,16,775,15,126.00477,0.61911,5.05504,696.80035,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4103.823497,0,16,800,15,898.391809,4.8184,665.24815,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.050203,{"v":4.3e-05,"d":"4.30E-05"},16,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},127.05556,763.40014,"normal"]
["Primary steel","h2","DRI-EAF with H2",377.375715,0.11514,16,950,15,475.659121,2.00321,-52.05496,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,16,1025,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",377.375715,0.11514,16,1150,15,475.659121,2.00321,-52.05496,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",511.513815,0,16,1150,15,475.659121,2.00321,17.89862,458.78853,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",100.997584,0.3,18,75,15,126.00477,0.61911,-78.36541,1000,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.057412,0,18,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},149.1519,1000,"comp"]
["CF","ccu","MTO using fossil CCU",855.542097,1.90135,18,225,15,898.391809,4.8184,-14.6894,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,18,300,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.051025,{"v":4.3e-05,"d":"4.30E-05"},18,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},149.88889,165.27567,"normal"]
["CF","efuel","MTO using non-fossil CO2",2738.589597,-0.314,18,425,15,898.391809,4.8184,358.54528,81.45472,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,18,450,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.090287,0,18,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,95.9113899999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3423.769597,0,18,625,15,898.391809,4.8184,524.11128,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",100.997584,0.3,18,725,15,126.00477,0.61911,-78.36541,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",381.075715,0.11514,18,775,15,475.659121,2.00321,-50.09529,1000,"ccu"]
["Maritime","ccu","syn-methanol (fossil CCU)",100.997584,0.3,18,800,15,126.00477,0.61911,-78.36541,1000,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",100.997584,0.3,18,925,15,126.00477,0.61911,-78.36541,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",495.064315,0,18,975,15,475.659121,2.00321,9.68705,400.21266,"comp"]
["CF","efuel","MTO using non-fossil CO2",5618.544597,-0.314,18,1075,15,898.391809,4.8184,919.6775,170.3225,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.146833,0,18,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1281.06329,1000,"comp"]
["Cement","ccs","CCS",191.775572,0,18,1175,15,62.166303,0.8654,149.76805,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1097.035697,0,20,50,15,898.391809,4.8184,41.22611,1000,"comp"]
["Aviation","comp","Compensation",0.056695,0,20,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},140.07595,32.6184899999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",384.775715,0.11514,20,200,15,475.659121,2.00321,-48.13561,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,20,275,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",2335.888197,-0.314,20,325,15,898.391809,4.8184,280.08269,59.9173099999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",432.558815,0,20,400,15,475.659121,2.00321,-21.51562,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,20,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.098686,0,20,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},671.60759,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",106.464246,0.3,20,625,15,126.00477,0.61911,-61.23445,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.051846,{"v":4.3e-05,"d":"4.30E-05"},20,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},172.69444,542.67265,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.051846,{"v":4.3e-05,"d":"4.30E-05"},20,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},172.69444,617.71062,"normal"]
["Maritime","h2","Low-emission ammonia",138.977917,0,20,825,15,126.00477,0.61911,20.95451,747.017229999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",487.250315,0,20,875,15,475.659121,2.00321,5.78631,365.94916,"comp"]
["Maritime","h2","Low-emission ammonia",138.977917,0,20,950,15,126.00477,0.61911,20.95451,868.15874,"comp"]
["Maritime","h2","Low-emission ammonia",138.977917,0,20,1025,15,126.00477,0.61911,20.95451,940.84365,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,20,1125,15,62.166303,0.8654,74.54509,1065.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5728.323197,0,20,1175,15,898.391809,4.8184,1002.3932,1000,"comp"]
["Aviation","comp","Compensation",0.048791,0,22,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,76.01265,"normal"]
["Primary steel","h2","DRI-EAF with H2",388.475715,0.11514,22,100,15,475.659121,2.00321,-46.17594,1000,"ccu"]
["CF","ccu","MTO using fossil CCU",936.279297,1.90135,22,175,15,898.391809,4.8184,12.98829,145.467789999999,"normal"]
["Maritime","h2","Low-emission ammonia",143.899677,0,22,250,15,126.00477,0.61911,28.90424,190.64638,"ccu"]
["Primary steel","h2","DRI-EAF with H2",424.744815,0,22,300,15,475.659121,2.00321,-25.41636,1000,"comp"]
["CF","ccu","MTO using fossil CCU",936.279297,1.90135,22,375,15,898.391809,4.8184,12.98829,318.12386,"normal"]
["Maritime","h2","Low-emission ammonia",143.899677,0,22,450,15,126.00477,0.61911,28.90424,384.47281,"comp"]
["Primary steel","h2","DRI-EAF with H2",388.475715,0.11514,22,525,15,475.659121,2.00321,-46.17594,1000,"normal"]
["Cement","ccs","CCS",156.759572,0,22,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.052667,{"v":4.3e-05,"d":"4.30E-05"},22,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},195.5,494.85443,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.114411,0,22,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},870.65823,1000,"comp"]
["CF","ccu","MTO using fossil CCU",936.279297,1.90135,22,825,15,898.391809,4.8184,12.98829,706.60001,"normal"]
["Aviation","comp","Compensation",0.115975,0,22,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,141.89873,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5048.269297,0,22,1000,15,898.391809,4.8184,861.25633,1000,"comp"]
["Aviation","comp","Compensation",0.131783,0,22,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,157.40507,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.144218,0,22,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1247.96203,1000,"comp"]
["CF","comp","Compensation",970.667809,0,24,0,15,898.391809,4.8184,15,0.24746,"normal"]
["Cement","ccs","CCS",123.202572,0,24,0,15,62.166303,0.8654,70.52955,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",408.295315,0,24,125,15,475.659121,2.00321,-33.62793,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",392.175715,0.11514,24,150,15,475.659121,2.00321,-44.21627,1000,"normal"]
["Maritime","h2","Low-emission ammonia",148.821437,0,24,275,15,126.00477,0.61911,36.85398,215.75482,"comp"]
["Primary steel","h2","DRI-EAF with H2",392.175715,0.11514,24,350,15,475.659121,2.00321,-44.21627,1000,"normal"]
["Maritime","h2","Low-emission ammonia",148.821437,0,24,350,15,126.00477,0.61911,36.85398,288.43973,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.053489,{"v":4.3e-05,"d":"4.30E-05"},24,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},218.33333,296.93249,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,24,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",976.647897,1.90135,24,650,15,898.391809,4.8184,26.82713,549.55255,"normal"]
["Aviation","comp","Compensation",0.102143,0,24,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,138.73418,"ccu"]
["Primary steel","h2","DRI-EAF with H2",483.136315,0,24,775,15,475.659121,2.00321,3.73261,329.838609999999,"comp"]
["CF","efuel","MTO using non-fossil CO2",4742.742897,-0.314,24,850,15,898.391809,4.8184,749.03575,115.964249999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.130135,0,24,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1069.6962,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",392.175715,0.11514,24,1000,15,475.659121,2.00321,-44.21627,1000,"normal"]
["Cement","ccs","CCS",184.480572,0,24,1050,15,62.166303,0.8654,141.33842,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.053489,{"v":4.3e-05,"d":"4.30E-05"},24,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},218.33333,947.26161,"normal"]
["Aviation","comp","Compensation",0.046815,0,26,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,94.87342,"normal"]
["Cement","comp","Compensation",118.417303,0,26,50,15,62.166303,0.8654,65,9.54509,"normal"]
["Aviation","comp","Compensation",0.056695,0,26,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},140.07595,104.55696,"ccu"]
["Maritime","h2","Low-emission ammonia",153.743197,0,26,175,15,126.00477,0.61911,44.80371,119.72174,"comp"]
["Primary steel","h2","DRI-EAF with H2",395.875715,0.11514,26,250,15,475.659121,2.00321,-42.25659,1000,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.081988,0,26,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},460.24051,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",122.864229,0.3,26,400,15,126.00477,0.61911,-9.84156,1000,"normal"]
["Cement","ccs","CCS",150.923572,0,26,475,15,62.166303,0.8654,102.56213,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1017.016497,1.90135,26,550,15,898.391809,4.8184,40.66598,457.25111,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,26,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,26,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",4340.041497,-0.314,26,750,15,898.391809,4.8184,670.57316,94.4268399999999,"ccu"]
["Maritime","h2","Low-emission ammonia",153.743197,0,26,825,15,126.00477,0.61911,44.80371,749.65764,"comp"]
["Primary steel","h2","DRI-EAF with H2",395.875715,0.11514,26,900,15,475.659121,2.00321,-42.25659,1000,"normal"]
["CF","ccu","MTO using fossil CCU",1017.016497,1.90135,26,1000,15,898.391809,4.8184,40.66598,845.72726,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",122.864229,0.3,26,1050,15,126.00477,0.61911,-9.84156,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",395.875715,0.11514,26,1100,15,475.659121,2.00321,-42.25659,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,26,1175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.057261,0,28,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},147.24051,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",409.938315,0,28,75,15,475.659121,2.00321,-32.80775,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",1832.757597,-0.314,28,175,15,898.391809,4.8184,182.05241,7.94758999999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.074293,0,28,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},362.83544,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",128.33089,0.3,28,300,15,126.00477,0.61911,7.2894,45.46405,"normal"]
["Maritime","h2","Low-emission ammonia",158.664957,0,28,400,15,126.00477,0.61911,52.75345,338.65661,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.055131,{"v":4.3e-05,"d":"4.30E-05"},28,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},263.94444,201.29607,"normal"]
["Primary steel","h2","DRI-EAF with H2",399.575715,0.11514,28,525,15,475.659121,2.00321,-40.29692,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,28,600,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,28,675,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",484.779315,0,28,725,15,475.659121,2.00321,4.55279,309.93631,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,28,800,15,62.166303,0.8654,74.54509,740.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",399.575715,0.11514,28,925,15,475.659121,2.00321,-40.29692,1000,"ccu"]
["Maritime","ccu","syn-methanol (fossil CCU)",128.33089,0.3,28,950,15,126.00477,0.61911,7.2894,45.46405,"normal"]
["CF","efuel","MTO using non-fossil CO2",5272.292597,0,28,1025,15,898.391809,4.8184,907.74962,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.055131,{"v":4.3e-05,"d":"4.30E-05"},28,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},263.94444,851.62518,"normal"]
["Maritime","h2","Low-emission ammonia",158.664957,0,28,1150,15,126.00477,0.61911,52.75345,1065.50571,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.060211,0,30,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},184.58228,1000,"comp"]
["CF","comp","Compensation",1332.047809,0,30,75,15,898.391809,4.8184,90,13.58982,"ccu"]
["Aviation","comp","Compensation",0.060647,0,30,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,129.22784,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.055953,{"v":4.3e-05,"d":"4.30E-05"},30,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},286.77778,3.37412,"normal"]
["Primary steel","h2","DRI-EAF with H2",403.275715,0.11514,30,350,15,475.659121,2.00321,-38.33725,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,30,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","ccu","syn-methanol (fossil CCU)",133.797552,0.3,30,450,15,126.00477,0.61911,24.42036,36.28282,"normal"]
["Primary steel","h2","DRI-EAF with H2",468.329815,0,30,550,15,475.659121,2.00321,-3.65878,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,30,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.115567,0,30,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},885.29114,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",133.797552,0.3,30,775,15,126.00477,0.61911,24.42036,36.28282,"normal"]
["Primary steel","h2","DRI-EAF with H2",497.114815,0,30,800,15,475.659121,2.00321,10.71066,332.40162,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.055953,{"v":4.3e-05,"d":"4.30E-05"},30,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},286.77778,653.70323,"normal"]
["Maritime","h2","Low-emission ammonia",163.586717,0,30,975,15,126.00477,0.61911,60.70318,896.78773,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,30,1075,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,30,1150,15,62.166303,0.8654,74.54509,1090.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",163.586717,0,30,1175,15,126.00477,0.61911,60.70318,1090.61416,"comp"]
["Cement","comp","Compensation",118.417303,0,32,50,15,62.166303,0.8654,65,9.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",1545.082297,0,32,100,15,898.391809,4.8184,134.2127,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",139.264213,0.3,32,200,15,126.00477,0.61911,41.55132,27.1015999999999,"normal"]
["Aviation","comp","Compensation",0.064599,0,32,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},240.12658,69.45675,"normal"]
["CF","ccu","MTO using fossil CCU",1138.122297,1.90135,32,325,15,898.391809,4.8184,82.18251,245.09284,"normal"]
["Maritime","h2","Low-emission ammonia",168.508477,0,32,400,15,126.00477,0.61911,68.65292,340.41688,"ccu"]
["Primary steel","h2","DRI-EAF with H2",460.515815,0,32,450,15,475.659121,2.00321,-7.55952,1000,"comp"]
["Maritime","h2","Low-emission ammonia",168.508477,0,32,550,15,126.00477,0.61911,68.65292,485.7867,"ccu"]
["Maritime","h2","Low-emission ammonia",168.508477,0,32,600,15,126.00477,0.61911,68.65292,534.24331,"comp"]
["Primary steel","h2","DRI-EAF with H2",406.975715,0.11514,32,675,15,475.659121,2.00321,-36.37757,1000,"normal"]
["CF","efuel","MTO using non-fossil CO2",4220.937297,0,32,750,15,898.391809,4.8184,689.55369,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.056774,{"v":4.3e-05,"d":"4.30E-05"},32,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},309.58333,530.84705,"normal"]
["Primary steel","h2","DRI-EAF with H2",406.975715,0.11514,32,925,15,475.659121,2.00321,-36.37757,1000,"normal"]
["CF","ccu","MTO using fossil CCU",1138.122297,1.90135,32,975,15,898.391809,4.8184,82.18251,806.22506,"normal"]
["Aviation","comp","Compensation",0.127831,0,32,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,205.50632,"ccu"]
["Primary steel","h2","DRI-EAF with H2",535.356815,0,32,1100,15,475.659121,2.00321,29.80102,427.804,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,32,1175,15,62.166303,0.8654,74.54509,1115.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,34,75,15,62.166303,0.8654,74.54509,15.4549099999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",410.675715,0.11514,34,100,15,475.659121,2.00321,-34.4179,1000,"normal"]
["Cement","ccs","CCS",131.956572,0,34,150,15,62.166303,0.8654,80.6451,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1178.490897,1.90135,34,225,15,898.391809,4.8184,96.02135,143.97865,"normal"]
["CF","efuel","MTO using non-fossil CO2",2511.708397,0,34,325,15,898.391809,4.8184,334.82413,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,34,375,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.082383,0,34,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,171.34177,"ccu"]
["Maritime","h2","Low-emission ammonia",173.430237,0,34,500,15,126.00477,0.61911,76.60265,438.210229999999,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.057596,{"v":4.3e-05,"d":"4.30E-05"},34,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},332.41667,332.9251,"normal"]
["Aviation","comp","Compensation",0.102143,0,34,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,190.72152,"ccu"]
["Maritime","ccu","syn-methanol (fossil CCU)",144.730874,0.3,34,725,15,126.00477,0.61911,58.68229,17.9203599999999,"normal"]
["Cement","ccs","CCS",169.890572,0,34,800,15,62.166303,0.8654,124.47916,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1178.490897,1.90135,34,875,15,898.391809,4.8184,96.02135,713.92362,"normal"]
["Primary steel","h2","DRI-EAF with H2",521.785815,0,34,950,15,475.659121,2.00321,23.02639,377.33226,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,34,1025,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",410.675715,0.11514,34,1150,15,475.659121,2.00321,-34.4179,1000,"normal"]
["Cement","ccs","CCS",193.23457200000001,0,34,1200,15,62.166303,0.8654,151.45397,1000,"comp"]
["Aviation","comp","Compensation",0.052743,0,36,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},90.05063,152.670889999999,"normal"]
["Cement","ccs","CCS",129.038572,0,36,100,15,62.166303,0.8654,77.27325,1000,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",150.197535,0.3,36,150,15,126.00477,0.61911,75.81325,8.73913,"normal"]
["Aviation","comp","Compensation",0.068551,0,36,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},290.1519,168.17721,"ccu"]
["Maritime","h2","Low-emission ammonia",178.351997,0,36,325,15,126.00477,0.61911,84.55238,269.49225,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,36,425,15,62.166303,0.8654,74.54509,365.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3323.441997,-0.314,36,475,15,898.391809,4.8184,472.49828,17.5017199999999,"ccu"]
["Maritime","ccu","syn-methanol (fossil CCU)",150.197535,0.3,36,550,15,126.00477,0.61911,75.81325,8.73913,"normal"]
["Cement","ccs","CCS",159.677572,0,36,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1218.859497,1.90135,36,700,15,898.391809,4.8184,109.8602,556.87616,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.058417,{"v":4.3e-05,"d":"4.30E-05"},36,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},355.22222,410.17019,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,36,850,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",5206.489497,-0.314,36,900,15,898.391809,4.8184,839.39243,75.60757,"ccu"]
["Maritime","h2","Low-emission ammonia",178.351997,0,36,975,15,126.00477,0.61911,84.55238,899.42814,"comp"]
["Primary steel","h2","DRI-EAF with H2",414.375715,0.11514,36,1050,15,475.659121,2.00321,-32.45823,1000,"normal"]
["Maritime","h2","Low-emission ammonia",178.351997,0,36,1100,15,126.00477,0.61911,84.55238,1020.56966,"comp"]
["Maritime","ccu","syn-methanol (fossil CCU)",150.197535,0.3,36,1200,15,126.00477,0.61911,75.81325,8.73913,"normal"]
["Primary steel","h2","DRI-EAF with H2",418.075715,0.11514,38,25,15,475.659121,2.00321,-30.49855,1000,"ccu"]
["CF","ccu","MTO using fossil CCU",1259.228097,1.90135,38,125,15,898.391809,4.8184,123.69904,16.30096,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,38,150,15,62.166303,0.8654,74.54509,90.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",445.709315,0,38,225,15,475.659121,2.00321,-14.95091,1000,"comp"]
["CF","comp","Compensation",2536.647809,0,38,325,15,898.391809,4.8184,340,10.87168,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.091175,0,38,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},576.53165,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",418.075715,0.11514,38,475,15,475.659121,2.00321,-30.49855,1000,"normal"]
["CF","ccu","MTO using fossil CCU",1259.228097,1.90135,38,525,15,898.391809,4.8184,123.69904,399.8287,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.059238,{"v":4.3e-05,"d":"4.30E-05"},38,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},378.02778,237.28868,"normal"]
["Primary steel","h2","DRI-EAF with H2",418.075715,0.11514,38,675,15,475.659121,2.00321,-30.49855,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,38,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",4753.713097,0,38,850,15,898.391809,4.8184,800.12479,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",520.550315,0,38,875,15,475.659121,2.00321,22.40963,349.32584,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,38,950,15,62.166303,0.8654,74.54509,890.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.146531,0,38,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1277.24051,1000,"comp"]
["Maritime","h2","Low-emission ammonia",183.273757,0,38,1100,15,126.00477,0.61911,92.50212,0.442089999999993,"normal"]
["Maritime","comp","Compensation",135.291427,0,40,0,15,126.00477,0.61911,15.00001,41.73641,"normal"]
["Aviation","comp","Compensation",0.048791,0,40,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,169.59493,"normal"]
["Maritime","comp","Compensation",181.724714,0,40,75,15,126.00477,0.61911,90.00007,10.45178,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,40,175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2054.807809,0,40,225,15,898.391809,4.8184,240,32.4090899999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,40,300,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,40,375,15,62.166303,0.8654,74.54509,315.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3044.484197,0,40,425,15,898.391809,4.8184,445.39523,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,40,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",159.677572,0,40,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",504.100815,0,40,700,15,475.659121,2.00321,14.19806,290.74998,"comp"]
["Maritime","h2","Low-emission ammonia",188.195517,0,40,725,15,126.00477,0.61911,100.45185,639.54874,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.132448,0,40,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1098.97468,1000,"comp"]
["Maritime","h2","Low-emission ammonia",188.195517,0,40,925,15,126.00477,0.61911,100.45185,9.62332,"normal"]
["CF","efuel","MTO using non-fossil CO2",5730.296697,-0.314,40,1000,15,898.391809,4.8184,941.45135,73.5486499999999,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.06006,{"v":4.3e-05,"d":"4.30E-05"},40,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},400.86111,689.695849999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",5720.339197,0,40,1075,15,898.391809,4.8184,1000.73622,1000,"comp"]
["Cement","comp","Compensation",75.147303,0,42,0,15,62.166303,0.8654,15,59.54509,"normal"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",181.597504,0,42,25,15,126.00477,0.61911,89.7946,18.6069899999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",441.595315,0,42,125,15,475.659121,2.00321,-17.00461,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,42,200,15,62.166303,0.8654,74.54509,140.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2364.430297,0,42,250,15,898.391809,4.8184,304.25836,1000,"comp"]
["Maritime","h2","Low-emission ammonia",193.117277,0,42,350,15,126.00477,0.61911,108.40159,18.80454,"normal"]
["Primary steel","h2","DRI-EAF with H2",425.475715,0.11514,42,400,15,475.659121,2.00321,-26.57921,1000,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.060881,{"v":4.3e-05,"d":"4.30E-05"},42,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},423.66667,91.5991499999999,"normal"]
["Maritime","h2","Low-emission ammonia",193.117277,0,42,550,15,126.00477,0.61911,108.40159,456.59886,"ccu"]
["Primary steel","h2","DRI-EAF with H2",496.286815,0,42,600,15,475.659121,2.00321,10.29732,256.48647,"comp"]
["CF","efuel","MTO using non-fossil CO2",4441.455297,-0.314,42,700,15,898.391809,4.8184,690.33269,24.66731,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,42,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",425.475715,0.11514,42,825,15,475.659121,2.00321,-26.57921,1000,"normal"]
["CF","efuel","MTO using non-fossil CO2",5040.285297,0,42,900,15,898.391809,4.8184,859.59935,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.060881,{"v":4.3e-05,"d":"4.30E-05"},42,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},423.66667,566.83966,"normal"]
["CF","ccu","MTO using fossil CCU",1339.965297,1.90135,42,1050,15,898.391809,4.8184,151.37673,841.10408,"normal"]
["CF","ccu","MTO using fossil CCU",1339.965297,1.90135,42,1125,15,898.391809,4.8184,151.37673,905.8501,"normal"]
["Aviation","comp","Compensation",0.139687,0,42,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,269.126589999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",433.781315,0,44,25,15,475.659121,2.00321,-20.90535,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,44,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.076606,0,44,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},392.11392,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",429.175715,0.11514,44,250,15,475.659121,2.00321,-24.61954,1000,"normal"]
["Cement","ccs","CCS",140.710572,0,44,300,15,62.166303,0.8654,90.76065,1000,"comp"]
["Aviation","comp","Compensation",0.078431,0,44,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,31.2570299999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",429.175715,0.11514,44,450,15,475.659121,2.00321,-24.61954,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,44,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.094239,0,44,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,234.949359999999,"ccu"]
["Maritime","h2","Low-emission ammonia",198.039037,0,44,650,15,126.00477,0.61911,116.35132,587.98074,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,44,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,44,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","h2","Low-emission ammonia",198.039037,0,44,875,15,126.00477,0.61911,116.35132,27.9857699999999,"normal"]
["Cement","ccs","CCS",178.644572,0,44,950,15,62.166303,0.8654,134.59472,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1380.333897,1.90135,44,1025,15,898.391809,4.8184,165.21557,813.548669999999,"normal"]
["Maritime","h2","Low-emission ammonia",198.039037,0,44,1100,15,126.00477,0.61911,116.35132,998.64957,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6212.746397,0,44,1175,15,898.391809,4.8184,1102.92931,1000,"comp"]
["CF","comp","Compensation",970.667809,0,46,0,15,898.391809,4.8184,15,86.76734,"ccu"]
["Maritime","h2","Low-emission ammonia",202.960797,0,46,75,15,126.00477,0.61911,124.30106,31.60989,"comp"]
["Primary steel","h2","DRI-EAF with H2",432.875715,0.11514,46,150,15,475.659121,2.00321,-22.65986,1000,"normal"]
["Maritime","h2","Low-emission ammonia",202.960797,0,46,225,15,126.00477,0.61911,124.30106,37.16699,"normal"]
["Maritime","h2","Low-emission ammonia",202.960797,0,46,300,15,126.00477,0.61911,124.30106,37.16699,"normal"]
["Aviation","comp","Compensation",0.080407,0,46,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,231.78481,"ccu"]
["CF","ccu","MTO using fossil CCU",1420.702497,1.90135,46,450,15,898.391809,4.8184,179.05442,285.94558,"normal"]
["Aviation","comp","Compensation",0.086335,0,46,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,237.59494,"ccu"]
["Primary steel","h2","DRI-EAF with H2",500.808315,0,46,575,15,475.659121,2.00321,12.55445,244.68828,"comp"]
["CF","efuel","MTO using non-fossil CO2",4300.657497,-0.314,46,650,15,898.391809,4.8184,662.89956,2.10044000000004,"ccu"]
["Cement","ccs","CCS",168.431572,0,46,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1420.702497,1.90135,46,850,15,898.391809,4.8184,179.05442,656.501199999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",432.875715,0.11514,46,925,15,475.659121,2.00321,-22.65986,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,46,1000,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",432.875715,0.11514,46,1000,15,475.659121,2.00321,-22.65986,1000,"ccu"]
["Maritime","h2","Low-emission ammonia",202.960797,0,46,1125,15,126.00477,0.61911,124.30106,1049.19863,"comp"]
["Primary steel","h2","DRI-EAF with H2",432.875715,0.11514,46,1200,15,475.659121,2.00321,-22.65986,1000,"normal"]
["CF","comp","Compensation",970.667809,0,48,0,15,898.391809,4.8184,15,94.63278,"ccu"]
["Maritime","h2","Low-emission ammonia",207.882557,0,48,125,15,126.00477,0.61911,132.25079,7.74932000000001,"normal"]
["Cement","ccs","CCS",134.874572,0,48,200,15,62.166303,0.8654,84.01695,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1461.071097,1.90135,48,275,15,898.391809,4.8184,192.89326,97.10674,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.091023,0,48,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},574.60759,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,48,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3259.407809,0,48,475,15,898.391809,4.8184,490,29.6909399999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.108056,0,48,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.21519,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",436.575715,0.11514,48,625,15,475.659121,2.00321,-20.70019,1000,"normal"]
["Maritime","h2","Low-emission ammonia",207.882557,0,48,700,15,126.00477,0.61911,132.25079,582.74978,"ccu"]
["Maritime","h2","Low-emission ammonia",207.882557,0,48,775,15,126.00477,0.61911,132.25079,46.34823,"normal"]
["Primary steel","h2","DRI-EAF with H2",436.575715,0.11514,48,825,15,475.659121,2.00321,-20.70019,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,48,900,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.123879,0,48,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},990.50633,284.810129999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",436.575715,0.11514,48,1075,15,475.659121,2.00321,-20.70019,1000,"normal"]
["CF","efuel","MTO using non-fossil CO2",6445.608597,-0.314,48,1125,15,898.391809,4.8184,1080.82316,59.17684,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.163412,0,48,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1490.92405,1000,"comp"]
["Maritime","comp","Compensation",150.769189,0,50,25,15,126.00477,0.61911,40.00003,85.1140499999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,50,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["Aviation","comp","Compensation",0.060647,0,50,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,233.20253,"normal"]
["Maritime","h2","Low-emission ammonia",212.804317,0,50,225,15,126.00477,0.61911,140.20052,99.7996699999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,50,325,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2777.567809,0,50,375,15,898.391809,4.8184,390,51.2283499999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3452.162197,0,50,475,15,898.391809,4.8184,530.00382,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,50,525,15,62.166303,0.8654,74.54509,465.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3863.832197,0,50,575,15,898.391809,4.8184,615.44089,1000,"comp"]
["Maritime","h2","Low-emission ammonia",212.804317,0,50,675,15,126.00477,0.61911,140.20052,55.52946,"normal"]
["Maritime","h2","Low-emission ammonia",212.804317,0,50,750,15,126.00477,0.61911,140.20052,55.52946,"normal"]
["CF","ccu","MTO using fossil CCU",1501.439697,1.90135,50,800,15,898.391809,4.8184,206.73211,601.390379999999,"normal"]
["Maritime","h2","Low-emission ammonia",212.804317,0,50,875,15,126.00477,0.61911,140.20052,749.80019,"ccu"]
["Primary steel","h2","DRI-EAF with H2",548.507315,0,50,925,15,475.659121,2.00321,36.36573,354.45186,"comp"]
["CF","efuel","MTO using non-fossil CO2",6042.907197,-0.314,50,1025,15,898.391809,4.8184,1002.36057,37.6394299999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",568.656815,0,50,1100,15,475.659121,2.00321,46.42434,411.18068,"comp"]
["Aviation","comp","Compensation",0.046815,0,52,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,230.03797,"normal"]
["CF","efuel","MTO using non-fossil CO2",1537.098297,0,52,0,15,898.391809,4.8184,132.55572,1000,"comp"]
["Aviation","comp","Compensation",0.052743,0,52,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},90.05063,235.8481,"normal"]
["Primary steel","h2","DRI-EAF with H2",443.975715,0.11514,52,150,15,475.659121,2.00321,-16.78084,1000,"ccu"]
["Cement","ccs","CCS",137.792572,0,52,250,15,62.166303,0.8654,87.3888,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,52,350,15,62.166303,0.8654,74.54509,290.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",486.001815,0,52,350,15,475.659121,2.00321,5.16306,166.21011,"comp"]
["Maritime","h2","Low-emission ammonia",217.726077,0,52,500,15,126.00477,0.61911,148.15026,64.71068,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.064988,{"v":4.3e-05,"d":"4.30E-05"},52,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},537.75,2.52847999999994,"normal"]
["Primary steel","h2","DRI-EAF with H2",443.975715,0.11514,52,575,15,475.659121,2.00321,-16.78084,1000,"normal"]
["Maritime","h2","Low-emission ammonia",217.726077,0,52,700,15,126.00477,0.61911,148.15026,566.85031,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.064988,{"v":4.3e-05,"d":"4.30E-05"},52,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},537.75,202.629749999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",5307.903297,-0.314,52,850,15,898.391809,4.8184,859.15195,5.84804999999994,"ccu"]
["Maritime","h2","Low-emission ammonia",217.726077,0,52,875,15,126.00477,0.61911,148.15026,809.55601,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,52,1000,15,62.166303,0.8654,74.54509,940.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5859.633297,0,52,1050,15,898.391809,4.8184,1029.645,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.064988,{"v":4.3e-05,"d":"4.30E-05"},52,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},537.75,602.83228,"normal"]
["Primary steel","h2","DRI-EAF with H2",443.975715,0.11514,52,1150,15,475.659121,2.00321,-16.78084,1000,"ccu"]
["CF","comp","Compensation",1211.587809,0,54,50,15,898.391809,4.8184,65,111.39313,"normal"]
["Maritime","comp","Compensation",212.680238,0,54,125,15,126.00477,0.61911,140.00011,16.0998799999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",469.552315,0,54,175,15,475.659121,2.00321,-3.04851,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,54,250,15,62.166303,0.8654,74.54509,190.454909999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,54,300,15,62.166303,0.8654,74.54509,240.454909999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",447.675715,0.11514,54,400,15,475.659121,2.00321,-14.82117,1000,"normal"]
["CF","efuel","MTO using non-fossil CO2",3532.899397,0,54,475,15,898.391809,4.8184,546.75983,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.065809,{"v":4.3e-05,"d":"4.30E-05"},54,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},560.55556,4.73558000000002,"normal"]
["Maritime","h2","Low-emission ammonia",222.647837,0,54,600,15,126.00477,0.61911,156.09999,458.9005,"ccu"]
["CF","ccu","MTO using fossil CCU",1582.176897,1.90135,54,675,15,898.391809,4.8184,234.40979,455.59021,"normal"]
["Aviation","comp","Compensation",0.106095,0,54,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,298.569619999999,"ccu"]
["Maritime","h2","Low-emission ammonia",222.647837,0,54,800,15,126.00477,0.61911,156.09999,737.75124,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,54,900,15,62.166303,0.8654,74.54509,840.45491,"ccu"]
["Aviation","comp","Compensation",0.125855,0,54,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,317.936709999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",447.675715,0.11514,54,1050,15,475.659121,2.00321,-14.82117,1000,"normal"]
["Cement","ccs","CCS",187.398572,0,54,1100,15,62.166303,0.8654,144.71027,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1582.176897,1.90135,54,1175,15,898.391809,4.8184,234.40979,913.17372,"normal"]
["Maritime","comp","Compensation",150.769189,0,56,25,15,126.00477,0.61911,40.00003,111.603659999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",451.375715,0.11514,56,75,15,475.659121,2.00321,-12.8615,1000,"normal"]
["Aviation","comp","Compensation",0.060647,0,56,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,264.3924,"ccu"]
["Maritime","h2","Low-emission ammonia",227.569597,0,56,225,15,126.00477,0.61911,164.04973,181.380389999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",451.375715,0.11514,56,300,15,475.659121,2.00321,-12.8615,1000,"normal"]
["Primary steel","h2","DRI-EAF with H2",499.158815,0,56,400,15,475.659121,2.00321,11.73102,178.72428,"comp"]
["Maritime","h2","Low-emission ammonia",227.569597,0,56,450,15,126.00477,0.61911,164.04973,83.0731299999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",451.375715,0.11514,56,500,15,475.659121,2.00321,-12.8615,1000,"ccu"]
["CF","ccu","MTO using fossil CCU",1622.545497,1.90135,56,600,15,898.391809,4.8184,248.24864,366.75136,"normal"]
["Aviation","comp","Compensation",0.098191,0,56,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,301.21519,"ccu"]
["Cement","ccs","CCS",168.431572,0,56,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["CF","comp","Compensation",4825.387809,0,56,800,15,898.391809,4.8184,815,16.71882,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.139019,0,56,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1182.1519,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",451.375715,0.11514,56,950,15,475.659121,2.00321,-12.8615,1000,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.066631,{"v":4.3e-05,"d":"4.30E-05"},56,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},583.38889,482.15541,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,56,1150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",451.375715,0.11514,56,1150,15,475.659121,2.00321,-12.8615,1000,"ccu"]
["Maritime","h2","Low-emission ammonia",232.491357,0,58,50,15,126.00477,0.61911,171.99946,12.6624099999999,"comp"]
["Aviation","comp","Compensation",0.052743,0,58,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},90.05063,267.03798,"ccu"]
["Maritime","h2","Low-emission ammonia",232.491357,0,58,175,15,126.00477,0.61911,171.99946,133.80392,"comp"]
["Maritime","h2","Low-emission ammonia",232.491357,0,58,275,15,126.00477,0.61911,171.99946,92.25436,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.090872,0,58,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},572.6962,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1662.914097,1.90135,58,425,15,898.391809,4.8184,262.08748,177.912519999999,"normal"]
["Cement","ccs","CCS",148.005572,0,58,425,15,62.166303,0.8654,99.19028,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",455.075715,0.11514,58,550,15,475.659121,2.00321,-10.90182,1000,"ccu"]
["CF","comp","Compensation",3982.167809,0,58,625,15,898.391809,4.8184,640,48.51021,"ccu"]
["Maritime","h2","Low-emission ammonia",232.491357,0,58,700,15,126.00477,0.61911,171.99946,642.5983,"comp"]
["Primary steel","h2","DRI-EAF with H2",455.075715,0.11514,58,775,15,475.659121,2.00321,-10.90182,1000,"normal"]
["CF","ccu","MTO using fossil CCU",1662.914097,1.90135,58,825,15,898.391809,4.8184,262.08748,577.91252,"normal"]
["Maritime","h2","Low-emission ammonia",232.491357,0,58,925,15,126.00477,0.61911,171.99946,92.25436,"normal"]
["Primary steel","h2","DRI-EAF with H2",455.075715,0.11514,58,975,15,475.659121,2.00321,-10.90182,1000,"ccu"]
["CF","ccu","MTO using fossil CCU",1662.914097,1.90135,58,1075,15,898.391809,4.8184,262.08748,814.89888,"normal"]
["Aviation","comp","Compensation",0.135735,0,58,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1140.58228,348.43038,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.167519,0,58,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1542.91139,1000,"comp"]
["CF","comp","Compensation",1211.587809,0,60,50,15,898.391809,4.8184,65,134.98946,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.07679,0,60,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},394.44304,1000,"comp"]
["Maritime","h2","Low-emission ammonia",237.413117,0,60,175,15,126.00477,0.61911,179.9492,10.05095,"normal"]
["Maritime","h2","Low-emission ammonia",237.413117,0,60,225,15,126.00477,0.61911,179.9492,60.05099,"ccu"]
["Aviation","comp","Compensation",0.072503,0,60,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},340.17722,288.82278,"normal"]
["Primary steel","h2","DRI-EAF with H2",458.775715,0.11514,60,400,15,475.659121,2.00321,-8.94215,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,60,475,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3500.327809,0,60,525,15,898.391809,4.8184,540,70.04762,"ccu"]
["Primary steel","h2","DRI-EAF with H2",458.775715,0.11514,60,600,15,475.659121,2.00321,-8.94215,1000,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,60,675,15,62.166303,0.8654,74.54509,615.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.132146,0,60,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1095.1519,1000,"comp"]
["Maritime","h2","Low-emission ammonia",237.413117,0,60,825,15,126.00477,0.61911,179.9492,101.43559,"normal"]
["Primary steel","h2","DRI-EAF with H2",458.775715,0.11514,60,875,15,475.659121,2.00321,-8.94215,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,60,975,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","h2","Low-emission ammonia",237.413117,0,60,1025,15,126.00477,0.61911,179.9492,860.051629999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",584.278315,0,60,1075,15,475.659121,2.00321,54.22257,393.84139,"comp"]
["CF","efuel","MTO using non-fossil CO2",6909.355197,-0.314,60,1175,15,898.391809,4.8184,1171.17984,18.8201599999999,"ccu"]
["Aviation","comp","Compensation",0.046815,0,62,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,282.02531,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,62,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2356.446297,0,62,150,15,898.391809,4.8184,302.60138,1000,"comp"]
["Aviation","comp","Compensation",0.064599,0,62,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},240.12658,299.468359999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",462.475715,0.11514,62,300,15,475.659121,2.00321,-6.98248,1000,"ccu"]
["Maritime","h2","Low-emission ammonia",242.334877,0,62,375,15,126.00477,0.61911,187.89893,110.61682,"normal"]
["Maritime","h2","Low-emission ammonia",242.334877,0,62,450,15,126.00477,0.61911,187.89893,277.101439999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",521.772815,0,62,500,15,475.659121,2.00321,23.0199,205.59964,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,62,575,15,62.166303,0.8654,74.54509,515.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",242.334877,0,62,700,15,126.00477,0.61911,187.89893,644.35857,"comp"]
["Primary steel","h2","DRI-EAF with H2",462.475715,0.11514,62,725,15,475.659121,2.00321,-6.98248,1000,"normal"]
["Maritime","h2","Low-emission ammonia",242.334877,0,62,850,15,126.00477,0.61911,187.89893,677.10176,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.069095,{"v":4.3e-05,"d":"4.30E-05"},62,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},651.83333,238.622369999999,"normal"]
["Maritime","h2","Low-emission ammonia",242.334877,0,62,925,15,126.00477,0.61911,187.89893,752.10182,"ccu"]
["Cement","ccs","CCS",181.562572,0,62,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["Aviation","comp","Compensation",0.131783,0,62,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,365.34177,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6678.981297,0,62,1200,15,898.391809,4.8184,1199.69066,1000,"comp"]
["Cement","comp","Compensation",75.147303,0,64,0,15,62.166303,0.8654,15,59.54509,"ccu"]
["CF","comp","Compensation",1572.967809,0,64,125,15,898.391809,4.8184,140,140.466369999999,"normal"]
["CF","comp","Compensation",1934.347809,0,64,200,15,898.391809,4.8184,215,88.60401,"normal"]
["Maritime","h2","Low-emission ammonia",247.256637,0,64,275,15,126.00477,0.61911,195.84867,94.1515599999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",505.323315,0,64,325,15,475.659121,2.00321,14.80833,147.02378,"comp"]
["Maritime","h2","Low-emission ammonia",247.256637,0,64,350,15,126.00477,0.61911,195.84867,169.15162,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.110369,0,64,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},819.49367,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",466.175715,0.11514,64,550,15,475.659121,2.00321,-5.0228,1000,"normal"]
["CF","efuel","MTO using non-fossil CO2",4352.247397,0,64,625,15,898.391809,4.8184,716.80549,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.069916,{"v":4.3e-05,"d":"4.30E-05"},64,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},674.63889,40.7282,"normal"]
["Primary steel","h2","DRI-EAF with H2",466.175715,0.11514,64,775,15,475.659121,2.00321,-5.0228,1000,"ccu"]
["Maritime","h2","Low-emission ammonia",247.256637,0,64,850,15,126.00477,0.61911,195.84867,669.15202,"ccu"]
["Aviation","comp","Compensation",0.117951,0,64,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,362.177219999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",580.164315,0,64,975,15,475.659121,2.00321,52.16887,357.73084,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,64,1050,15,62.166303,0.8654,74.54509,990.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,64,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",466.175715,0.11514,64,1200,15,475.659121,2.00321,-5.0228,1000,"normal"]
["Cement","ccs","CCS",124.661572,0,66,25,15,62.166303,0.8654,72.21547,1000,"comp"]
["Aviation","comp","Compensation",0.056695,0,66,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},140.07595,312.50633,"normal"]
["Maritime","comp","Compensation",243.635763,0,66,175,15,126.00477,0.61911,190.00015,13.7982499999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2848.853497,0,66,250,15,898.391809,4.8184,404.79447,1000,"comp"]
["Aviation","comp","Compensation",0.072503,0,66,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},340.17722,328.01265,"ccu"]
["Maritime","h2","Low-emission ammonia",252.178397,0,66,375,15,126.00477,0.61911,203.7984,331.15089,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,66,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["Aviation","comp","Compensation",0.088311,0,66,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,343.50633,"ccu"]
["Maritime","h2","Low-emission ammonia",252.178397,0,66,600,15,126.00477,0.61911,203.7984,128.97927,"normal"]
["Cement","ccs","CCS",162.595572,0,66,675,15,62.166303,0.8654,116.04954,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1824.388497,1.90135,66,750,15,898.391809,4.8184,317.44286,447.55714,"normal"]
["Aviation","comp","Compensation",0.110047,0,66,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,364.82279,"ccu"]
["Maritime","h2","Low-emission ammonia",252.178397,0,66,900,15,126.00477,0.61911,203.7984,128.97927,"normal"]
["CF","comp","Compensation",5548.147809,0,66,950,15,898.391809,4.8184,965,35.53809,"ccu"]
["Maritime","h2","Low-emission ammonia",252.178397,0,66,1025,15,126.00477,0.61911,203.7984,961.08679,"comp"]
["Primary steel","h2","DRI-EAF with H2",469.875715,0.11514,66,1100,15,475.659121,2.00321,-3.06313,1000,"normal"]
["Cement","ccs","CCS",190.316572,0,66,1150,15,62.166303,0.8654,148.08212,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",478.181315,0,68,25,15,475.659121,2.00321,1.25908,46.08029,"comp"]
["Primary steel","h2","DRI-EAF with H2",473.575715,0.11514,68,75,15,475.659121,2.00321,-1.10346,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,68,150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.064599,0,68,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},240.12658,330.65823,"ccu"]
["CF","comp","Compensation",2416.187809,0,68,300,15,898.391809,4.8184,315,132.27131,"ccu"]
["CF","comp","Compensation",2777.567809,0,68,375,15,898.391809,4.8184,390,122.017339999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.107753,0,68,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},786.37975,1000,"comp"]
["Maritime","h2","Low-emission ammonia",257.100157,0,68,500,15,126.00477,0.61911,211.74813,138.1605,"normal"]
["Cement","ccs","CCS",156.759572,0,68,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["Aviation","comp","Compensation",0.100167,0,68,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,29.92335,"normal"]
["Primary steel","h2","DRI-EAF with H2",473.575715,0.11514,68,725,15,475.659121,2.00321,-1.10346,1000,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,68,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",473.575715,0.11514,68,925,15,475.659121,2.00321,-1.10346,1000,"normal"]
["Maritime","h2","Low-emission ammonia",257.100157,0,68,925,15,126.00477,0.61911,211.74813,865.05371,"comp"]
["Maritime","h2","Low-emission ammonia",257.100157,0,68,1075,15,126.00477,0.61911,211.74813,138.1605,"normal"]
["Primary steel","h2","DRI-EAF with H2",473.575715,0.11514,68,1125,15,475.659121,2.00321,-1.10346,1000,"ccu"]
["Maritime","h2","Low-emission ammonia",257.100157,0,68,1150,15,126.00477,0.61911,211.74813,138.1605,"normal"]
["Aviation","comp","Compensation",0.050767,0,70,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},65.03797,327.49368,"ccu"]
["Primary steel","h2","DRI-EAF with H2",477.275715,0.11514,70,75,15,475.659121,2.00321,0.85622,51.01292,"ccu"]
["CF","comp","Compensation",1934.347809,0,70,200,15,898.391809,4.8184,215,153.80872,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.093671,0,70,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},608.12658,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",477.275715,0.11514,70,350,15,475.659121,2.00321,0.85622,51.01292,"normal"]
["Cement","ccs","CCS",146.546572,0,70,400,15,62.166303,0.8654,97.50436,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1905.125697,1.90135,70,450,15,898.391809,4.8184,345.12055,119.87945,"normal"]
["Primary steel","h2","DRI-EAF with H2",477.275715,0.11514,70,550,15,475.659121,2.00321,0.85622,51.01292,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,70,625,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.102143,0,70,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,377.87342,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.131995,0,70,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1093.24051,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,70,825,15,62.166303,0.8654,74.54509,765.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.149027,0,70,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1308.83544,1000,"comp"]
["Maritime","h2","Low-emission ammonia",262.021917,0,70,975,15,126.00477,0.61911,219.69787,147.34173,"normal"]
["Cement","ccs","CCS",184.480572,0,70,1050,15,62.166303,0.8654,141.33842,1000,"comp"]
["Maritime","h2","Low-emission ammonia",262.021917,0,70,1075,15,126.00477,0.61911,219.69787,870.303,"ccu"]
["Maritime","h2","Low-emission ammonia",262.021917,0,70,1175,15,126.00477,0.61911,219.69787,970.303069999999,"ccu"]
["Cement","comp","Compensation",118.417303,0,72,50,15,62.166303,0.8654,65,9.54509,"normal"]
["CF","comp","Compensation",1452.507809,0,72,100,15,898.391809,4.8184,115,175.34613,"ccu"]
["Primary steel","h2","DRI-EAF with H2",502.852315,0,72,175,15,475.659121,2.00321,13.57481,91.01093,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,72,250,15,62.166303,0.8654,74.54509,190.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3175.794297,0,72,300,15,898.391809,4.8184,472.64704,1000,"comp"]
["Maritime","h2","Low-emission ammonia",266.943677,0,72,400,15,126.00477,0.61911,227.6476,156.52296,"normal"]
["Primary steel","h2","DRI-EAF with H2",480.975715,0.11514,72,450,15,475.659121,2.00321,2.81589,49.05325,"ccu"]
["Cement","ccs","CCS",155.300572,0,72,550,15,62.166303,0.8654,107.61991,1000,"comp"]
["Maritime","h2","Low-emission ammonia",266.943677,0,72,600,15,126.00477,0.61911,227.6476,387.35289,"ccu"]
["Primary steel","h2","DRI-EAF with H2",557.543815,0,72,650,15,475.659121,2.00321,40.87674,244.98917,"comp"]
["CF","comp","Compensation",4584.467809,0,72,750,15,898.391809,4.8184,765,86.4783499999999,"ccu"]
["CF","comp","Compensation",4945.847809,0,72,825,15,898.391809,4.8184,840,76.22438,"ccu"]
["Primary steel","h2","DRI-EAF with H2",480.975715,0.11514,72,875,15,475.659121,2.00321,2.81589,49.05325,"normal"]
["CF","efuel","MTO using non-fossil CO2",5851.649297,0,72,950,15,898.391809,4.8184,1027.98802,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.073202,{"v":4.3e-05,"d":"4.30E-05"},72,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.91667,274.614979999999,"normal"]
["Maritime","h2","Low-emission ammonia",266.943677,0,72,1075,15,126.00477,0.61911,227.6476,862.35327,"ccu"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.073202,{"v":4.3e-05,"d":"4.30E-05"},72,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.91667,449.70358,"normal"]
["Aviation","comp","Compensation",0.046815,0,74,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,344.40506,"ccu"]
["Primary steel","h2","DRI-EAF with H2",495.038315,0,74,75,15,475.659121,2.00321,9.67407,56.7474299999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,74,150,15,62.166303,0.8654,74.54509,90.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2804.492897,0,74,200,15,898.391809,4.8184,395.58797,1000,"comp"]
["Maritime","h2","Low-emission ammonia",271.865437,0,74,325,15,126.00477,0.61911,235.59734,286.21483,"comp"]
["Cement","ccs","CCS",143.628572,0,74,350,15,62.166303,0.8654,94.1325,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",541.094315,0,74,475,15,475.659121,2.00321,32.66517,186.41331,"comp"]
["Maritime","h2","Low-emission ammonia",271.865437,0,74,500,15,126.00477,0.61911,235.59734,279.403069999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,74,600,15,62.166303,0.8654,74.54509,540.45491,"ccu"]
["Aviation","comp","Compensation",0.098191,0,74,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,394.78481,"ccu"]
["Maritime","h2","Low-emission ammonia",271.865437,0,74,700,15,126.00477,0.61911,235.59734,649.63938,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.074023,{"v":4.3e-05,"d":"4.30E-05"},74,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},788.72222,76.72082,"normal"]
["CF","efuel","MTO using non-fossil CO2",5480.347897,0,74,850,15,898.391809,4.8184,950.92896,1000,"comp"]
["CF","ccu","MTO using fossil CCU",1985.862897,1.90135,74,975,15,898.391809,4.8184,372.79823,617.20177,"normal"]
["Cement","ccs","CCS",181.562572,0,74,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",615.935315,0,74,1125,15,475.659121,2.00321,70.02571,397.12037,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,74,1200,15,62.166303,0.8654,74.54509,1140.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.074845,0,76,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},369.82278,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",488.375715,0.11514,76,125,15,475.659121,2.00321,6.73523,45.13391,"normal"]
["Cement","ccs","CCS",133.415572,0,76,175,15,62.166303,0.8654,82.33102,1000,"comp"]
["Aviation","comp","Compensation",0.068551,0,76,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},290.1519,376.113919999999,"normal"]
["Maritime","h2","Low-emission ammonia",276.787197,0,76,325,15,126.00477,0.61911,243.54707,96.4532,"ccu"]
["Maritime","h2","Low-emission ammonia",276.787197,0,76,375,15,126.00477,0.61911,243.54707,146.45324,"ccu"]
["Aviation","comp","Compensation",0.084359,0,76,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},490.25316,391.62026,"ccu"]
["Maritime","h2","Low-emission ammonia",276.787197,0,76,525,15,126.00477,0.61911,243.54707,480.9214,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,76,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4800.293997,0,76,675,15,898.391809,4.8184,809.79209,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,76,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",171.349572,0,76,825,15,62.166303,0.8654,126.16509,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2026.231497,1.90135,76,900,15,898.391809,4.8184,386.63708,528.36292,"normal"]
["Maritime","h2","Low-emission ammonia",276.787197,0,76,975,15,126.00477,0.61911,243.54707,746.45372,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6138.221497,0,76,1000,15,898.391809,4.8184,1087.46258,1000,"comp"]
["CF","comp","Compensation",6270.907809,0,76,1100,15,898.391809,4.8184,1115,54.35735,"ccu"]
["Maritime","h2","Low-emission ammonia",276.787197,0,76,1175,15,126.00477,0.61911,243.54707,1110.85729,"comp"]
["Primary steel","h2","DRI-EAF with H2",492.075715,0.11514,78,25,15,475.659121,2.00321,8.69491,31.30509,"normal"]
["CF","efuel","MTO using non-fossil CO2",2473.560097,0,78,100,15,898.391809,4.8184,326.90692,1000,"comp"]
["Aviation","comp","Compensation",0.058671,0,78,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},165.08861,376.822779999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",492.075715,0.11514,78,225,15,475.659121,2.00321,8.69491,43.17423,"ccu"]
["CF","comp","Compensation",2536.647809,0,78,325,15,898.391809,4.8184,340,60.4759199999999,"normal"]
["Aviation","comp","Compensation",0.076455,0,78,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},390.20253,394.265819999999,"ccu"]
["Maritime","h2","Low-emission ammonia",281.708957,0,78,475,15,126.00477,0.61911,251.49681,433.34492,"comp"]
["CF","comp","Compensation",3500.327809,0,78,525,15,898.391809,4.8184,540,140.836599999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.124635,0,78,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1000.07595,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",492.075715,0.11514,78,675,15,475.659121,2.00321,8.69491,43.17423,"normal"]
["Cement","ccs","CCS",165.513572,0,78,725,15,62.166303,0.8654,119.42139,1000,"comp"]
["Cement","ccs","CCS",168.431572,0,78,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",492.075715,0.11514,78,875,15,475.659121,2.00321,8.69491,43.17423,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,78,950,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.127831,0,78,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,444.64557,"ccu"]
["Maritime","h2","Low-emission ammonia",281.708957,0,78,1075,15,126.00477,0.61911,251.49681,1014.82421,"comp"]
["CF","comp","Compensation",6511.827809,0,78,1150,15,898.391809,4.8184,1165,55.3868099999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.076487,0,80,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},390.60759,1000,"comp"]
["Maritime","comp","Compensation",181.724714,0,80,75,15,126.00477,0.61911,90.00007,169.44647,"normal"]
["Aviation","comp","Compensation",0.062623,0,80,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},215.11392,391.10127,"ccu"]
["CF","comp","Compensation",2295.727809,0,80,275,15,898.391809,4.8184,290,124.31477,"normal"]
["Maritime","h2","Low-emission ammonia",286.630717,0,80,275,15,126.00477,0.61911,259.44654,30.5536899999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,80,375,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3018.487809,0,80,425,15,898.391809,4.8184,440,162.37401,"ccu"]
["Cement","ccs","CCS",155.300572,0,80,550,15,62.166303,0.8654,107.61991,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.129714,0,80,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1064.36709,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",495.775715,0.11514,80,700,15,475.659121,2.00321,10.65458,41.21456,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,80,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",495.775715,0.11514,80,775,15,475.659121,2.00321,10.65458,41.21456,"ccu"]
["Primary steel","h2","DRI-EAF with H2",495.775715,0.11514,80,900,15,475.659121,2.00321,10.65458,41.21456,"normal"]
["Maritime","h2","Low-emission ammonia",286.630717,0,80,925,15,126.00477,0.61911,259.44654,680.55421,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.165909,0,80,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1522.53165,1000,"comp"]
["Maritime","h2","Low-emission ammonia",286.630717,0,80,1125,15,126.00477,0.61911,259.44654,193.247869999999,"normal"]
["Cement","ccs","CCS",193.23457200000001,0,80,1200,15,62.166303,0.8654,151.45397,1000,"comp"]
["Cement","comp","Compensation",118.417303,0,82,50,15,62.166303,0.8654,65,9.54509,"normal"]
["Primary steel","h2","DRI-EAF with H2",499.475715,0.11514,82,125,15,475.659121,2.00321,12.61425,39.25489,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,82,200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2175.267809,0,82,250,15,898.391809,4.8184,265,194.165399999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3377.637297,0,82,300,15,898.391809,4.8184,514.53708,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,82,400,15,62.166303,0.8654,74.54509,340.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3995.142297,0,82,450,15,898.391809,4.8184,642.6927,1000,"comp"]
["Maritime","h2","Low-emission ammonia",291.552477,0,82,550,15,126.00477,0.61911,267.39627,202.4291,"normal"]
["Primary steel","h2","DRI-EAF with H2",499.475715,0.11514,82,600,15,475.659121,2.00321,12.61425,39.25489,"ccu"]
["Aviation","comp","Compensation",0.100167,0,82,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,438.31646,"ccu"]
["Maritime","h2","Low-emission ammonia",291.552477,0,82,750,15,126.00477,0.61911,267.39627,497.60434,"ccu"]
["Primary steel","h2","DRI-EAF with H2",593.314815,0,82,800,15,475.659121,2.00321,58.73358,284.3787,"comp"]
["CF","comp","Compensation",5307.227809,0,82,900,15,898.391809,4.8184,915,105.29762,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.158214,0,82,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1425.12658,1000,"comp"]
["Maritime","h2","Low-emission ammonia",291.552477,0,82,1050,15,126.00477,0.61911,267.39627,202.4291,"normal"]
["CF","efuel","MTO using non-fossil CO2",6670.997297,0,82,1100,15,898.391809,4.8184,1198.03368,1000,"comp"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.077309,{"v":4.3e-05,"d":"4.30E-05"},82,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},880,310.60759,"normal"]
["Primary steel","h2","DRI-EAF with H2",503.175715,0.11514,84,25,15,475.659121,2.00321,14.57393,25.42607,"ccu"]
["Cement","ccs","CCS",127.579572,0,84,75,15,62.166303,0.8654,75.58732,1000,"comp"]
["Aviation","comp","Compensation",0.058671,0,84,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},165.08861,408.02531,"ccu"]
["Primary steel","h2","DRI-EAF with H2",530.809315,0,84,225,15,475.659121,2.00321,27.53091,96.1369599999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,84,300,15,62.166303,0.8654,74.54509,240.454909999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.110066,0,84,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.65823,1000,"comp"]
["CF","comp","Compensation",3138.947809,0,84,450,15,898.391809,4.8184,465,174.68691,"ccu"]
["Cement","ccs","CCS",152.382572,0,84,500,15,62.166303,0.8654,104.24806,1000,"comp"]
["Aviation","comp","Compensation",0.094239,0,84,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,287.4891,"normal"]
["Maritime","h2","Low-emission ammonia",296.474237,0,84,650,15,126.00477,0.61911,275.34601,389.65452,"ccu"]
["Maritime","h2","Low-emission ammonia",296.474237,0,84,700,15,126.00477,0.61911,275.34601,654.04007,"comp"]
["Aviation","comp","Compensation",0.110047,0,84,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,458.405059999999,"ccu"]
["Maritime","h2","Low-emission ammonia",296.474237,0,84,850,15,126.00477,0.61911,275.34601,799.40989,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,84,950,15,62.166303,0.8654,74.54509,890.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6299.695897,0,84,1000,15,898.391809,4.8184,1120.97462,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",503.175715,0.11514,84,1075,15,475.659121,2.00321,14.57393,37.29521,"ccu"]
["Cement","ccs","CCS",190.316572,0,84,1150,15,62.166303,0.8654,148.08212,1000,"comp"]
["CF","comp","Compensation",970.667809,0,86,0,15,898.391809,4.8184,15,244.076199999999,"normal"]
["Maritime","comp","Compensation",181.724714,0,86,75,15,126.00477,0.61911,90.00007,193.29567,"ccu"]
["Primary steel","h2","DRI-EAF with H2",522.995315,0,86,125,15,475.659121,2.00321,23.63017,61.87345,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,86,225,15,62.166303,0.8654,74.54509,165.454909999999,"ccu"]
["Maritime","h2","Low-emission ammonia",301.395997,0,86,275,15,126.00477,0.61911,283.29574,243.039049999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",506.875715,0.11514,86,350,15,475.659121,2.00321,16.5336,35.33554,"normal"]
["Maritime","h2","Low-emission ammonia",301.395997,0,86,475,15,126.00477,0.61911,283.29574,206.704649999999,"ccu"]
["CF","ccu","MTO using fossil CCU",2228.074497,1.90135,86,500,15,898.391809,4.8184,455.8313,59.1687,"normal"]
["Aviation","comp","Compensation",0.096215,0,86,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,455.227849999999,"ccu"]
["CF","ccu","MTO using fossil CCU",2228.074497,1.90135,86,650,15,898.391809,4.8184,455.8313,209.1687,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,86,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5619.641997,0,86,825,15,898.391809,4.8184,979.83774,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.15134,0,86,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1338.11392,1000,"comp"]
["Cement","ccs","CCS",180.103572,0,86,975,15,62.166303,0.8654,136.28064,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2228.074497,1.90135,86,1050,15,898.391809,4.8184,455.8313,609.1687,"normal"]
["Maritime","h2","Low-emission ammonia",301.395997,0,86,1125,15,126.00477,0.61911,283.29574,856.70516,"ccu"]
["Maritime","h2","Low-emission ammonia",301.395997,0,86,1200,15,126.00477,0.61911,283.29574,220.791549999999,"normal"]
["Aviation","comp","Compensation",0.050767,0,88,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},65.03797,421.0633,"ccu"]
["Maritime","h2","Low-emission ammonia",306.317757,0,88,100,15,126.00477,0.61911,291.24548,74.32105,"comp"]
["Primary steel","h2","DRI-EAF with H2",510.575715,0.11514,88,175,15,475.659121,2.00321,18.49327,33.37587,"normal"]
["CF","efuel","MTO using non-fossil CO2",3292.908097,0,88,250,15,898.391809,4.8184,496.95258,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",549.723315,0,88,325,15,475.659121,2.00321,36.97276,124.85935,"comp"]
["Cement","ccs","CCS",146.546572,0,88,400,15,62.166303,0.8654,97.50436,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2268.443097,1.90135,88,475,15,898.391809,4.8184,469.67014,20.3298599999999,"normal"]
["Aviation","comp","Compensation",0.088311,0,88,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,457.87342,"ccu"]
["Primary steel","h2","DRI-EAF with H2",581.386815,0,88,600,15,475.659121,2.00321,52.77914,214.00465,"comp"]
["CF","efuel","MTO using non-fossil CO2",4836.670597,0,88,625,15,898.391809,4.8184,817.3416,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.141516,0,88,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1213.75949,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",510.575715,0.11514,88,825,15,475.659121,2.00321,18.49327,33.37587,"normal"]
["Cement","ccs","CCS",174.267572,0,88,875,15,62.166303,0.8654,129.53694,1000,"comp"]
["CF","comp","Compensation",5668.607809,0,88,975,15,898.391809,4.8184,990,118.639969999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",510.575715,0.11514,88,1025,15,475.659121,2.00321,18.49327,33.37587,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,88,1100,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.139687,0,88,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,508.253169999999,"ccu"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",297.797388,0,90,0,15,126.00477,0.61911,277.48319,21.7120199999999,"comp"]
["Aviation","comp","Compensation",0.056695,0,90,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},140.07595,437.278479999999,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.093369,0,90,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},604.3038,1000,"comp"]
["Maritime","comp","Compensation",274.591288,0,90,225,15,126.00477,0.61911,240.00019,59.1950199999999,"normal"]
["Cement","ccs","CCS",140.710572,0,90,300,15,62.166303,0.8654,90.76065,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",514.275715,0.11514,90,375,15,475.659121,2.00321,20.45295,31.41619,"ccu"]
["Maritime","h2","Low-emission ammonia",311.239517,0,90,425,15,126.00477,0.61911,299.19521,140.80514,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,90,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3741.247809,0,90,575,15,898.391809,4.8184,590,181.193279999999,"ccu"]
["Maritime","h2","Low-emission ammonia",311.239517,0,90,650,15,126.00477,0.61911,299.19521,608.22387,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,90,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5494.544197,0,90,775,15,898.391809,4.8184,953.87523,1000,"comp"]
["Maritime","h2","Low-emission ammonia",311.239517,0,90,875,15,126.00477,0.61911,299.19521,239.154009999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",514.275715,0.11514,90,925,15,475.659121,2.00321,20.45295,31.41619,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.165757,0,90,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1520.60759,1000,"comp"]
["Maritime","h2","Low-emission ammonia",311.239517,0,90,1075,15,126.00477,0.61911,299.19521,790.80566,"ccu"]
["Primary steel","h2","DRI-EAF with H2",645.535315,0,90,1125,15,475.659121,2.00321,84.80199,382.34409,"comp"]
["CF","comp","Compensation",970.667809,0,92,0,15,898.391809,4.8184,15,267.67253,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.085674,0,92,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},506.89873,1000,"comp"]
["Maritime","comp","Compensation",228.158001,0,92,150,15,126.00477,0.61911,165.00013,142.144819999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3167.810297,0,92,200,15,898.391809,4.8184,470.99006,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,92,350,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",517.975715,0.11514,92,350,15,475.659121,2.00321,22.41262,29.45652,"ccu"]
["Maritime","h2","Low-emission ammonia",316.161277,0,92,475,15,126.00477,0.61911,307.14495,439.50588,"comp"]
["Primary steel","h2","DRI-EAF with H2",517.975715,0.11514,92,525,15,475.659121,2.00321,22.41262,29.45652,"normal"]
["Primary steel","h2","DRI-EAF with H2",583.029815,0,92,550,15,475.659121,2.00321,53.59932,194.10235,"comp"]
["Maritime","h2","Low-emission ammonia",316.161277,0,92,700,15,126.00477,0.61911,307.14495,248.33523,"normal"]
["Primary steel","h2","DRI-EAF with H2",517.975715,0.11514,92,750,15,475.659121,2.00321,22.41262,29.45652,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,92,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","h2","Low-emission ammonia",316.161277,0,92,900,15,126.00477,0.61911,307.14495,607.85578,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,92,1000,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6029.987809,0,92,1050,15,898.391809,4.8184,1065,124.11688,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.175095,0,92,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1638.81013,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7078.675297,0,92,1150,15,898.391809,4.8184,1282.64226,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",2487.756397,0,94,25,15,898.391809,4.8184,329.85319,1000,"comp"]
["Maritime","comp","Compensation",212.680238,0,94,125,15,126.00477,0.61911,140.00011,175.094569999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",521.675715,0.11514,94,175,15,475.659121,2.00321,24.37229,27.49685,"ccu"]
["Aviation","comp","Compensation",0.068551,0,94,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},290.1519,469.6962,"normal"]
["Maritime","h2","Low-emission ammonia",321.083037,0,94,325,15,126.00477,0.61911,315.09468,24.90559,"ccu"]
["Primary steel","h2","DRI-EAF with H2",566.580315,0,94,375,15,475.659121,2.00321,45.38775,135.52649,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,94,450,15,62.166303,0.8654,74.54509,390.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.126948,0,94,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1029.35443,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",586.729815,0,94,550,15,475.659121,2.00321,55.44636,192.25531,"comp"]
["CF","efuel","MTO using non-fossil CO2",5163.611397,0,94,675,15,898.391809,4.8184,885.19417,1000,"comp"]
["Aviation","comp","Compensation",0.106095,0,94,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,251.496479999999,"normal"]
["Maritime","h2","Low-emission ammonia",321.083037,0,94,800,15,126.00477,0.61911,315.09468,499.905969999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,94,900,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",177.185572,0,94,925,15,62.166303,0.8654,132.90879,1000,"comp"]
["Maritime","h2","Low-emission ammonia",321.083037,0,94,1000,15,126.00477,0.61911,315.09468,949.18039,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,94,1100,15,62.166303,0.8654,74.54509,1040.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7119.043897,0,94,1150,15,898.391809,4.8184,1291.02027,1000,"comp"]
["Cement","comp","Compensation",118.417303,0,96,50,15,62.166303,0.8654,65,9.54509,"ccu"]
["Cement","ccs","CCS",127.579572,0,96,75,15,62.166303,0.8654,75.58732,1000,"comp"]
["CF","comp","Compensation",1693.427809,0,96,150,15,898.391809,4.8184,165,262.89547,"normal"]
["Maritime","comp","Compensation",274.591288,0,96,225,15,126.00477,0.61911,240.00019,83.04422,"ccu"]
["Primary steel","h2","DRI-EAF with H2",558.766315,0,96,275,15,475.659121,2.00321,41.48701,101.26298,"comp"]
["Aviation","comp","Compensation",0.074479,0,96,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},365.18987,485.89874,"normal"]
["Maritime","h2","Low-emission ammonia",326.004797,0,96,425,15,126.00477,0.61911,323.04441,392.80955,"comp"]
["Primary steel","h2","DRI-EAF with H2",525.375715,0.11514,96,500,15,475.659121,2.00321,26.33197,25.53717,"normal"]
["CF","efuel","MTO using non-fossil CO2",4792.309997,0,96,575,15,898.391809,4.8184,808.1351,1000,"comp"]
["Maritime","h2","Low-emission ammonia",326.004797,0,96,675,15,126.00477,0.61911,323.04441,366.956139999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",525.375715,0.11514,96,700,15,475.659121,2.00321,26.33197,25.53717,"ccu"]
["CF","ccu","MTO using fossil CCU",2429.917497,1.90135,96,800,15,898.391809,4.8184,525.02552,289.974479999999,"normal"]
["Aviation","comp","Compensation",0.113999,0,96,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,524.65823,"ccu"]
["Primary steel","h2","DRI-EAF with H2",633.607315,0,96,925,15,475.659121,2.00321,78.84755,311.97004,"comp"]
["Primary steel","h2","DRI-EAF with H2",525.375715,0.11514,96,1050,15,475.659121,2.00321,26.33197,25.53717,"normal"]
["Cement","ccs","CCS",188.857572,0,96,1125,15,62.166303,0.8654,146.3962,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",525.375715,0.11514,96,1150,15,475.659121,2.00321,26.33197,25.53717,"normal"]
["Maritime","comp","Compensation",166.246952,0,98,50,15,126.00477,0.61911,65.00005,265.9941,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2774.328597,0,98,75,15,898.391809,4.8184,389.32774,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",529.075715,0.11514,98,125,15,475.659121,2.00321,28.29164,23.5775,"ccu"]
["Maritime","h2","Low-emission ammonia",330.926557,0,98,250,15,126.00477,0.61911,330.99415,224.091559999999,"comp"]
["Aviation","comp","Compensation",0.068551,0,98,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},290.1519,490.49367,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4112.256097,0,98,400,15,898.391809,4.8184,666.99823,1000,"comp"]
["Aviation","comp","Compensation",0.082383,0,98,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,504.05063,"ccu"]
["Cement","ccs","CCS",155.300572,0,98,550,15,62.166303,0.8654,107.61991,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2470.286097,1.90135,98,625,15,898.391809,4.8184,538.86436,101.135639999999,"normal"]
["Cement","ccs","CCS",159.677572,0,98,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",617.157815,0,98,750,15,475.659121,2.00321,70.63598,253.39418,"comp"]
["Maritime","h2","Low-emission ammonia",330.926557,0,98,825,15,126.00477,0.61911,330.99415,275.87891,"normal"]
["Maritime","h2","Low-emission ammonia",330.926557,0,98,900,15,126.00477,0.61911,330.99415,854.02745,"comp"]
["Primary steel","h2","DRI-EAF with H2",529.075715,0.11514,98,975,15,475.659121,2.00321,28.29164,23.5775,"normal"]
["Cement","ccs","CCS",183.021572,0,98,1025,15,62.166303,0.8654,139.65249,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",654.578315,0,98,1075,15,475.659121,2.00321,89.31624,358.74772,"comp"]
["Primary steel","h2","DRI-EAF with H2",529.075715,0.11514,98,1175,15,475.659121,2.00321,28.29164,23.5775,"ccu"]
["CF","comp","Compensation",1211.587809,0,100,50,15,898.391809,4.8184,65,292.29832,"normal"]
["Aviation","comp","Compensation",0.054719,0,100,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},115.06329,487.316459999999,"ccu"]
["Maritime","h2","Low-emission ammonia",335.848317,0,100,150,15,126.00477,0.61911,338.94388,128.05848,"comp"]
["Cement","ccs","CCS",136.333572,0,100,225,15,62.166303,0.8654,85.70288,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.11025,0,100,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},817.98734,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",532.775715,0.11514,100,400,15,475.659121,2.00321,30.25131,21.61783,"normal"]
["Cement","ccs","CCS",149.464572,0,100,450,15,62.166303,0.8654,100.87621,1000,"comp"]
["Aviation","comp","Compensation",0.086335,0,100,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,518.32912,"normal"]
["Primary steel","h2","DRI-EAF with H2",532.775715,0.11514,100,600,15,475.659121,2.00321,30.25131,21.61783,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,100,675,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4464.007809,0,100,725,15,898.391809,4.8184,740,200.01255,"ccu"]
["Maritime","h2","Low-emission ammonia",335.848317,0,100,800,15,126.00477,0.61911,338.94388,757.994379999999,"comp"]
["Maritime","h2","Low-emission ammonia",335.848317,0,100,850,15,126.00477,0.61911,338.94388,806.45098,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.165606,0,100,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1518.6962,1000,"comp"]
["Maritime","h2","Low-emission ammonia",335.848317,0,100,1025,15,126.00477,0.61911,338.94388,285.06014,"normal"]
["Primary steel","h2","DRI-EAF with H2",532.775715,0.11514,100,1075,15,475.659121,2.00321,30.25131,21.61783,"ccu"]
["CF","ccu","MTO using fossil CCU",2510.654697,1.90135,100,1175,15,898.391809,4.8184,552.70321,637.29679,"normal"]
["Primary steel","comp","Compensation",505.707271,0,102,0,15,475.659121,2.00321,15,17.21098,"ccu"]
["Primary steel","h2","DRI-EAF with H2",543.959815,0,102,50,15,475.659121,2.00321,34.09562,22.78481,"comp"]
["CF","comp","Compensation",1693.427809,0,102,150,15,898.391809,4.8184,165,286.49179,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.102555,0,102,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},720.58228,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,102,275,15,62.166303,0.8654,74.54509,215.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3987.158297,0,102,350,15,898.391809,4.8184,641.03571,1000,"comp"]
["Aviation","comp","Compensation",0.080407,0,102,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,522.91139,"normal"]
["Primary steel","h2","DRI-EAF with H2",536.475715,0.11514,102,500,15,475.659121,2.00321,32.21098,19.65816,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,102,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","ccu","MTO using fossil CCU",2551.023297,1.90135,102,650,15,898.391809,4.8184,566.54205,98.4579499999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",618.800815,0,102,700,15,475.659121,2.00321,71.45616,233.49187999999901,"comp"]
["Maritime","h2","Low-emission ammonia",340.770077,0,102,850,15,126.00477,0.61911,346.89362,294.24136,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.157911,0,102,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1421.29114,1000,"comp"]
["Aviation","comp","Compensation",0.123879,0,102,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},990.50633,565.53164,"ccu"]
["Maritime","h2","Low-emission ammonia",340.770077,0,102,1050,15,126.00477,0.61911,346.89362,718.107229999999,"ccu"]
["Aviation","comp","Compensation",0.131783,0,102,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,17.58193,"normal"]
["CF","comp","Compensation",6752.747809,0,102,1200,15,898.391809,4.8184,1215,142.93615,"ccu"]
["Cement","comp","Compensation",75.147303,0,104,0,15,62.166303,0.8654,15,59.54509,"normal"]
["Maritime","comp","Compensation",212.680238,0,104,125,15,126.00477,0.61911,140.00011,214.843239999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",3307.104397,0,104,175,15,898.391809,4.8184,499.89884,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,104,200,15,62.166303,0.8654,74.54509,140.454909999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",540.175715,0.11514,104,325,15,475.659121,2.00321,34.17066,17.69848,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,104,400,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,104,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",602.351315,0,104,525,15,475.659121,2.00321,63.24459,174.91602,"comp"]
["CF","comp","Compensation",3982.167809,0,104,625,15,898.391809,4.8184,640,229.415399999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.143829,0,104,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1243.03797,1000,"comp"]
["CF","comp","Compensation",4584.467809,0,104,750,15,898.391809,4.8184,765,212.325439999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5982.959397,0,104,825,15,898.391809,4.8184,1055.23983,1000,"comp"]
["Aviation","comp","Compensation",0.117951,0,104,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,215.50387,"normal"]
["Primary steel","h2","DRI-EAF with H2",540.175715,0.11514,104,975,15,475.659121,2.00321,34.17066,17.69848,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,104,1050,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","ccu","Syn-kerosene (fossil CCU)",0.086344,{"v":4.3e-05,"d":"4.30E-05"},104,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1130.97222,9.61005999999997,"normal"]
["Primary steel","h2","DRI-EAF with H2",677.192315,0,104,1175,15,475.659121,2.00321,100.60513,385.623079999999,"comp"]
["Cement","comp","Compensation",96.782303,0,106,25,15,62.166303,0.8654,40,34.54509,"ccu"]
["CF","efuel","MTO using non-fossil CO2",2935.802997,0,106,75,15,898.391809,4.8184,422.83978,1000,"comp"]
["Maritime","h2","Low-emission ammonia",350.613597,0,106,150,15,126.00477,0.61911,362.79309,130.69889,"comp"]
["Cement","ccs","CCS",136.333572,0,106,225,15,62.166303,0.8654,85.70288,1000,"comp"]
["Aviation","comp","Compensation",0.072503,0,106,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},340.17722,535.94936,"normal"]
["Maritime","h2","Low-emission ammonia",350.613597,0,106,375,15,126.00477,0.61911,362.79309,27.20722,"ccu"]
["Primary steel","h2","DRI-EAF with H2",594.537315,0,106,425,15,475.659121,2.00321,59.34385,140.65251,"comp"]
["Primary steel","h2","DRI-EAF with H2",543.875715,0.11514,106,525,15,475.659121,2.00321,36.13033,15.73881,"ccu"]
["Maritime","h2","Low-emission ammonia",350.613597,0,106,575,15,126.00477,0.61911,362.79309,542.58005,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,106,675,15,62.166303,0.8654,74.54509,615.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5611.657997,0,106,725,15,898.391809,4.8184,978.18076,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2631.760497,1.90135,106,800,15,898.391809,4.8184,594.21974,220.78026,"normal"]
["Cement","ccs","CCS",174.267572,0,106,875,15,62.166303,0.8654,129.53694,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2631.760497,1.90135,106,950,15,898.391809,4.8184,594.21974,370.78026,"normal"]
["Aviation","comp","Compensation",0.125855,0,106,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,588.26582,"ccu"]
["Primary steel","h2","DRI-EAF with H2",669.378315,0,106,1075,15,475.659121,2.00321,96.70439,351.35957,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.185103,0,106,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1765.49367,1000,"comp"]
["Maritime","efuel","Syn-methanol (non-fossil CO2)",346.997338,0,108,0,15,126.00477,0.61911,356.95202,13.7907999999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",547.575715,0.11514,108,75,15,475.659121,2.00321,38.09,13.7791399999999,"normal"]
["Cement","ccs","CCS",130.497572,0,108,125,15,62.166303,0.8654,78.95917,1000,"comp"]
["Aviation","comp","Compensation",0.064599,0,108,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},240.12658,538.59494,"normal"]
["Maritime","comp","Compensation",321.024575,0,108,300,15,126.00477,0.61911,315.00025,55.74257,"ccu"]
["Maritime","h2","Low-emission ammonia",355.535357,0,108,400,15,126.00477,0.61911,370.74282,373.86206,"comp"]
["Aviation","comp","Compensation",0.080407,0,108,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,554.10126,"ccu"]
["Maritime","h2","Low-emission ammonia",355.535357,0,108,475,15,126.00477,0.61911,370.74282,446.54697,"comp"]
["Primary steel","h2","DRI-EAF with H2",547.575715,0.11514,108,575,15,475.659121,2.00321,38.09,13.7791399999999,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.141214,0,108,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1209.93671,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2672.129097,1.90135,108,775,15,898.391809,4.8184,608.05858,181.94142,"normal"]
["Cement","ccs","CCS",168.431572,0,108,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",652.928815,0,108,900,15,475.659121,2.00321,88.49282,292.78371,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,108,950,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,108,1000,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",547.575715,0.11514,108,1125,15,475.659121,2.00321,38.09,13.7791399999999,"normal"]
["Maritime","h2","Low-emission ammonia",355.535357,0,108,1125,15,126.00477,0.61911,370.74282,1076.48286,"comp"]
["CF","comp","Compensation",1211.587809,0,110,50,15,898.391809,4.8184,65,331.62553,"ccu"]
["Primary steel","h2","DRI-EAF with H2",551.275715,0.11514,110,100,15,475.659121,2.00321,40.04968,11.81946,"ccu"]
["CF","comp","Compensation",1934.347809,0,110,200,15,898.391809,4.8184,215,311.11758,"normal"]
["Aviation","comp","Compensation",0.066575,0,110,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},265.13924,550.93671,"ccu"]
["Primary steel","h2","DRI-EAF with H2",590.423315,0,110,325,15,475.659121,2.00321,57.29015,104.54196,"comp"]
["Maritime","comp","Compensation",351.980099,0,110,350,15,126.00477,0.61911,365.00029,13.6922599999999,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.127131,0,110,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1031.67089,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",551.275715,0.11514,110,550,15,475.659121,2.00321,40.04968,11.81946,"normal"]
["Cement","ccs","CCS",158.218572,0,110,600,15,62.166303,0.8654,110.99176,1000,"comp"]
["Aviation","comp","Compensation",0.102143,0,110,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,484.04958,"normal"]
["Primary steel","h2","DRI-EAF with H2",633.600815,0,110,700,15,475.659121,2.00321,78.8443,226.10374,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,110,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.117951,0,110,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,601.31646,"ccu"]
["Maritime","h2","Low-emission ammonia",360.457117,0,110,950,15,126.00477,0.61911,378.69255,907.76488,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,110,1050,15,62.166303,0.8654,74.54509,990.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.182487,0,110,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1732.37975,1000,"comp"]
["Maritime","h2","Low-emission ammonia",360.457117,0,110,1175,15,126.00477,0.61911,378.69255,330.96628,"normal"]
["Cement","ccs","CCS",124.661572,0,112,25,15,62.166303,0.8654,72.21547,1000,"comp"]
["CF","comp","Compensation",1452.507809,0,112,100,15,898.391809,4.8184,115,332.65499,"normal"]
["CF","comp","Compensation",1934.347809,0,112,200,15,898.391809,4.8184,215,318.98303,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,112,250,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2416.187809,0,112,300,15,898.391809,4.8184,315,305.31106,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.119436,0,112,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},934.26582,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.127953,0,112,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1042.07595,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",4806.506297,0,112,500,15,898.391809,4.8184,811.08137,1000,"comp"]
["Maritime","h2","Low-emission ammonia",365.378877,0,112,600,15,126.00477,0.61911,386.64229,228.3582,"normal"]
["Primary steel","h2","DRI-EAF with H2",554.975715,0.11514,112,650,15,475.659121,2.00321,42.00935,9.85979,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,112,725,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","h2","Low-emission ammonia",365.378877,0,112,825,15,126.00477,0.61911,386.64229,453.35838,"ccu"]
["Primary steel","h2","DRI-EAF with H2",654.571815,0,112,850,15,475.659121,2.00321,89.313,272.88141,"comp"]
["CF","comp","Compensation",5548.147809,0,112,950,15,898.391809,4.8184,965,216.443279999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.174792,0,112,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1634.97468,1000,"comp"]
["Maritime","h2","Low-emission ammonia",365.378877,0,112,1075,15,126.00477,0.61911,386.64229,340.1475,"normal"]
["Primary steel","h2","DRI-EAF with H2",554.975715,0.11514,112,1200,15,475.659121,2.00321,42.00935,9.85979,"normal"]
["Aviation","comp","Compensation",0.046815,0,114,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,552.35443,"normal"]
["Maritime","comp","Compensation",166.246952,0,114,50,15,126.00477,0.61911,65.00005,329.59197,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,114,150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",3714.782397,0,114,225,15,898.391809,4.8184,584.50743,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",592.066315,0,114,275,15,475.659121,2.00321,58.11033,84.6396599999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,114,350,15,62.166303,0.8654,74.54509,290.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",558.675715,0.11514,114,475,15,475.659121,2.00321,43.96902,7.90012,"ccu"]
["Maritime","h2","Low-emission ammonia",370.300637,0,114,500,15,126.00477,0.61911,394.59202,120.40839,"normal"]
["Aviation","comp","Compensation",0.094239,0,114,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,598.86076,"ccu"]
["Primary steel","h2","DRI-EAF with H2",638.122315,0,114,675,15,475.659121,2.00321,81.10143,214.30554,"comp"]
["Maritime","h2","Low-emission ammonia",370.300637,0,114,700,15,126.00477,0.61911,394.59202,320.40855,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.16071,0,114,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1456.72152,1000,"comp"]
["Maritime","h2","Low-emission ammonia",370.300637,0,114,875,15,126.00477,0.61911,394.59202,349.32873,"normal"]
["CF","efuel","MTO using non-fossil CO2",6802.307397,0,114,975,15,898.391809,4.8184,1225.28549,1000,"comp"]
["Aviation","comp","Compensation",0.129807,0,114,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,179.51126,"normal"]
["Primary steel","h2","DRI-EAF with H2",558.675715,0.11514,114,1125,15,475.659121,2.00321,43.96902,7.90012,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,114,1200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",551.377077,0,116,0,15,475.659121,2.00321,37.79831,6.35266999999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",575.616815,0,116,100,15,475.659121,2.00321,49.89876,26.0637999999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,116,175,15,62.166303,0.8654,74.54509,115.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.112563,0,116,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},847.26582,1000,"comp"]
["CF","comp","Compensation",2295.727809,0,116,275,15,898.391809,4.8184,290,324.459939999999,"ccu"]
["Cement","ccs","CCS",145.087572,0,116,375,15,62.166303,0.8654,95.81843,1000,"comp"]
["Aviation","comp","Compensation",0.084359,0,116,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},490.25316,599.56962,"normal"]
["Maritime","h2","Low-emission ammonia",375.222397,0,116,525,15,126.00477,0.61911,402.54176,137.45867,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,116,625,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.098191,0,116,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,602.51934,"normal"]
["Maritime","h2","Low-emission ammonia",375.222397,0,116,725,15,126.00477,0.61911,402.54176,692.350549999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,116,825,15,62.166303,0.8654,74.54509,765.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6431.005997,0,116,875,15,898.391809,4.8184,1148.22642,1000,"comp"]
["Maritime","h2","Low-emission ammonia",375.222397,0,116,975,15,126.00477,0.61911,402.54176,358.50996,"normal"]
["Maritime","h2","Low-emission ammonia",375.222397,0,116,1000,15,126.00477,0.61911,402.54176,958.861889999999,"comp"]
["CF","ccu","MTO using fossil CCU",2833.603497,1.90135,116,1100,15,898.391809,4.8184,663.41396,451.58604,"normal"]
["Maritime","h2","Low-emission ammonia",375.222397,0,116,1175,15,126.00477,0.61911,402.54176,787.459179999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",551.377077,0,118,0,15,475.659121,2.00321,37.79831,8.19970999999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",566.075715,0.11514,118,125,15,475.659121,2.00321,47.88837,3.98076999999999,"normal"]
["Maritime","h2","Low-emission ammonia",380.144157,0,118,150,15,126.00477,0.61911,410.49149,135.979709999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",566.075715,0.11514,118,225,15,475.659121,2.00321,47.88837,3.98076999999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",4104.272097,0,118,300,15,898.391809,4.8184,665.34125,1000,"comp"]
["Aviation","comp","Compensation",0.076455,0,118,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},390.20253,602.21519,"normal"]
["CF","comp","Compensation",3018.487809,0,118,425,15,898.391809,4.8184,440,237.252799999999,"normal"]
["CF","comp","Compensation",3500.327809,0,118,525,15,898.391809,4.8184,540,137.252799999999,"normal"]
["Aviation","comp","Compensation",0.092263,0,118,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,617.70886,"ccu"]
["Maritime","h2","Low-emission ammonia",380.144157,0,118,625,15,126.00477,0.61911,410.49149,596.31748,"comp"]
["CF","efuel","MTO using non-fossil CO2",5956.787097,0,118,750,15,898.391809,4.8184,1049.80809,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.158095,0,118,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1423.62025,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",566.075715,0.11514,118,875,15,475.659121,2.00321,47.88837,3.98076999999999,"normal"]
["Cement","ccs","CCS",177.185572,0,118,925,15,62.166303,0.8654,132.90879,1000,"comp"]
["CF","ccu","MTO using fossil CCU",2873.972097,1.90135,118,1000,15,898.391809,4.8184,677.2528,337.7472,"normal"]
["Aviation","comp","Compensation",0.135735,0,118,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1140.58228,660.34177,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,118,1150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.046815,0,120,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,583.5443,"ccu"]
["Maritime","h2","Low-emission ammonia",385.065917,0,120,50,15,126.00477,0.61911,418.44123,39.9466299999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",569.775715,0.11514,120,125,15,475.659121,2.00321,49.84804,2.0211,"normal"]
["Primary steel","h2","DRI-EAF with H2",569.775715,0.11514,120,200,15,475.659121,2.00321,49.84804,2.0211,"normal"]
["Maritime","comp","Compensation",305.546812,0,120,275,15,126.00477,0.61911,290.00023,128.441,"normal"]
["Aviation","comp","Compensation",0.078431,0,120,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,614.544299999999,"ccu"]
["CF","comp","Compensation",3018.487809,0,120,425,15,898.391809,4.8184,440,251.091649999999,"normal"]
["Cement","ccs","CCS",153.841572,0,120,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,120,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",569.775715,0.11514,120,700,15,475.659121,2.00321,49.84804,2.0211,"normal"]
["Cement","ccs","CCS",166.972572,0,120,750,15,62.166303,0.8654,121.10731,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",569.775715,0.11514,120,775,15,475.659121,2.00321,49.84804,2.0211,"normal"]
["CF","comp","Compensation",5307.227809,0,120,900,15,898.391809,4.8184,915,254.741029999999,"ccu"]
["Maritime","h2","Low-emission ammonia",385.065917,0,120,925,15,126.00477,0.61911,418.44123,376.872409999999,"normal"]
["Aviation","comp","Compensation",0.129807,0,120,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,664.92405,"ccu"]
["Maritime","h2","Low-emission ammonia",385.065917,0,120,1100,15,126.00477,0.61911,418.44123,1057.53537999999,"comp"]
["Aviation","comp","Compensation",0.139687,0,120,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,122.892409999999,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.095865,0,122,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},635.89873,1000,"comp"]
["Maritime","comp","Compensation",197.202476,0,122,100,15,126.00477,0.61911,115.00009,311.39087,"normal"]
["Cement","ccs","CCS",133.415572,0,122,175,15,62.166303,0.8654,82.33102,1000,"comp"]
["CF","comp","Compensation",2175.267809,0,122,250,15,898.391809,4.8184,265,351.474259999999,"normal"]
["Maritime","h2","Low-emission ammonia",389.987677,0,122,300,15,126.00477,0.61911,426.39096,283.1098,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,122,400,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3138.947809,0,122,450,15,898.391809,4.8184,465,324.130329999999,"ccu"]
["Maritime","h2","Low-emission ammonia",389.987677,0,122,525,15,126.00477,0.61911,426.39096,501.164529999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,122,575,15,62.166303,0.8654,74.54509,515.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5625.854297,0,122,650,15,898.391809,4.8184,981.12703,1000,"comp"]
["Maritime","h2","Low-emission ammonia",389.987677,0,122,750,15,126.00477,0.61911,426.39096,338.60965,"normal"]
["Primary steel","h2","DRI-EAF with H2",573.475715,0.11514,122,800,15,475.659121,2.00321,51.80772,0.0614199999999982,"ccu"]
["CF","ccu","MTO using fossil CCU",2954.709297,1.90135,122,900,15,898.391809,4.8184,704.93049,210.06951,"normal"]
["CF","ccu","MTO using fossil CCU",2954.709297,1.90135,122,950,15,898.391809,4.8184,704.93049,260.06951,"normal"]
["Primary steel","h2","DRI-EAF with H2",690.342815,0,122,1000,15,475.659121,2.00321,107.16984,312.27094,"comp"]
["CF","comp","Compensation",6270.907809,0,122,1100,15,898.391809,4.8184,1115,235.262549999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.191674,0,122,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1848.67089,1000,"comp"]
["Primary steel","comp","Compensation",555.787521,0,124,25,15,475.659121,2.00321,40,11.86914,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.10094500000000001,0,124,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},700.20253,1000,"comp"]
["Aviation","comp","Compensation",0.058671,0,124,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},165.08861,615.962019999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,124,225,15,475.659121,2.00321,51.86914,1.89824999999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,124,300,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,124,350,15,475.659121,2.00321,51.86914,1.89824999999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",627.837315,0,124,425,15,475.659121,2.00321,75.96717,124.02919,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,124,500,15,62.166303,0.8654,74.54509,440.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.143526,0,124,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1239.20253,1000,"comp"]
["Maritime","h2","Low-emission ammonia",394.909437,0,124,650,15,126.00477,0.61911,434.34069,230.65984,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,124,725,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.110047,0,124,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,543.721169999999,"normal"]
["Maritime","h2","Low-emission ammonia",394.909437,0,124,850,15,126.00477,0.61911,434.34069,430.659999999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",682.528815,0,124,900,15,475.659121,2.00321,103.2691,278.00743,"comp"]
["Cement","ccs","CCS",184.480572,0,124,1050,15,62.166303,0.8654,141.33842,1000,"comp"]
["Maritime","h2","Low-emission ammonia",394.909437,0,124,1050,15,126.00477,0.61911,434.34069,1010.83905,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,124,1150,15,62.166303,0.8654,74.54509,1090.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7930.407897,0,124,1200,15,898.391809,4.8184,1459.40895,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,126,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["Aviation","comp","Compensation",0.056695,0,126,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},140.07595,624.417719999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",611.387815,0,126,250,15,475.659121,2.00321,67.7556,65.45333,"comp"]
["Maritime","comp","Compensation",305.546812,0,126,275,15,126.00477,0.61911,290.00023,152.2902,"ccu"]
["Primary steel","h2","DRI-EAF with H2",620.023315,0,126,325,15,475.659121,2.00321,72.06643,89.76568,"comp"]
["Maritime","h2","Low-emission ammonia",399.831197,0,126,475,15,126.00477,0.61911,442.29043,47.7099599999999,"normal"]
["Maritime","h2","Low-emission ammonia",399.831197,0,126,500,15,126.00477,0.61911,442.29043,72.7099799999999,"normal"]
["Aviation","comp","Compensation",0.096215,0,126,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,663.177219999999,"normal"]
["Maritime","h2","Low-emission ammonia",399.831197,0,126,675,15,126.00477,0.61911,442.29043,247.710119999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,126,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,126,825,15,475.659121,2.00321,51.86914,3.85792,"ccu"]
["CF","ccu","MTO using fossil CCU",3035.446497,1.90135,126,850,15,898.391809,4.8184,732.60818,132.39182,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,126,975,15,62.166303,0.8654,74.54509,915.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7250.353997,0,126,1025,15,898.391809,4.8184,1318.27208,1000,"comp"]
["Maritime","h2","Low-emission ammonia",399.831197,0,126,1125,15,126.00477,0.61911,442.29043,404.416089999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,126,1200,15,62.166303,0.8654,74.54509,1140.45491,"ccu"]
["Aviation","comp","Compensation",0.050767,0,128,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},65.03797,629.01266,"normal"]
["Maritime","comp","Compensation",197.202476,0,128,100,15,126.00477,0.61911,115.00009,335.24007,"ccu"]
["Primary steel","h2","DRI-EAF with H2",603.573815,0,128,150,15,475.659121,2.00321,63.85486,31.1898199999999,"comp"]
["CF","comp","Compensation",2175.267809,0,128,250,15,898.391809,4.8184,265,375.07059,"normal"]
["Maritime","h2","Low-emission ammonia",404.752957,0,128,300,15,126.00477,0.61911,450.24016,285.75021,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,128,375,15,475.659121,2.00321,51.86914,5.81759999999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",4923.620097,0,128,450,15,898.391809,4.8184,835.38691,1000,"comp"]
["Aviation","comp","Compensation",0.088311,0,128,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,665.82279,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.147298,0,128,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1286.94937,1000,"comp"]
["CF","comp","Compensation",4223.087809,0,128,675,15,898.391809,4.8184,690,56.4470199999999,"normal"]
["Aviation","comp","Compensation",0.104119,0,128,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,681.32911,"ccu"]
["Primary steel","h2","DRI-EAF with H2",678.414815,0,128,800,15,475.659121,2.00321,101.2154,241.89688,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,128,875,15,62.166303,0.8654,74.54509,815.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,128,975,15,475.659121,2.00321,51.86914,5.81759999999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,128,1025,15,475.659121,2.00321,51.86914,5.81759999999999,"normal"]
["Cement","ccs","CCS",185.939572,0,128,1075,15,62.166303,0.8654,143.02435,1000,"comp"]
["Aviation","comp","Compensation",0.139687,0,128,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,214.142409999999,"normal"]
["Cement","comp","Compensation",96.782303,0,130,25,15,62.166303,0.8654,40,34.54509,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,130,75,15,62.166303,0.8654,74.54509,15.4549099999999,"normal"]
["Aviation","comp","Compensation",0.058671,0,130,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},165.08861,647.1519,"ccu"]
["Maritime","h2","Low-emission ammonia",409.674717,0,130,200,15,126.00477,0.61911,458.1899,189.717129999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,130,300,15,62.166303,0.8654,74.54509,240.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4655.236197,0,130,375,15,898.391809,4.8184,779.68711,1000,"comp"]
["Maritime","comp","Compensation",398.413386,0,130,425,15,126.00477,0.61911,440.00035,18.1895499999999,"normal"]
["Cement","ccs","CCS",152.382572,0,130,500,15,62.166303,0.8654,104.24806,1000,"comp"]
["CF","comp","Compensation",3741.247809,0,130,575,15,898.391809,4.8184,590,170.28587,"normal"]
["Maritime","h2","Low-emission ammonia",409.674717,0,130,650,15,126.00477,0.61911,458.1899,206.81063,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,130,725,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4704.927809,0,130,775,15,898.391809,4.8184,790,311.15821,"ccu"]
["Maritime","h2","Low-emission ammonia",409.674717,0,130,850,15,126.00477,0.61911,458.1899,819.65302,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,130,925,15,475.659121,2.00321,51.86914,7.77727,"normal"]
["Primary steel","h2","DRI-EAF with H2",705.142815,0,130,1000,15,475.659121,2.00321,114.55798,304.8828,"comp"]
["Maritime","h2","Low-emission ammonia",409.674717,0,130,1075,15,126.00477,0.61911,458.1899,422.778549999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,130,1125,15,475.659121,2.00321,51.86914,7.77727,"ccu"]
["Maritime","h2","Low-emission ammonia",414.596477,0,132,25,15,126.00477,0.61911,466.13963,20.9991499999999,"comp"]
["Cement","ccs","CCS",126.120572,0,132,50,15,62.166303,0.8654,73.9014,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.112747,0,132,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},849.59494,1000,"comp"]
["CF","comp","Compensation",1934.347809,0,132,200,15,898.391809,4.8184,215,397.63746,"ccu"]
["Cement","ccs","CCS",142.169572,0,132,325,15,62.166303,0.8654,92.44658,1000,"comp"]
["CF","comp","Compensation",2898.027809,0,132,400,15,898.391809,4.8184,415,359.12471,"normal"]
["CF","comp","Compensation",3018.487809,0,132,425,15,898.391809,4.8184,440,366.87553,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,132,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,132,550,15,475.659121,2.00321,51.86914,9.73693999999999,"ccu"]
["Maritime","h2","Low-emission ammonia",414.596477,0,132,675,15,126.00477,0.61911,466.13963,650.93504,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,132,750,15,475.659121,2.00321,51.86914,9.73693999999999,"normal"]
["Aviation","comp","Compensation",0.110047,0,132,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,634.971169999999,"normal"]
["Maritime","h2","Low-emission ammonia",414.596477,0,132,900,15,126.00477,0.61911,466.13963,431.95978,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,132,950,15,475.659121,2.00321,51.86914,9.73693999999999,"ccu"]
["CF","ccu","MTO using fossil CCU",3156.552297,1.90135,132,1050,15,898.391809,4.8184,774.12471,290.875289999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,132,1050,15,475.659121,2.00321,51.86914,9.73693999999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,132,1200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",1091.127809,0,134,25,15,898.391809,4.8184,40,429.42884,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.105052,0,134,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},752.18987,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,134,175,15,475.659121,2.00321,51.86914,11.69661,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,134,200,15,62.166303,0.8654,74.54509,140.454909999999,"ccu"]
["Maritime","comp","Compensation",336.502337,0,134,325,15,126.00477,0.61911,340.00027,134.089099999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,134,375,15,475.659121,2.00321,51.86914,11.69661,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,134,450,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,134,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",663.608315,0,134,575,15,475.659121,2.00321,93.82401,163.41872,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,134,650,15,62.166303,0.8654,74.54509,590.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.160408,0,134,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1452.89873,1000,"comp"]
["Maritime","h2","Low-emission ammonia",419.518237,0,134,800,15,126.00477,0.61911,474.08937,340.91128,"normal"]
["CF","efuel","MTO using non-fossil CO2",6897.240897,0,134,900,15,898.391809,4.8184,1244.98777,1000,"comp"]
["Aviation","comp","Compensation",0.121903,0,134,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},965.49367,507.72855,"normal"]
["Maritime","h2","Low-emission ammonia",419.518237,0,134,1000,15,126.00477,0.61911,474.08937,540.91144,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,134,1100,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6511.827809,0,134,1150,15,898.391809,4.8184,1165,275.61922,"ccu"]
["Maritime","comp","Compensation",166.246952,0,136,50,15,126.00477,0.61911,65.00005,417.03905,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,136,75,15,62.166303,0.8654,74.54509,15.4549099999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3747.166997,0,136,125,15,898.391809,4.8184,591.22846,1000,"comp"]
["Maritime","comp","Compensation",274.591288,0,136,225,15,126.00477,0.61911,240.00019,242.03891,"normal"]
["Primary steel","h2","DRI-EAF with H2",635.644815,0,136,300,15,475.659121,2.00321,79.86466,72.42639,"comp"]
["CF","comp","Compensation",2657.107809,0,136,350,15,898.391809,4.8184,365,392.86039,"normal"]
["Maritime","comp","Compensation",398.413386,0,136,425,15,126.00477,0.61911,440.00035,42.0387499999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",655.794315,0,136,475,15,475.659121,2.00321,89.92327,129.15521,"comp"]
["CF","comp","Compensation",3741.247809,0,136,575,15,898.391809,4.8184,590,362.09847,"ccu"]
["Cement","ccs","CCS",162.595572,0,136,675,15,62.166303,0.8654,116.04954,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,136,700,15,475.659121,2.00321,51.86914,13.6562899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",6423.021997,0,136,775,15,898.391809,4.8184,1146.56944,1000,"comp"]
["Aviation","comp","Compensation",0.113999,0,136,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,630.584739999999,"normal"]
["Aviation","comp","Compensation",0.121903,0,136,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},965.49367,530.534109999999,"normal"]
["CF","ccu","MTO using fossil CCU",3237.289497,1.90135,136,1000,15,898.391809,4.8184,801.8024,213.197599999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,136,1125,15,62.166303,0.8654,74.54509,1065.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",730.635315,0,136,1125,15,475.659121,2.00321,127.28381,339.862269999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,136,1200,15,62.166303,0.8654,74.54509,1140.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",429.361757,0,138,75,15,126.00477,0.61911,489.98883,72.0961599999999,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,138,125,15,475.659121,2.00321,51.86914,15.61596,"normal"]
["Maritime","comp","Compensation",290.06905,0,138,250,15,126.00477,0.61911,265.00021,224.98862,"ccu"]
["Aviation","comp","Compensation",0.068551,0,138,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},290.1519,698.43038,"normal"]
["CF","comp","Compensation",2898.027809,0,138,400,15,898.391809,4.8184,415,393.88985,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,138,450,15,475.659121,2.00321,51.86914,15.61596,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,138,550,15,62.166303,0.8654,74.54509,490.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5742.968097,0,138,600,15,898.391809,4.8184,1005.43257,1000,"comp"]
["Aviation","comp","Compensation",0.100167,0,138,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,729.43038,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,138,725,15,62.166303,0.8654,74.54509,665.45491,"ccu"]
["CF","ccu","MTO using fossil CCU",3277.658097,1.90135,138,825,15,898.391809,4.8184,815.64124,24.3587599999999,"normal"]
["Maritime","h2","Low-emission ammonia",429.361757,0,138,900,15,126.00477,0.61911,489.98883,425.011899999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",714.185815,0,138,950,15,475.659121,2.00321,119.07224,281.28641,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,138,1025,15,62.166303,0.8654,74.54509,965.45491,"ccu"]
["CF","ccu","MTO using fossil CCU",3277.658097,1.90135,138,1100,15,898.391809,4.8184,815.64124,299.358759999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,138,1175,15,475.659121,2.00321,51.86914,15.61596,"normal"]
["Cement","ccs","CCS",123.202572,0,140,0,15,62.166303,0.8654,70.52955,1000,"comp"]
["Aviation","comp","Compensation",0.054719,0,140,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},115.06329,695.26582,"normal"]
["Maritime","comp","Compensation",212.680238,0,140,125,15,126.00477,0.61911,140.00011,357.93846,"ccu"]
["CF","comp","Compensation",2175.267809,0,140,250,15,898.391809,4.8184,265,422.263249999999,"normal"]
["Aviation","comp","Compensation",0.070527,0,140,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},315.16456,710.77215,"ccu"]
["Maritime","h2","Low-emission ammonia",434.283517,0,140,350,15,126.00477,0.61911,497.93857,339.487639999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,140,450,15,62.166303,0.8654,74.54509,390.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,140,500,15,475.659121,2.00321,51.86914,17.57563,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,140,600,15,475.659121,2.00321,51.86914,17.57563,"normal"]
["Cement","ccs","CCS",161.136572,0,140,650,15,62.166303,0.8654,114.36361,1000,"comp"]
["CF","comp","Compensation",4464.007809,0,140,725,15,898.391809,4.8184,740,89.48009,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,140,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,140,875,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5427.687809,0,140,925,15,898.391809,4.8184,940,329.97747,"ccu"]
["Maritime","h2","Low-emission ammonia",434.283517,0,140,1000,15,126.00477,0.61911,497.93857,969.42353,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,140,1075,15,475.659121,2.00321,51.86914,17.57563,"normal"]
["CF","efuel","MTO using non-fossil CO2",7944.604197,0,140,1125,15,898.391809,4.8184,1462.35522,1000,"comp"]
["Maritime","comp","Compensation",135.291427,0,142,0,15,126.00477,0.61911,15.00001,490.88829,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,142,50,15,475.659121,2.00321,51.86914,13.1308599999999,"ccu"]
["CF","comp","Compensation",1693.427809,0,142,150,15,898.391809,4.8184,165,443.80066,"normal"]
["Aviation","comp","Compensation",0.062623,0,142,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},215.11392,713.41773,"ccu"]
["Maritime","comp","Compensation",305.546812,0,142,275,15,126.00477,0.61911,290.00023,215.88807,"normal"]
["CF","comp","Compensation",2657.107809,0,142,350,15,898.391809,4.8184,365,416.45672,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.136015,0,142,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1144.12658,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,142,500,15,475.659121,2.00321,51.86914,19.5353099999999,"normal"]
["Maritime","h2","Low-emission ammonia",439.205277,0,142,600,15,126.00477,0.61911,505.8883,582.650809999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,142,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,142,700,15,475.659121,2.00321,51.86914,19.5353099999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,142,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.113999,0,142,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,763.79747,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,142,975,15,475.659121,2.00321,51.86914,19.5353099999999,"ccu"]
["Maritime","h2","Low-emission ammonia",439.205277,0,142,1050,15,126.00477,0.61911,505.8883,477.86592,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.191371,0,142,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1844.83544,1000,"comp"]
["CF","ccu","MTO using fossil CCU",3358.395297,1.90135,142,1200,15,898.391809,4.8184,843.31893,371.68107,"normal"]
["CF","comp","Compensation",1091.127809,0,144,25,15,898.391809,4.8184,40,468.75606,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,144,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["CF","comp","Compensation",1813.887809,0,144,175,15,898.391809,4.8184,190,448.24811,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,144,200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,144,325,15,475.659121,2.00321,51.86914,21.4949799999999,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.134708,0,144,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1127.58228,1000,"comp"]
["Maritime","comp","Compensation",429.368911,0,144,475,15,126.00477,0.61911,490.00039,23.8376499999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,144,525,15,475.659121,2.00321,51.86914,21.4949799999999,"ccu"]
["CF","comp","Compensation",3982.167809,0,144,625,15,898.391809,4.8184,640,217.15778,"normal"]
["Aviation","comp","Compensation",0.100167,0,144,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,760.632909999999,"ccu"]
["Maritime","h2","Low-emission ammonia",444.127037,0,144,750,15,126.00477,0.61911,513.83804,251.16257,"ccu"]
["CF","comp","Compensation",4945.847809,0,144,825,15,898.391809,4.8184,840,359.380329999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.177289,0,144,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1666.58228,1000,"comp"]
["Maritime","h2","Low-emission ammonia",444.127037,0,144,950,15,126.00477,0.61911,513.83804,451.16273,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,144,1025,15,475.659121,2.00321,51.86914,21.4949799999999,"normal"]
["Aviation","comp","Compensation",0.133759,0,144,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,471.708159999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,144,1175,15,475.659121,2.00321,51.86914,21.4949799999999,"ccu"]
["Cement","comp","Compensation",96.782303,0,146,25,15,62.166303,0.8654,40,34.54509,"normal"]
["CF","comp","Compensation",1332.047809,0,146,75,15,898.391809,4.8184,90,469.78552,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,146,175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,146,225,15,62.166303,0.8654,74.54509,165.454909999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4566.514997,0,146,275,15,898.391809,4.8184,761.27411,1000,"comp"]
["Maritime","comp","Compensation",367.457861,0,146,375,15,126.00477,0.61911,390.00031,131.78746,"normal"]
["Aviation","comp","Compensation",0.080407,0,146,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,751.645569999999,"ccu"]
["Aviation","comp","Compensation",0.088311,0,146,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,759.39241,"normal"]
["Maritime","h2","Low-emission ammonia",449.048797,0,146,575,15,126.00477,0.61911,521.78777,68.2126999999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",691.565315,0,146,625,15,475.659121,2.00321,107.78011,168.54474,"comp"]
["CF","comp","Compensation",4464.007809,0,146,725,15,898.391809,4.8184,740,380.91774,"ccu"]
["Maritime","h2","Low-emission ammonia",449.048797,0,146,800,15,126.00477,0.61911,521.78777,293.212879999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,146,875,15,62.166303,0.8654,74.54509,815.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7242.369997,0,146,925,15,898.391809,4.8184,1316.6151,1000,"comp"]
["Aviation","comp","Compensation",0.125855,0,146,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,594.59212,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,146,1075,15,475.659121,2.00321,51.86914,23.45465,"ccu"]
["Primary steel","h2","DRI-EAF with H2",752.013815,0,146,1150,15,475.659121,2.00321,137.95593,338.73122,"comp"]
["Aviation","comp","Compensation",0.141663,0,146,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,811.72152,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",589.602577,0,148,50,15,475.659121,2.00321,56.88043,19.69701,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,148,125,15,62.166303,0.8654,74.54509,65.45491,"ccu"]
["Cement","ccs","CCS",134.874572,0,148,200,15,62.166303,0.8654,84.01695,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,148,275,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",142.169572,0,148,325,15,62.166303,0.8654,92.44658,1000,"comp"]
["Aviation","comp","Compensation",0.080407,0,148,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,762.03797,"normal"]
["Maritime","comp","Compensation",429.368911,0,148,475,15,126.00477,0.61911,490.00039,39.73712,"ccu"]
["Aviation","comp","Compensation",0.092263,0,148,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,773.67088,"normal"]
["Aviation","comp","Compensation",0.096215,0,148,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,777.544309999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6562.316097,0,148,750,15,898.391809,4.8184,1175.47823,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,148,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",453.970557,0,148,825,15,126.00477,0.61911,529.73751,803.34594,"comp"]
["CF","ccu","MTO using fossil CCU",3479.501097,1.90135,148,975,15,898.391809,4.8184,884.83546,105.164539999999,"normal"]
["Cement","ccs","CCS",180.103572,0,148,975,15,62.166303,0.8654,136.28064,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",749.956815,0,148,1100,15,475.659121,2.00321,136.92908,320.67594,"comp"]
["Maritime","h2","Low-emission ammonia",453.970557,0,148,1125,15,126.00477,0.61911,529.73751,610.26339,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,148,1200,15,475.659121,2.00321,51.86914,25.4143299999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,150,100,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",4235.582197,0,150,175,15,898.391809,4.8184,692.59306,1000,"comp"]
["Aviation","comp","Compensation",0.066575,0,150,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},265.13924,758.87342,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,150,325,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2898.027809,0,150,400,15,898.391809,4.8184,415,441.082509999999,"normal"]
["Aviation","comp","Compensation",0.082383,0,150,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,774.37974,"ccu"]
["Primary steel","h2","DRI-EAF with H2",687.451315,0,150,525,15,475.659121,2.00321,105.72641,132.434199999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,150,600,15,62.166303,0.8654,74.54509,540.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6293.932197,0,150,675,15,898.391809,4.8184,1119.77843,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,150,750,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",169.890572,0,150,800,15,62.166303,0.8654,124.47916,1000,"comp"]
["Aviation","comp","Compensation",0.117951,0,150,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,740.28165,"normal"]
["Maritime","h2","Low-emission ammonia",458.892317,0,150,950,15,126.00477,0.61911,537.68724,427.31353,"ccu"]
["Maritime","h2","Low-emission ammonia",458.892317,0,150,975,15,126.00477,0.61911,537.68724,452.31355,"ccu"]
["Aviation","comp","Compensation",0.133759,0,150,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,824.759489999999,"ccu"]
["Maritime","h2","Low-emission ammonia",458.892317,0,150,1150,15,126.00477,0.61911,537.68724,1119.19403,"comp"]
["Primary steel","comp","Compensation",505.707271,0,152,0,15,475.659121,2.00321,15,36.86914,"normal"]
["Maritime","comp","Compensation",197.202476,0,152,100,15,126.00477,0.61911,115.00009,430.63688,"normal"]
["Maritime","comp","Compensation",228.158001,0,152,150,15,126.00477,0.61911,165.00013,380.63684,"normal"]
["Cement","ccs","CCS",136.333572,0,152,225,15,62.166303,0.8654,85.70288,1000,"comp"]
["CF","comp","Compensation",2416.187809,0,152,300,15,898.391809,4.8184,315,462.61992,"normal"]
["Aviation","comp","Compensation",0.074479,0,152,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},365.18987,777.02532,"ccu"]
["Primary steel","h2","DRI-EAF with H2",682.515815,0,152,450,15,475.659121,2.00321,103.26261,106.27481,"comp"]
["CF","comp","Compensation",3379.867809,0,152,500,15,898.391809,4.8184,515,435.27599,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.152897,0,152,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1357.82278,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,152,650,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","comp","Compensation",4464.007809,0,152,725,15,898.391809,4.8184,740,404.514069999999,"ccu"]
["Maritime","h2","Low-emission ammonia",463.814077,0,152,800,15,126.00477,0.61911,545.63697,269.363679999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,152,850,15,475.659121,2.00321,51.86914,29.3336699999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,152,925,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.125855,0,152,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,827.40506,"ccu"]
["Aviation","comp","Compensation",0.133759,0,152,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,562.98594,"normal"]
["CF","comp","Compensation",6511.827809,0,152,1150,15,898.391809,4.8184,1165,346.40821,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.208253,0,152,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2058.53165,1000,"comp"]
["Maritime","comp","Compensation",166.246952,0,154,50,15,126.00477,0.61911,65.00005,488.58666,"normal"]
["Cement","ccs","CCS",130.497572,0,154,125,15,62.166303,0.8654,78.95917,1000,"comp"]
["Maritime","h2","Low-emission ammonia",468.735837,0,154,225,15,126.00477,0.61911,553.58671,224.50707,"comp"]
["CF","comp","Compensation",2536.647809,0,154,325,15,898.391809,4.8184,340,467.06737,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,154,350,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,154,475,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,154,500,15,475.659121,2.00321,51.86914,31.29335,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,154,550,15,62.166303,0.8654,74.54509,490.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,154,675,15,475.659121,2.00321,51.86914,31.29335,"ccu"]
["Maritime","h2","Low-emission ammonia",468.735837,0,154,700,15,126.00477,0.61911,553.58671,161.41386,"normal"]
["Aviation","comp","Compensation",0.112023,0,154,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,824.24051,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,154,875,15,62.166303,0.8654,74.54509,815.45491,"ccu"]
["CF","comp","Compensation",5668.607809,0,154,975,15,898.391809,4.8184,990,378.199589999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.194171,0,154,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1880.27848,1000,"comp"]
["CF","comp","Compensation",6029.987809,0,154,1050,15,898.391809,4.8184,1065,367.945619999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.202687,0,154,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1988.07595,1000,"comp"]
["Aviation","comp","Compensation",0.048791,0,156,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,772.63291,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,156,100,15,475.659121,2.00321,51.86914,33.2530199999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,156,175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.066575,0,156,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},265.13924,790.06329,"ccu"]
["Maritime","comp","Compensation",305.546812,0,156,275,15,126.00477,0.61911,290.00023,271.53621,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,156,375,15,62.166303,0.8654,74.54509,315.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.146023,0,156,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1270.81013,1000,"comp"]
["Maritime","comp","Compensation",460.324435,0,156,525,15,126.00477,0.61911,540.00043,21.5360099999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",707.186815,0,156,600,15,475.659121,2.00321,115.57834,151.20545,"comp"]
["Aviation","comp","Compensation",0.100167,0,156,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,823.01266,"normal"]
["Maritime","h2","Low-emission ammonia",473.657597,0,156,725,15,126.00477,0.61911,561.53644,178.46415,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,156,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5186.767809,0,156,875,15,898.391809,4.8184,890,399.737,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7341.295497,0,156,900,15,898.391809,4.8184,1337.14588,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,156,1025,15,62.166303,0.8654,74.54509,965.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",8061.717997,0,156,1075,15,898.391809,4.8184,1486.66076,1000,"comp"]
["Maritime","h2","Low-emission ammonia",473.657597,0,156,1175,15,126.00477,0.61911,561.53644,542.13451,"normal"]
["Primary steel","comp","Compensation",505.707271,0,158,0,15,475.659121,2.00321,15,36.86914,"ccu"]
["Aviation","comp","Compensation",0.050767,0,158,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},65.03797,784.96203,"ccu"]
["Maritime","comp","Compensation",228.158001,0,158,150,15,126.00477,0.61911,165.00013,404.48605,"ccu"]
["Primary steel","h2","DRI-EAF with H2",664.830815,0,158,200,15,475.659121,2.00321,94.43428,19.69252,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,158,275,15,62.166303,0.8654,74.54509,215.454909999999,"ccu"]
["Aviation","comp","Compensation",0.078431,0,158,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,812.088609999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,158,425,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",5734.984097,0,158,500,15,898.391809,4.8184,1003.77559,1000,"comp"]
["Aviation","comp","Compensation",0.092263,0,158,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,825.658229999999,"normal"]
["Maritime","h2","Low-emission ammonia",478.579357,0,158,625,15,126.00477,0.61911,569.48618,70.5143299999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",719.522315,0,158,675,15,475.659121,2.00321,121.73621,173.67076,"comp"]
["Aviation","comp","Compensation",0.108071,0,158,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,841.151899999999,"ccu"]
["Maritime","h2","Low-emission ammonia",478.579357,0,158,825,15,126.00477,0.61911,569.48618,807.74663,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,158,925,15,62.166303,0.8654,74.54509,865.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,158,1025,15,62.166303,0.8654,74.54509,965.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,158,1075,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",188.857572,0,158,1125,15,62.166303,0.8654,146.3962,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",570.489827,0,160,25,15,475.659121,2.00321,47.33937,38.88334,"comp"]
["Maritime","comp","Compensation",166.246952,0,160,50,15,126.00477,0.61911,65.00005,512.43586,"ccu"]
["CF","comp","Compensation",1813.887809,0,160,175,15,898.391809,4.8184,190,511.17165,"normal"]
["Aviation","comp","Compensation",0.062623,0,160,200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},215.11392,806.98735,"ccu"]
["Maritime","h2","Low-emission ammonia",483.501117,0,160,250,15,126.00477,0.61911,577.43591,251.375789999999,"comp"]
["Aviation","comp","Compensation",0.078431,0,160,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,822.49367,"normal"]
["CF","efuel","MTO using non-fossil CO2",5363.682697,0,160,400,15,898.391809,4.8184,926.71652,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.154053,0,160,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1372.4557,1000,"comp"]
["Aviation","comp","Compensation",0.094239,0,160,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,837.987339999999,"ccu"]
["CF","comp","Compensation",3982.167809,0,160,625,15,898.391809,4.8184,640,327.868529999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,160,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",483.501117,0,160,800,15,126.00477,0.61911,577.43591,237.564739999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,160,900,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",178.644572,0,160,950,15,62.166303,0.8654,134.59472,1000,"comp"]
["Aviation","comp","Compensation",0.129807,0,160,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,704.26126,"normal"]
["Maritime","h2","Low-emission ammonia",483.501117,0,160,1100,15,126.00477,0.61911,577.43591,537.56498,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,160,1175,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Aviation","comp","Compensation",0.048791,0,162,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,803.82278,"ccu"]
["Maritime","h2","Low-emission ammonia",488.422877,0,162,75,15,126.00477,0.61911,585.38565,82.6577899999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,162,175,15,62.166303,0.8654,74.54509,115.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4580.711297,0,162,200,15,898.391809,4.8184,764.22038,1000,"comp"]
["Maritime","comp","Compensation",321.024575,0,162,300,15,126.00477,0.61911,315.00025,270.3854,"normal"]
["Cement","ccs","CCS",145.087572,0,162,375,15,62.166303,0.8654,95.81843,1000,"comp"]
["CF","comp","Compensation",3138.947809,0,162,450,15,898.391809,4.8184,465,481.43919,"normal"]
["Maritime","comp","Compensation",460.324435,0,162,525,15,126.00477,0.61911,540.00043,45.38522,"ccu"]
["Aviation","comp","Compensation",0.092263,0,162,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,846.455689999999,"ccu"]
["CF","comp","Compensation",4102.627809,0,162,650,15,898.391809,4.8184,665,454.09526,"ccu"]
["Maritime","h2","Low-emission ammonia",488.422877,0,162,725,15,126.00477,0.61911,585.38565,712.593679999999,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,162,800,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",172.808572,0,162,850,15,62.166303,0.8654,127.85102,1000,"comp"]
["Maritime","h2","Low-emission ammonia",488.422877,0,162,950,15,126.00477,0.61911,585.38565,379.615119999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,162,1000,15,475.659121,2.00321,51.86914,39.13204,"ccu"]
["CF","ccu","MTO using fossil CCU",3762.081297,1.90135,162,1100,15,898.391809,4.8184,981.70737,133.29263,"normal"]
["Aviation","comp","Compensation",0.137711,0,162,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1165.59494,891.01265,"ccu"]
["Cement","ccs","CCS",193.23457200000001,0,162,1200,15,62.166303,0.8654,151.45397,1000,"comp"]
["CF","comp","Compensation",1332.047809,0,164,75,15,898.391809,4.8184,90,540.5745,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.121631,0,164,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},962.05063,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,164,225,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",139.251572,0,164,275,15,62.166303,0.8654,89.07473,1000,"comp"]
["CF","comp","Compensation",2657.107809,0,164,350,15,898.391809,4.8184,365,502.976599999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,164,425,15,475.659121,2.00321,51.86914,41.0917099999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,164,500,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3620.787809,0,164,550,15,898.391809,4.8184,565,475.63266,"ccu"]
["Aviation","comp","Compensation",0.096215,0,164,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,860.721519999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,164,700,15,62.166303,0.8654,74.54509,640.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.176987,0,164,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1662.75949,1000,"comp"]
["Maritime","h2","Low-emission ammonia",493.344637,0,164,850,15,126.00477,0.61911,593.33538,271.66531,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,164,900,15,475.659121,2.00321,51.86914,41.0917099999999,"ccu"]
["Maritime","h2","Low-emission ammonia",493.344637,0,164,975,15,126.00477,0.61911,593.33538,955.75686,"comp"]
["Maritime","h2","Low-emission ammonia",493.344637,0,164,1050,15,126.00477,0.61911,593.33538,471.665469999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,164,1150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6752.747809,0,164,1200,15,898.391809,4.8184,1215,386.764879999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,166,100,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,166,125,15,62.166303,0.8654,74.54509,65.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4558.530997,0,166,175,15,898.391809,4.8184,759.61713,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,166,325,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,166,325,15,475.659121,2.00321,51.86914,43.0513799999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,166,475,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","comp","Compensation",429.368911,0,166,475,15,126.00477,0.61911,490.00039,111.28472,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.162904,0,166,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1484.49367,1000,"comp"]
["Maritime","h2","Low-emission ammonia",498.266397,0,166,675,15,126.00477,0.61911,601.28511,88.7154399999999,"normal"]
["Cement","ccs","CCS",166.972572,0,166,750,15,62.166303,0.8654,121.10731,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.175679,0,166,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1646.20253,1000,"comp"]
["Maritime","h2","Low-emission ammonia",498.266397,0,166,875,15,126.00477,0.61911,601.28511,288.7156,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,166,975,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5909.527809,0,166,1025,15,898.391809,4.8184,1040,418.55627,"ccu"]
["Aviation","comp","Compensation",0.133759,0,166,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,907.93671,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,166,1175,15,62.166303,0.8654,74.54509,1115.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",3878.477097,0,168,0,15,898.391809,4.8184,618.48026,1000,"comp"]
["Maritime","comp","Compensation",197.202476,0,168,100,15,126.00477,0.61911,115.00009,494.23476,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,168,150,15,475.659121,2.00321,51.86914,45.01106,"ccu"]
["Maritime","comp","Compensation",290.06905,0,168,250,15,126.00477,0.61911,265.00021,344.23464,"normal"]
["Maritime","comp","Compensation",321.024575,0,168,300,15,126.00477,0.61911,315.00025,294.2346,"ccu"]
["Primary steel","h2","DRI-EAF with H2",700.601815,0,168,350,15,475.659121,2.00321,112.29112,59.0820499999999,"comp"]
["CF","comp","Compensation",3138.947809,0,168,450,15,898.391809,4.8184,465,505.03552,"ccu"]
["Cement","ccs","CCS",152.382572,0,168,500,15,62.166303,0.8654,104.24806,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,168,575,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",6554.332097,0,168,650,15,898.391809,4.8184,1173.82125,1000,"comp"]
["Aviation","comp","Compensation",0.104119,0,168,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,889.26582,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,168,800,15,475.659121,2.00321,51.86914,45.01106,"ccu"]
["CF","comp","Compensation",5186.767809,0,168,875,15,898.391809,4.8184,890,446.92966,"ccu"]
["Aviation","comp","Compensation",0.119927,0,168,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},940.48101,904.77215,"ccu"]
["Primary steel","h2","DRI-EAF with H2",775.442815,0,168,1000,15,475.659121,2.00321,149.65166,269.78912,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,168,1075,15,62.166303,0.8654,74.54509,1015.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",8509.764597,0,168,1125,15,898.391809,4.8184,1579.64735,1000,"comp"]
["Aviation","comp","Compensation",0.048791,0,170,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,845.40506,"normal"]
["Cement","ccs","CCS",126.120572,0,170,50,15,62.166303,0.8654,73.9014,1000,"comp"]
["Aviation","comp","Compensation",0.058671,0,170,150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},165.08861,855.10126,"normal"]
["Maritime","comp","Compensation",259.113525,0,170,200,15,126.00477,0.61911,215.00017,402.184409999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,170,275,15,475.659121,2.00321,51.86914,46.97073,"ccu"]
["Aviation","comp","Compensation",0.074479,0,170,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},365.18987,870.59494,"ccu"]
["Maritime","h2","Low-emission ammonia",508.109917,0,170,400,15,126.00477,0.61911,617.18458,401.14629,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,170,500,15,62.166303,0.8654,74.54509,440.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6183.030697,0,170,550,15,898.391809,4.8184,1096.76218,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,170,650,15,62.166303,0.8654,74.54509,590.45491,"ccu"]
["Cement","ccs","CCS",164.054572,0,170,700,15,62.166303,0.8654,117.73546,1000,"comp"]
["CF","comp","Compensation",4704.927809,0,170,775,15,898.391809,4.8184,790,247.06275,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,170,900,15,62.166303,0.8654,74.54509,840.45491,"ccu"]
["CF","comp","Compensation",5427.687809,0,170,925,15,898.391809,4.8184,940,97.06275,"normal"]
["CF","comp","Compensation",5668.607809,0,170,975,15,898.391809,4.8184,990,441.123139999999,"ccu"]
["Maritime","h2","Low-emission ammonia",508.109917,0,170,1050,15,126.00477,0.61911,617.18458,1031.08217999999,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,170,1125,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Maritime","comp","Compensation",150.769189,0,172,25,15,126.00477,0.61911,40.00003,585.13429,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.118529,0,172,50,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},922.78481,1000,"comp"]
["Aviation","comp","Compensation",0.060647,0,172,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,867.430379999999,"ccu"]
["CF","comp","Compensation",1934.347809,0,172,200,15,898.391809,4.8184,215,554.94632,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,172,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5502.976797,0,172,375,15,898.391809,4.8184,955.62531,1000,"comp"]
["Maritime","comp","Compensation",398.413386,0,172,425,15,126.00477,0.61911,440.00035,185.133969999999,"ccu"]
["Cement","ccs","CCS",153.841572,0,172,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["CF","comp","Compensation",3861.707809,0,172,600,15,898.391809,4.8184,615,435.901589999999,"normal"]
["Maritime","h2","Low-emission ammonia",513.031677,0,172,675,15,126.00477,0.61911,625.13432,64.8662299999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,172,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.112023,0,172,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,917.81013,"ccu"]
["Maritime","h2","Low-emission ammonia",513.031677,0,172,875,15,126.00477,0.61911,625.13432,862.364189999999,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,172,950,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",8178.831797,0,172,1025,15,898.391809,4.8184,1510.96629,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8281.749297,0,172,1050,15,898.391809,4.8184,1532.32556,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,172,1150,15,475.659121,2.00321,51.86914,48.9303999999999,"ccu"]
["CF","comp","Compensation",1091.127809,0,174,25,15,898.391809,4.8184,40,586.7377,"normal"]
["Aviation","comp","Compensation",0.052743,0,174,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},90.05063,870.07595,"ccu"]
["CF","comp","Compensation",1813.887809,0,174,175,15,898.391809,4.8184,190,566.22975,"ccu"]
["CF","comp","Compensation",2054.807809,0,174,225,15,898.391809,4.8184,240,559.39377,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.138512,0,174,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1175.73418,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,174,375,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",148.005572,0,174,425,15,62.166303,0.8654,99.19028,1000,"comp"]
["Maritime","comp","Compensation",429.368911,0,174,475,15,126.00477,0.61911,490.00039,143.08366,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,174,575,15,475.659121,2.00321,51.86914,50.89008,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,174,650,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.104119,0,174,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,920.45569,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,174,800,15,475.659121,2.00321,51.86914,50.89008,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,174,850,15,62.166303,0.8654,74.54509,790.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.193868,0,174,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1876.44304,1000,"comp"]
["Maritime","h2","Low-emission ammonia",517.953437,0,174,1000,15,126.00477,0.61911,633.08405,381.916759999999,"normal"]
["Cement","ccs","CCS",185.939572,0,174,1075,15,62.166303,0.8654,143.02435,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,174,1175,15,62.166303,0.8654,74.54509,1115.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",517.953437,0,174,1200,15,126.00477,0.61911,633.08405,581.91691,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,176,75,15,62.166303,0.8654,74.54509,15.4549099999999,"normal"]
["CF","comp","Compensation",1572.967809,0,176,125,15,898.391809,4.8184,140,580.93118,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.130817,0,176,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1078.32911,1000,"comp"]
["CF","comp","Compensation",2536.647809,0,176,325,15,898.391809,4.8184,340,553.58725,"normal"]
["CF","efuel","MTO using non-fossil CO2",5377.878997,0,176,325,15,898.391809,4.8184,929.66279,1000,"comp"]
["Maritime","comp","Compensation",398.413386,0,176,425,15,126.00477,0.61911,440.00035,201.033439999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,176,475,15,475.659121,2.00321,51.86914,52.84975,"ccu"]
["Maritime","comp","Compensation",491.27996,0,176,575,15,126.00477,0.61911,590.00047,51.03332,"ccu"]
["Maritime","comp","Compensation",522.235484,0,176,625,15,126.00477,0.61911,640.00051,1.03327999999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",752.822315,0,176,675,15,475.659121,2.00321,138.35953,157.04744,"comp"]
["CF","comp","Compensation",4704.927809,0,176,775,15,898.391809,4.8184,790,492.0634,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.186173,0,176,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1779.03797,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,176,950,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",8053.733997,0,176,975,15,898.391809,4.8184,1485.00377,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,176,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6632.287809,0,176,1175,15,898.391809,4.8184,1190,437.37553,"ccu"]
["Cement","comp","Compensation",75.147303,0,178,0,15,62.166303,0.8654,15,59.54509,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,178,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",627.828077,0,178,100,15,475.659121,2.00321,75.96256,31.1943,"comp"]
["Maritime","comp","Compensation",290.06905,0,178,250,15,126.00477,0.61911,265.00021,383.98331,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,178,300,15,475.659121,2.00321,51.86914,54.80942,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5521.165097,0,178,350,15,898.391809,4.8184,959.40007,1000,"comp"]
["Maritime","comp","Compensation",413.891148,0,178,450,15,126.00477,0.61911,465.00037,183.98315,"ccu"]
["Aviation","comp","Compensation",0.084359,0,178,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},490.25316,921.87342,"normal"]
["CF","comp","Compensation",3861.707809,0,178,600,15,898.391809,4.8184,615,523.854779999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.172091,0,178,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1600.78481,1000,"comp"]
["Aviation","comp","Compensation",0.104119,0,178,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,941.25316,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7373.680097,0,178,800,15,898.391809,4.8184,1343.8669,1000,"comp"]
["Aviation","comp","Compensation",0.115975,0,178,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,952.88607,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,178,950,15,475.659121,2.00321,51.86914,54.80942,"ccu"]
["Primary steel","h2","DRI-EAF with H2",791.064315,0,178,975,15,475.659121,2.00321,157.44989,252.44982,"comp"]
["Maritime","h2","Low-emission ammonia",527.796957,0,178,1100,15,126.00477,0.61911,648.98352,466.01737,"ccu"]
["Primary steel","h2","DRI-EAF with H2",811.213815,0,178,1150,15,475.659121,2.00321,167.5085,309.178649999999,"comp"]
["Cement","comp","Compensation",75.147303,0,180,0,15,62.166303,0.8654,15,59.54509,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.123943,0,180,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},991.31646,1000,"comp"]
["Cement","ccs","CCS",130.497572,0,180,125,15,62.166303,0.8654,78.95917,1000,"comp"]
["Cement","ccs","CCS",134.874572,0,180,200,15,62.166303,0.8654,84.01695,1000,"comp"]
["Aviation","comp","Compensation",0.070527,0,180,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},315.16456,918.70886,"normal"]
["Maritime","comp","Compensation",351.980099,0,180,350,15,126.00477,0.61911,365.00029,291.93296,"ccu"]
["CF","comp","Compensation",2898.027809,0,180,400,15,898.391809,4.8184,415,559.06416,"ccu"]
["Aviation","comp","Compensation",0.086335,0,180,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,934.21519,"ccu"]
["Maritime","h2","Low-emission ammonia",532.718717,0,180,550,15,126.00477,0.61911,656.93325,550.9168,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,180,650,15,62.166303,0.8654,74.54509,590.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7002.378697,0,180,700,15,898.391809,4.8184,1266.80784,1000,"comp"]
["Aviation","comp","Compensation",0.108071,0,180,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,955.531649999999,"normal"]
["Cement","ccs","CCS",172.808572,0,180,850,15,62.166303,0.8654,127.85102,1000,"comp"]
["CF","comp","Compensation",5427.687809,0,180,925,15,898.391809,4.8184,940,166.256969999999,"normal"]
["Maritime","h2","Low-emission ammonia",532.718717,0,180,1000,15,126.00477,0.61911,656.93325,358.067559999999,"ccu"]
["Maritime","h2","Low-emission ammonia",532.718717,0,180,1100,15,126.00477,0.61911,656.93325,458.06764,"ccu"]
["CF","comp","Compensation",6391.367809,0,180,1125,15,898.391809,4.8184,1140,459.942399999999,"ccu"]
["Maritime","h2","Low-emission ammonia",532.718717,0,180,1200,15,126.00477,0.61911,656.93325,1180.85269,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,182,50,15,475.659121,2.00321,51.86914,13.1308599999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",4675.644797,0,182,125,15,898.391809,4.8184,783.92267,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,182,250,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,182,250,15,475.659121,2.00321,51.86914,58.72877,"ccu"]
["CF","comp","Compensation",2657.107809,0,182,350,15,898.391809,4.8184,365,573.76558,"normal"]
["Aviation","comp","Compensation",0.078431,0,182,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,936.860759999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",740.894315,0,182,475,15,475.659121,2.00321,132.40509,86.67339,"comp"]
["CF","comp","Compensation",3620.787809,0,182,550,15,898.391809,4.8184,565,546.42165,"normal"]
["Cement","ccs","CCS",162.595572,0,182,675,15,62.166303,0.8654,116.04954,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,182,700,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",166.972572,0,182,750,15,62.166303,0.8654,121.10731,1000,"comp"]
["Aviation","comp","Compensation",0.115975,0,182,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,973.67088,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,182,900,15,475.659121,2.00321,51.86914,58.72877,"ccu"]
["Maritime","h2","Low-emission ammonia",537.640477,0,182,1025,15,126.00477,0.61911,664.88299,1012.13469,"comp"]
["Aviation","comp","Compensation",0.129807,0,182,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,987.24051,"ccu"]
["CF","efuel","MTO using non-fossil CO2",8998.179797,0,182,1175,15,898.391809,4.8184,1681.01195,1000,"comp"]
["Maritime","comp","Compensation",150.769189,0,184,25,15,126.00477,0.61911,40.00003,632.83269,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.121328,0,184,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},958.21519,1000,"comp"]
["CF","comp","Compensation",1813.887809,0,184,175,15,898.391809,4.8184,190,605.55697,"normal"]
["Aviation","comp","Compensation",0.064599,0,184,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},240.12658,933.6962,"ccu"]
["Primary steel","h2","DRI-EAF with H2",721.566315,0,184,275,15,475.659121,2.00321,122.75657,19.99342,"comp"]
["CF","comp","Compensation",2777.567809,0,184,375,15,898.391809,4.8184,390,578.21304,"ccu"]
["Maritime","h2","Low-emission ammonia",542.562237,0,184,450,15,126.00477,0.61911,672.83272,455.763849999999,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,184,525,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",156.759572,0,184,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["Cement","ccs","CCS",161.136572,0,184,650,15,62.166303,0.8654,114.36361,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,184,725,15,475.659121,2.00321,51.86914,60.68844,"ccu"]
["CF","comp","Compensation",4945.847809,0,184,825,15,898.391809,4.8184,840,293.934659999999,"normal"]
["Aviation","comp","Compensation",0.115975,0,184,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,984.075949999999,"ccu"]
["Maritime","h2","Low-emission ammonia",542.562237,0,184,925,15,126.00477,0.61911,672.83272,916.10162,"comp"]
["CF","comp","Compensation",5909.527809,0,184,1025,15,898.391809,4.8184,1040,489.34526,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.210749,0,184,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2090.12658,1000,"comp"]
["Maritime","h2","Low-emission ammonia",542.562237,0,184,1150,15,126.00477,0.61911,672.83272,492.168209999999,"normal"]
["Cement","ccs","CCS",123.202572,0,186,0,15,62.166303,0.8654,70.52955,1000,"comp"]
["Maritime","h2","Low-emission ammonia",547.483997,0,186,50,15,126.00477,0.61911,680.78246,68.99113,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,186,150,15,475.659121,2.00321,51.86914,62.6481199999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,186,225,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2295.727809,0,186,275,15,898.391809,4.8184,290,599.75045,"ccu"]
["Maritime","h2","Low-emission ammonia",547.483997,0,186,350,15,126.00477,0.61911,680.78246,359.73077,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,186,425,15,475.659121,2.00321,51.86914,62.6481199999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6197.226997,0,186,475,15,898.391809,4.8184,1099.70845,1000,"comp"]
["Maritime","comp","Compensation",491.27996,0,186,575,15,126.00477,0.61911,590.00047,90.78199,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,186,625,15,475.659121,2.00321,51.86914,62.6481199999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,186,700,15,62.166303,0.8654,74.54509,640.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",547.483997,0,186,775,15,126.00477,0.61911,680.78246,109.218169999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",788.593315,0,186,825,15,475.659121,2.00321,156.21637,196.43697,"comp"]
["CF","comp","Compensation",5427.687809,0,186,925,15,898.391809,4.8184,940,510.88266,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.203054,0,186,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1992.72152,1000,"comp"]
["CF","comp","Compensation",6150.447809,0,186,1075,15,898.391809,4.8184,1090,57.7735,"normal"]
["CF","efuel","MTO using non-fossil CO2",8873.081997,0,186,1125,15,898.391809,4.8184,1655.04943,1000,"comp"]
["Aviation","comp","Compensation",0.141663,0,186,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,850.79642,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,188,50,15,475.659121,2.00321,51.86914,13.1308599999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,188,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["Maritime","comp","Compensation",259.113525,0,188,200,15,126.00477,0.61911,215.00017,473.732019999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",726.087815,0,188,250,15,475.659121,2.00321,125.0137,8.19523000000001,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,188,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.154907,0,188,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1383.26582,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,188,475,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Maritime","comp","Compensation",506.757722,0,188,600,15,126.00477,0.61911,615.00049,73.7316999999999,"ccu"]
["Aviation","comp","Compensation",0.096215,0,188,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,985.49367,"normal"]
["CF","comp","Compensation",4584.467809,0,188,750,15,898.391809,4.8184,765,542.67405,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,188,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,188,850,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","efuel","MTO using non-fossil CO2",8193.028097,0,188,950,15,898.391809,4.8184,1513.91256,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,188,975,15,62.166303,0.8654,74.54509,915.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,188,1100,15,475.659121,2.00321,51.86914,64.60779,"ccu"]
["CF","comp","Compensation",6632.287809,0,188,1175,15,898.391809,4.8184,1190,484.568189999999,"ccu"]
["Maritime","comp","Compensation",150.769189,0,190,25,15,126.00477,0.61911,40.00003,656.681899999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",608.715327,0,190,75,15,475.659121,2.00321,66.4215,50.38063,"comp"]
["CF","comp","Compensation",1813.887809,0,190,175,15,898.391809,4.8184,190,629.1533,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.140825,0,190,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1205.01266,1000,"comp"]
["Aviation","comp","Compensation",0.072503,0,190,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},340.17722,972.63291,"normal"]
["CF","efuel","MTO using non-fossil CO2",5866.294197,0,190,375,15,898.391809,4.8184,1031.02739,1000,"comp"]
["Aviation","comp","Compensation",0.082383,0,190,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,982.32911,"normal"]
["Maritime","comp","Compensation",444.846673,0,190,500,15,126.00477,0.61911,515.00041,181.681519999999,"ccu"]
["Maritime","h2","Low-emission ammonia",557.327517,0,190,575,15,126.00477,0.61911,696.68193,579.54577,"comp"]
["Aviation","comp","Compensation",0.098191,0,190,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,997.822789999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",784.479315,0,190,725,15,475.659121,2.00321,154.16267,160.32643,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,190,800,15,62.166303,0.8654,74.54509,740.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7821.726697,0,190,850,15,898.391809,4.8184,1436.8535,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,190,950,15,475.659121,2.00321,51.86914,66.56746,"ccu"]
["Cement","ccs","CCS",181.562572,0,190,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["Aviation","comp","Compensation",0.133759,0,190,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,996.485939999999,"normal"]
["Maritime","h2","Low-emission ammonia",557.327517,0,190,1150,15,126.00477,0.61911,696.68193,468.318999999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",839.170815,0,190,1200,15,475.659121,2.00321,181.4646,314.30467,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,192,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",562.249277,0,192,125,15,126.00477,0.61911,704.63166,144.31645,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,192,200,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",5494.992797,0,192,275,15,898.391809,4.8184,953.96833,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.152292,0,192,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1350.16456,1000,"comp"]
["Cement","ccs","CCS",148.005572,0,192,425,15,62.166303,0.8654,99.19028,1000,"comp"]
["CF","comp","Compensation",3379.867809,0,192,500,15,898.391809,4.8184,515,592.58485,"normal"]
["Aviation","comp","Compensation",0.090287,0,192,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,1000.46834999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",776.665315,0,192,625,15,475.659121,2.00321,150.26193,126.06292,"comp"]
["Maritime","h2","Low-emission ammonia",562.249277,0,192,725,15,126.00477,0.61911,704.63166,35.3689299999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.186357,0,192,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1781.36709,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,192,850,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",175.726572,0,192,900,15,62.166303,0.8654,131.22287,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,192,1000,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,192,1050,15,475.659121,2.00321,51.86914,68.52713,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,192,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.141663,0,192,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,1050.8481,"ccu"]
["Maritime","h2","Low-emission ammonia",567.171037,0,194,25,15,126.00477,0.61911,712.58139,48.2833799999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,194,150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.138209,0,194,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1171.89873,1000,"comp"]
["CF","comp","Compensation",2536.647809,0,194,325,15,898.391809,4.8184,340,624.37623,"normal"]
["Cement","ccs","CCS",142.169572,0,194,325,15,62.166303,0.8654,92.44658,1000,"comp"]
["CF","comp","Compensation",2898.027809,0,194,400,15,898.391809,4.8184,415,614.12226,"normal"]
["Aviation","comp","Compensation",0.086335,0,194,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,1006.98734,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,194,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,194,675,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Maritime","h2","Low-emission ammonia",567.171037,0,194,675,15,126.00477,0.61911,712.58139,678.21927,"comp"]
["Maritime","h2","Low-emission ammonia",567.171037,0,194,775,15,126.00477,0.61911,712.58139,77.4192399999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,194,875,15,475.659121,2.00321,51.86914,70.48681,"ccu"]
["CF","comp","Compensation",5668.607809,0,194,975,15,898.391809,4.8184,990,213.128879999999,"normal"]
["Aviation","comp","Compensation",0.127831,0,194,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,1047.68354,"ccu"]
["CF","comp","Compensation",6029.987809,0,194,1050,15,898.391809,4.8184,1065,138.128879999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",837.935315,0,194,1125,15,475.659121,2.00321,180.84784,286.298239999999,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.124127,0,196,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},993.64557,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,196,100,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",131.956572,0,196,150,15,62.166303,0.8654,80.6451,1000,"comp"]
["CF","comp","Compensation",1813.887809,0,196,175,15,898.391809,4.8184,190,652.74963,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,196,300,15,475.659121,2.00321,51.86914,72.44648,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,196,375,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.082383,0,196,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,1013.51897999999,"ccu"]
["Maritime","h2","Low-emission ammonia",572.092797,0,196,500,15,126.00477,0.61911,720.53113,509.50127,"comp"]
["Aviation","comp","Compensation",0.090287,0,196,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,1021.26581999999,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.179483,0,196,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1694.35443,1000,"comp"]
["Maritime","h2","Low-emission ammonia",572.092797,0,196,725,15,126.00477,0.61911,720.53113,19.46946,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,196,775,15,475.659121,2.00321,51.86914,72.44648,"ccu"]
["CF","comp","Compensation",5186.767809,0,196,875,15,898.391809,4.8184,890,326.96772,"normal"]
["Maritime","h2","Low-emission ammonia",572.092797,0,196,900,15,126.00477,0.61911,720.53113,897.15413,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,196,1025,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6150.447809,0,196,1075,15,898.391809,4.8184,1090,529.70193,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.219936,0,196,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2206.41772,1000,"comp"]
["Maritime","comp","Compensation",150.769189,0,198,25,15,126.00477,0.61911,40.00003,688.48083,"ccu"]
["CF","efuel","MTO using non-fossil CO2",4689.841097,0,198,50,15,898.391809,4.8184,786.86894,1000,"comp"]
["Maritime","comp","Compensation",228.158001,0,198,150,15,126.00477,0.61911,165.00013,563.48073,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,198,200,15,475.659121,2.00321,51.86914,74.40615,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,198,275,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,198,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",761.858815,0,198,400,15,475.659121,2.00321,142.87054,47.5847599999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,198,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.171788,0,198,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1596.94937,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7159.861097,0,198,650,15,898.391809,4.8184,1299.49138,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7365.696097,0,198,700,15,898.391809,4.8184,1342.20992,1000,"comp"]
["Aviation","comp","Compensation",0.108071,0,198,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,1049.10126999999,"normal"]
["Maritime","h2","Low-emission ammonia",577.014557,0,198,825,15,126.00477,0.61911,728.48086,111.51981,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,198,925,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.127831,0,198,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,1068.48101,"ccu"]
["Primary steel","h2","DRI-EAF with H2",836.699815,0,198,1050,15,475.659121,2.00321,180.23108,258.29182,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,198,1125,15,62.166303,0.8654,74.54509,1065.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",9321.128597,0,198,1175,15,898.391809,4.8184,1748.03603,1000,"comp"]
["Maritime","comp","Compensation",181.724714,0,200,75,15,126.00477,0.61911,90.00007,646.43053,"normal"]
["Cement","ccs","CCS",129.038572,0,200,100,15,62.166303,0.8654,77.27325,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",723.391827,0,200,225,15,475.659121,2.00321,123.66787,10.9911,"comp"]
["Maritime","comp","Compensation",290.06905,0,200,250,15,126.00477,0.61911,265.00021,471.43039,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.157706,0,200,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1418.6962,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",768.437315,0,200,425,15,475.659121,2.00321,146.15452,53.84184,"comp"]
["CF","efuel","MTO using non-fossil CO2",6685.642197,0,200,525,15,898.391809,4.8184,1201.07305,1000,"comp"]
["Aviation","comp","Compensation",0.094239,0,200,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,1045.9367,"normal"]
["CF","efuel","MTO using non-fossil CO2",6994.394697,0,200,600,15,898.391809,4.8184,1265.15086,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,200,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4825.387809,0,200,800,15,898.391809,4.8184,815,583.03072,"ccu"]
["Primary steel","h2","DRI-EAF with H2",820.250315,0,200,875,15,475.659121,2.00321,172.01951,199.71596,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,200,950,15,62.166303,0.8654,74.54509,890.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.213062,0,200,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2119.40506,1000,"comp"]
["Aviation","comp","Compensation",0.131783,0,200,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,1082.74684,"normal"]
["Cement","ccs","CCS",190.316572,0,200,1150,15,62.166303,0.8654,148.08212,1000,"comp"]
["Aviation","comp","Compensation",0.048791,0,202,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,1011.75949,"normal"]
["Maritime","comp","Compensation",181.724714,0,202,75,15,126.00477,0.61911,90.00007,654.380259999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,202,175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","h2","Low-emission ammonia",586.858077,0,202,200,15,126.00477,0.61911,744.38033,221.40204,"comp"]
["Maritime","h2","Low-emission ammonia",586.858077,0,202,275,15,126.00477,0.61911,744.38033,294.08695,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,202,375,15,62.166303,0.8654,74.54509,315.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6314.340797,0,202,425,15,898.391809,4.8184,1124.01399,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,202,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["Cement","ccs","CCS",156.759572,0,202,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["CF","comp","Compensation",4102.627809,0,202,650,15,898.391809,4.8184,665,593.48425,"normal"]
["Maritime","comp","Compensation",584.146534,0,202,725,15,126.00477,0.61911,740.00059,4.37973999999997,"ccu"]
["Primary steel","h2","DRI-EAF with H2",812.436315,0,202,775,15,475.659121,2.00321,168.11877,165.452449999999,"comp"]
["CF","comp","Compensation",5066.307809,0,202,850,15,898.391809,4.8184,865,393.48425,"normal"]
["Maritime","h2","Low-emission ammonia",586.858077,0,202,925,15,126.00477,0.61911,744.38033,924.02285,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,202,1000,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",184.480572,0,202,1050,15,62.166303,0.8654,141.33842,1000,"comp"]
["Aviation","comp","Compensation",0.137711,0,202,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1165.59494,1083.3495,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.228787,0,202,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2318.4557,1000,"comp"]
["CF","comp","Compensation",1332.047809,0,204,75,15,898.391809,4.8184,90,697.88337,"normal"]
["Aviation","comp","Compensation",0.056695,0,204,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},140.07595,1029.91139,"ccu"]
["Maritime","h2","Low-emission ammonia",591.779837,0,204,175,15,126.00477,0.61911,752.33007,198.05387,"comp"]
["Maritime","comp","Compensation",290.06905,0,204,250,15,126.00477,0.61911,265.00021,487.32986,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.155091,0,204,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1385.59494,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,204,425,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",150.923572,0,204,475,15,62.166303,0.8654,102.56213,1000,"comp"]
["CF","comp","Compensation",3620.787809,0,204,550,15,898.391809,4.8184,565,632.94153,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,204,625,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,204,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4584.467809,0,204,750,15,898.391809,4.8184,765,605.59759,"ccu"]
["Maritime","h2","Low-emission ammonia",591.779837,0,204,825,15,126.00477,0.61911,752.33007,827.989759999999,"comp"]
["Cement","ccs","CCS",178.644572,0,204,950,15,62.166303,0.8654,134.59472,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.210447,0,204,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2086.3038,1000,"comp"]
["Maritime","h2","Low-emission ammonia",591.779837,0,204,1050,15,126.00477,0.61911,752.33007,312.670779999999,"normal"]
["Aviation","comp","Compensation",0.139687,0,204,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,1111.29113999999,"ccu"]
["CF","comp","Compensation",6752.747809,0,204,1200,15,898.391809,4.8184,1215,57.3231,"normal"]
["CF","comp","Compensation",1452.507809,0,206,100,15,898.391809,4.8184,115,702.33082,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,206,125,15,62.166303,0.8654,74.54509,65.45491,"normal"]
["CF","comp","Compensation",1813.887809,0,206,175,15,898.391809,4.8184,190,692.07684,"ccu"]
["Cement","ccs","CCS",140.710572,0,206,300,15,62.166303,0.8654,90.76065,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,206,325,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Maritime","comp","Compensation",382.935624,0,206,400,15,126.00477,0.61911,415.00033,345.27947,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,206,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.094239,0,206,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,1077.12658,"ccu"]
["Maritime","h2","Low-emission ammonia",596.701597,0,206,650,15,126.00477,0.61911,760.2798,659.27178,"comp"]
["Maritime","h2","Low-emission ammonia",596.701597,0,206,725,15,126.00477,0.61911,760.2798,731.95669,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.196365,0,206,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1908.05063,1000,"comp"]
["Maritime","h2","Low-emission ammonia",596.701597,0,206,875,15,126.00477,0.61911,760.2798,129.72091,"normal"]
["Cement","ccs","CCS",178.644572,0,206,950,15,62.166303,0.8654,134.59472,1000,"comp"]
["CF","comp","Compensation",5909.527809,0,206,1025,15,898.391809,4.8184,1040,246.161939999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,206,1100,15,62.166303,0.8654,74.54509,1040.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,206,1175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",970.667809,0,208,0,15,898.391809,4.8184,15,723.86823,"ccu"]
["Maritime","h2","Low-emission ammonia",601.623357,0,208,75,15,126.00477,0.61911,768.22953,102.900939999999,"comp"]
["CF","comp","Compensation",1693.427809,0,208,150,15,898.391809,4.8184,165,703.36028,"normal"]
["CF","efuel","MTO using non-fossil CO2",5509.189097,0,208,200,15,898.391809,4.8184,956.9146,1000,"comp"]
["Maritime","comp","Compensation",321.024575,0,208,300,15,126.00477,0.61911,315.00025,453.229279999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,208,350,15,475.659121,2.00321,51.86914,84.2045199999999,"ccu"]
["CF","comp","Compensation",3138.947809,0,208,450,15,898.391809,4.8184,465,662.34438,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.171637,0,208,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1595.03797,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",797.629815,0,208,550,15,475.659121,2.00321,160.72738,86.97429,"comp"]
["CF","comp","Compensation",4102.627809,0,208,650,15,898.391809,4.8184,665,635.00045,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.18867,0,208,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1810.64557,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,208,775,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",8185.044097,0,208,850,15,898.391809,4.8184,1512.25558,1000,"comp"]
["Aviation","comp","Compensation",0.119927,0,208,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},940.48101,1112.70886,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,208,1000,15,475.659121,2.00321,51.86914,84.2045199999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,208,1075,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,208,1150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",872.470815,0,208,1200,15,475.659121,2.00321,198.08792,297.68135,"comp"]
["Cement","comp","Compensation",118.417303,0,210,50,15,62.166303,0.8654,65,9.54509,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.140522,0,210,125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1201.17722,1000,"comp"]
["Maritime","comp","Compensation",259.113525,0,210,200,15,126.00477,0.61911,215.00017,561.1791,"normal"]
["CF","efuel","MTO using non-fossil CO2",5858.310197,0,210,275,15,898.391809,4.8184,1029.37041,1000,"comp"]
["Aviation","comp","Compensation",0.074479,0,210,350,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},365.18987,1078.54431,"normal"]
["Maritime","comp","Compensation",382.935624,0,210,400,15,126.00477,0.61911,415.00033,361.178939999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",789.815815,0,210,450,15,475.659121,2.00321,156.82664,52.71078,"comp"]
["Aviation","comp","Compensation",0.090287,0,210,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,1094.05063,"ccu"]
["Maritime","h2","Low-emission ammonia",606.545117,0,210,600,15,126.00477,0.61911,776.17927,612.57544,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,210,700,15,62.166303,0.8654,74.54509,640.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7813.742697,0,210,750,15,898.391809,4.8184,1435.19652,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,210,900,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","h2","Low-emission ammonia",606.545117,0,210,925,15,126.00477,0.61911,776.17927,163.82148,"normal"]
["CF","comp","Compensation",5668.607809,0,210,975,15,898.391809,4.8184,990,323.839629999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,210,1100,15,62.166303,0.8654,74.54509,1040.45491,"ccu"]
["Primary steel","h2","DRI-EAF with H2",864.656815,0,210,1100,15,475.659121,2.00321,194.18718,263.41784,"comp"]
["Cement","ccs","CCS",191.775572,0,210,1175,15,62.166303,0.8654,149.76805,1000,"comp"]
["Maritime","h2","Low-emission ammonia",611.466877,0,212,25,15,126.00477,0.61911,784.129,56.2046,"comp"]
["Aviation","comp","Compensation",0.060647,0,212,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,1075.37973999999,"normal"]
["Maritime","comp","Compensation",274.591288,0,212,225,15,126.00477,0.61911,240.00019,544.12881,"ccu"]
["Aviation","comp","Compensation",0.066575,0,212,250,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},265.13924,1081.18987,"normal"]
["CF","comp","Compensation",2536.647809,0,212,325,15,898.391809,4.8184,340,695.16522,"ccu"]
["CF","comp","Compensation",2898.027809,0,212,400,15,898.391809,4.8184,415,684.91125,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,212,525,15,62.166303,0.8654,74.54509,465.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",7133.688797,0,212,575,15,898.391809,4.8184,1294.05964,1000,"comp"]
["Maritime","comp","Compensation",553.191009,0,212,675,15,126.00477,0.61911,690.00055,94.12845,"normal"]
["Aviation","comp","Compensation",0.102143,0,212,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,1116.06329,"normal"]
["CF","comp","Compensation",4825.387809,0,212,800,15,898.391809,4.8184,815,512.67847,"normal"]
["Maritime","h2","Low-emission ammonia",611.466877,0,212,875,15,126.00477,0.61911,784.129,105.87171,"ccu"]
["Primary steel","h2","DRI-EAF with H2",848.207315,0,212,925,15,475.659121,2.00321,185.97561,204.84198,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.21799,0,212,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2181.78481,1000,"comp"]
["Maritime","h2","Low-emission ammonia",611.466877,0,212,1075,15,126.00477,0.61911,784.129,1073.79335,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,212,1150,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",4806.954897,0,214,0,15,898.391809,4.8184,811.17447,1000,"comp"]
["Aviation","comp","Compensation",0.052743,0,214,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},90.05063,1078.02532,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,214,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["CF","comp","Compensation",2054.807809,0,214,225,15,898.391809,4.8184,240,716.70263,"normal"]
["Aviation","comp","Compensation",0.068551,0,214,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},290.1519,1093.53164,"ccu"]
["Primary steel","h2","DRI-EAF with H2",785.701815,0,214,350,15,475.659121,2.00321,154.77294,16.6002299999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,214,450,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.171972,0,214,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1599.27848,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,214,575,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",159.677572,0,214,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["Aviation","comp","Compensation",0.104119,0,214,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,1128.40506,"normal"]
["CF","efuel","MTO using non-fossil CO2",8100.314897,0,214,800,15,898.391809,4.8184,1494.67107,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,214,850,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.119927,0,214,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},940.48101,1143.9114,"ccu"]
["Maritime","h2","Low-emission ammonia",616.388637,0,214,975,15,126.00477,0.61911,792.07874,977.760269999999,"comp"]
["Maritime","h2","Low-emission ammonia",616.388637,0,214,1075,15,126.00477,0.61911,792.07874,297.92213,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.227328,0,214,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2299.98734,1000,"comp"]
["Maritime","h2","Low-emission ammonia",616.388637,0,214,1200,15,126.00477,0.61911,792.07874,422.92222,"normal"]
["Cement","ccs","CCS",126.120572,0,216,50,15,62.166303,0.8654,73.9014,1000,"comp"]
["CF","comp","Compensation",1572.967809,0,216,125,15,898.391809,4.8184,140,738.24004,"normal"]
["Primary steel","ccs","BF-BOF + CCS",704.279077,0,216,200,15,475.659121,2.00321,114.1268,33.87151,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,216,275,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2536.647809,0,216,325,15,898.391809,4.8184,340,710.896109999999,"ccu"]
["Maritime","h2","Low-emission ammonia",621.310397,0,216,400,15,126.00477,0.61911,800.02847,421.389429999999,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,216,475,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",156.759572,0,216,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["Maritime","comp","Compensation",522.235484,0,216,625,15,126.00477,0.61911,640.00051,160.02796,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,216,675,15,475.659121,2.00321,51.86914,92.04321,"ccu"]
["Maritime","h2","Low-emission ammonia",621.310397,0,216,800,15,126.00477,0.61911,800.02847,809.04228,"comp"]
["CF","comp","Compensation",5066.307809,0,216,850,15,898.391809,4.8184,865,639.118289999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.213246,0,216,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2121.73418,1000,"comp"]
["CF","comp","Compensation",5668.607809,0,216,975,15,898.391809,4.8184,990,622.02833,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.219633,0,216,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2202.58228,1000,"comp"]
["CF","comp","Compensation",6632.287809,0,216,1175,15,898.391809,4.8184,1190,165.35616,"normal"]
["Aviation","comp","Compensation",0.046815,0,218,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,1093,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,218,100,15,62.166303,0.8654,74.54509,40.45491,"normal"]
["CF","comp","Compensation",1693.427809,0,218,150,15,898.391809,4.8184,165,742.68749,"ccu"]
["Maritime","h2","Low-emission ammonia",626.232157,0,218,225,15,126.00477,0.61911,807.97821,252.67143,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,218,250,15,475.659121,2.00321,51.86914,94.0028799999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.165099,0,218,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1512.27848,1000,"comp"]
["Maritime","comp","Compensation",413.891148,0,218,450,15,126.00477,0.61911,465.00037,342.97784,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,218,500,15,475.659121,2.00321,51.86914,94.0028799999999,"ccu"]
["CF","comp","Compensation",3861.707809,0,218,600,15,898.391809,4.8184,615,681.16364,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,218,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,218,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4825.387809,0,218,800,15,898.391809,4.8184,815,653.81971,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.205551,0,218,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2024.32911,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,218,950,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","comp","Compensation",5789.067809,0,218,1000,15,898.391809,4.8184,1015,354.194999999999,"normal"]
["Aviation","comp","Compensation",0.131783,0,218,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,1176.32912,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,218,1150,15,475.659121,2.00321,51.86914,94.0028799999999,"ccu"]
["Cement","comp","Compensation",75.147303,0,220,0,15,62.166303,0.8654,15,59.54509,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.136113,0,220,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1145.36709,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",646.940827,0,220,125,15,475.659121,2.00321,85.50362,61.87793,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,220,200,15,62.166303,0.8654,74.54509,140.454909999999,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.157404,0,220,275,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1414.87342,1000,"comp"]
["Maritime","comp","Compensation",351.980099,0,220,350,15,126.00477,0.61911,365.00029,450.92765,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,220,400,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Aviation","comp","Compensation",0.086335,0,220,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,1142.15189999999,"normal"]
["Maritime","comp","Compensation",475.802198,0,220,550,15,126.00477,0.61911,565.00045,250.92749,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,220,650,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","h2","DRI-EAF with H2",839.979315,0,220,725,15,475.659121,2.00321,181.8682,132.6209,"comp"]
["Maritime","h2","Low-emission ammonia",631.153917,0,220,750,15,126.00477,0.61911,815.92794,762.345949999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,220,850,15,62.166303,0.8654,74.54509,790.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",8633.090697,0,220,900,15,898.391809,4.8184,1605.24217,1000,"comp"]
["Maritime","h2","Low-emission ammonia",631.153917,0,220,1000,15,126.00477,0.61911,815.92794,199.072869999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",9147.678197,0,220,1025,15,898.391809,4.8184,1712.03852,1000,"comp"]
["CF","comp","Compensation",6391.367809,0,220,1125,15,898.391809,4.8184,1140,243.03385,"normal"]
["Maritime","h2","Low-emission ammonia",631.153917,0,220,1200,15,126.00477,0.61911,815.92794,399.07302,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",570.489827,0,222,25,15,475.659121,2.00321,47.33937,96.1414399999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,222,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["Aviation","comp","Compensation",0.060647,0,222,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,1127.36708,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,222,250,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",6306.356797,0,222,325,15,898.391809,4.8184,1122.357,1000,"comp"]
["Aviation","comp","Compensation",0.078431,0,222,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,1144.79747,"normal"]
["Maritime","h2","Low-emission ammonia",636.075677,0,222,500,15,126.00477,0.61911,823.87767,520.94305,"comp"]
["CF","comp","Compensation",3620.787809,0,222,550,15,898.391809,4.8184,565,703.73051,"normal"]
["Aviation","comp","Compensation",0.094239,0,222,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,1160.30379,"ccu"]
["Primary steel","h2","DRI-EAF with H2",837.922315,0,222,675,15,475.659121,2.00321,180.84135,114.56562,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,222,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,222,875,15,475.659121,2.00321,51.86914,97.92223,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,222,900,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Maritime","h2","Low-emission ammonia",636.075677,0,222,1025,15,126.00477,0.61911,823.87767,216.123159999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",883.978315,0,222,1075,15,475.659121,2.00321,203.83245,244.23151,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,222,1150,15,62.166303,0.8654,74.54509,1090.45491,"ccu"]
["Maritime","h2","Low-emission ammonia",640.997437,0,224,0,15,126.00477,0.61911,831.82741,37.25711,"comp"]
["Aviation","comp","Compensation",0.048791,0,224,25,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},40.02532,1126.13924,"ccu"]
["CF","efuel","MTO using non-fossil CO2",5626.302897,0,224,150,15,898.391809,4.8184,981.22013,1000,"comp"]
["Aviation","comp","Compensation",0.064599,0,224,225,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},240.12658,1141.63290999999,"normal"]
["CF","comp","Compensation",2416.187809,0,224,300,15,898.391809,4.8184,315,745.775869999999,"normal"]
["CF","comp","Compensation",2777.567809,0,224,375,15,898.391809,4.8184,390,735.5219,"normal"]
["Aviation","comp","Compensation",0.080407,0,224,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,1157.13924,"ccu"]
["Primary steel","h2","DRI-EAF with H2",821.472815,0,224,500,15,475.659121,2.00321,172.62978,55.9897599999999,"comp"]
["Maritime","comp","Compensation",475.802198,0,224,550,15,126.00477,0.61911,565.00045,266.82696,"ccu"]
["Maritime","h2","Low-emission ammonia",640.997437,0,224,650,15,126.00477,0.61911,831.82741,667.193,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,224,725,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",168.431572,0,224,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["Aviation","comp","Compensation",0.115975,0,224,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,1192.01265,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,224,925,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","comp","Compensation",5909.527809,0,224,1025,15,898.391809,4.8184,1040,370.71154,"normal"]
["Aviation","comp","Compensation",0.131783,0,224,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,1207.51899,"ccu"]
["Maritime","h2","Low-emission ammonia",640.997437,0,224,1125,15,126.00477,0.61911,831.82741,1127.53076999999,"comp"]
["Cement","comp","Compensation",75.147303,0,226,0,15,62.166303,0.8654,15,59.54509,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,226,75,15,62.166303,0.8654,74.54509,15.4549099999999,"normal"]
["Maritime","comp","Compensation",212.680238,0,226,125,15,126.00477,0.61911,140.00011,699.77703,"normal"]
["Cement","ccs","CCS",134.874572,0,226,200,15,62.166303,0.8654,84.01695,1000,"comp"]
["CF","comp","Compensation",2295.727809,0,226,275,15,898.391809,4.8184,290,757.05931,"normal"]
["CF","efuel","MTO using non-fossil CO2",6387.093997,0,226,325,15,898.391809,4.8184,1139.11302,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,226,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3259.407809,0,226,475,15,898.391809,4.8184,490,729.715369999999,"ccu"]
["Maritime","h2","Low-emission ammonia",645.919197,0,226,550,15,126.00477,0.61911,839.77714,571.159929999999,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,226,625,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Aviation","comp","Compensation",0.102143,0,226,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,1188.8481,"ccu"]
["Maritime","comp","Compensation",615.102058,0,226,775,15,126.00477,0.61911,790.00063,49.77651,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,226,825,15,475.659121,2.00321,51.86914,101.84158,"ccu"]
["CF","comp","Compensation",5427.687809,0,226,925,15,898.391809,4.8184,940,484.550379999999,"normal"]
["Primary steel","h2","DRI-EAF with H2",876.985815,0,226,950,15,475.659121,2.00321,200.3418,200.01685,"comp"]
["Primary steel","h2","DRI-EAF with H2",885.621315,0,226,1025,15,475.659121,2.00321,204.65263,224.32921,"comp"]
["CF","comp","Compensation",6391.367809,0,226,1125,15,898.391809,4.8184,1140,640.84759,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.236515,0,226,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2416.27848,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,228,50,15,475.659121,2.00321,51.86914,13.1308599999999,"normal"]
["Cement","ccs","CCS",129.038572,0,228,100,15,62.166303,0.8654,77.27325,1000,"comp"]
["Aviation","comp","Compensation",0.060647,0,228,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,1158.55696,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,228,250,15,475.659121,2.00321,51.86914,103.80125,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,228,325,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,228,450,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","comp","Compensation",3259.407809,0,228,475,15,898.391809,4.8184,490,737.580819999999,"ccu"]
["Maritime","comp","Compensation",506.757722,0,228,600,15,126.00477,0.61911,615.00049,232.72639,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.188367,0,228,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1806.81013,1000,"comp"]
["CF","comp","Compensation",4584.467809,0,228,750,15,898.391809,4.8184,765,673.38922,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.2054,0,228,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2022.41772,1000,"comp"]
["Aviation","comp","Compensation",0.112023,0,228,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,1208.93671,"normal"]
["CF","comp","Compensation",5548.147809,0,228,950,15,898.391809,4.8184,965,672.63898,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,228,975,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,228,1100,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,228,1100,15,475.659121,2.00321,51.86914,103.80125,"ccu"]
["Maritime","comp","Compensation",150.769189,0,230,25,15,126.00477,0.61911,40.00003,815.67658,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,230,75,15,475.659121,2.00321,51.86914,38.13086,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,230,150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,230,225,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",761.617327,0,230,275,15,475.659121,2.00321,142.74999,22.4884,"comp"]
["CF","comp","Compensation",2777.567809,0,230,375,15,898.391809,4.8184,390,759.11823,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.174285,0,230,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1628.55696,1000,"comp"]
["Maritime","comp","Compensation",444.846673,0,230,500,15,126.00477,0.61911,515.00041,340.6762,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,230,600,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.098191,0,230,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,1205.77215,"normal"]
["Maritime","comp","Compensation",568.668771,0,230,700,15,126.00477,0.61911,715.00057,140.676039999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,230,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5066.307809,0,230,850,15,898.391809,4.8184,865,694.17639,"ccu"]
["CF","efuel","MTO using non-fossil CO2",9040.768697,0,230,950,15,898.391809,4.8184,1689.85076,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,230,1000,15,62.166303,0.8654,74.54509,940.45491,"ccu"]
["CF","efuel","MTO using non-fossil CO2",9452.438697,0,230,1050,15,898.391809,4.8184,1775.28783,1000,"comp"]
["Maritime","h2","Low-emission ammonia",655.762717,0,230,1150,15,126.00477,0.61911,855.67661,309.324319999999,"normal"]
["Maritime","comp","Compensation",135.291427,0,232,0,15,126.00477,0.61911,15.00001,848.62634,"normal"]
["Aviation","comp","Compensation",0.052743,0,232,75,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},90.05063,1171.59494,"normal"]
["Maritime","comp","Compensation",212.680238,0,232,125,15,126.00477,0.61911,140.00011,723.62624,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",685.166327,0,232,175,15,475.659121,2.00321,104.58574,56.7519099999999,"comp"]
["CF","comp","Compensation",2295.727809,0,232,275,15,898.391809,4.8184,290,780.65564,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",818.955577,0,232,350,15,475.659121,2.00321,171.37317,0.0230900000000247,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,232,400,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["CF","efuel","MTO using non-fossil CO2",7125.704797,0,232,475,15,898.391809,4.8184,1292.40266,1000,"comp"]
["Aviation","comp","Compensation",0.090287,0,232,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,1208.41772,"normal"]
["Cement","ccs","CCS",159.677572,0,232,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["CF","comp","Compensation",4343.547809,0,232,700,15,898.391809,4.8184,715,722.54978,"normal"]
["Aviation","comp","Compensation",0.106095,0,232,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,1223.91138999999,"ccu"]
["Primary steel","h2","DRI-EAF with H2",873.693315,0,232,825,15,475.659121,2.00321,198.69819,153.95515,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,232,900,15,62.166303,0.8654,74.54509,840.45491,"ccu"]
["CF","comp","Compensation",5789.067809,0,232,1000,15,898.391809,4.8184,1015,681.53388,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,232,1050,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",187.398572,0,232,1100,15,62.166303,0.8654,144.71027,1000,"comp"]
["Aviation","comp","Compensation",0.141663,0,232,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,1258.79747,"normal"]
["Maritime","h2","Low-emission ammonia",665.606237,0,234,25,15,126.00477,0.61911,871.57608,65.8860999999999,"comp"]
["Maritime","h2","Low-emission ammonia",665.606237,0,234,150,15,126.00477,0.61911,871.57608,187.027619999999,"comp"]
["Aviation","comp","Compensation",0.060647,0,234,175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},190.10127,1189.74683,"ccu"]
["CF","efuel","MTO using non-fossil CO2",6445.650897,0,234,300,15,898.391809,4.8184,1151.26579,1000,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,234,325,15,62.166303,0.8654,74.54509,265.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,234,400,15,475.659121,2.00321,51.86914,109.68027,"ccu"]
["CF","comp","Compensation",3500.327809,0,234,525,15,898.391809,4.8184,540,754.34116,"normal"]
["Cement","ccs","CCS",153.841572,0,234,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["Primary steel","h2","DRI-EAF with H2",857.243815,0,234,650,15,475.659121,2.00321,190.48662,95.37929,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,234,725,15,62.166303,0.8654,74.54509,665.45491,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,234,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,234,875,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Maritime","h2","Low-emission ammonia",665.606237,0,234,875,15,126.00477,0.61911,871.57608,889.64842,"comp"]
["Aviation","comp","Compensation",0.127831,0,234,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,1255.63291,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.227026,0,234,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2296.16456,1000,"comp"]
["CF","comp","Compensation",6632.287809,0,234,1175,15,898.391809,4.8184,1190,289.90576,"normal"]
["Aviation","comp","Compensation",0.046815,0,236,0,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},15.01266,1186.58227999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",608.715327,0,236,75,15,475.659121,2.00321,66.4215,92.86245,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,236,150,15,62.166303,0.8654,74.54509,90.45491,"ccu"]
["Maritime","comp","Compensation",243.635763,0,236,175,15,126.00477,0.61911,190.00015,689.52566,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,236,300,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",143.628572,0,236,350,15,62.166303,0.8654,94.1325,1000,"comp"]
["CF","comp","Compensation",3018.487809,0,236,425,15,898.391809,4.8184,440,775.87857,"normal"]
["Maritime","comp","Compensation",460.324435,0,236,525,15,126.00477,0.61911,540.00043,339.525379999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,236,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.098191,0,236,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,1236.96203,"ccu"]
["Maritime","h2","Low-emission ammonia",670.527997,0,236,700,15,126.00477,0.61911,879.52581,720.93043,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,236,775,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,236,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Maritime","h2","Low-emission ammonia",670.527997,0,236,925,15,126.00477,0.61911,879.52581,60.47494,"normal"]
["Cement","ccs","CCS",181.562572,0,236,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["CF","comp","Compensation",6150.447809,0,236,1075,15,898.391809,4.8184,1090,403.7446,"normal"]
["Aviation","comp","Compensation",0.135735,0,236,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1140.58228,1273.77214999999,"ccu"]
["CF","efuel","MTO using non-fossil CO2",10088.131997,0,236,1175,15,898.391809,4.8184,1907.2182,1000,"comp"]
["CF","comp","Compensation",1211.587809,0,238,50,15,898.391809,4.8184,65,835.01389,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.149893,0,238,100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1319.79747,1000,"comp"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,238,200,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Aviation","comp","Compensation",0.070527,0,238,300,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},315.16456,1220.22785,"normal"]
["Maritime","comp","Compensation",351.980099,0,238,350,15,126.00477,0.61911,365.00029,522.475259999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,238,400,15,475.659121,2.00321,51.86914,113.59962,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,238,475,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["Aviation","comp","Compensation",0.090287,0,238,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,1239.60758999999,"ccu"]
["Maritime","h2","Low-emission ammonia",675.449757,0,238,650,15,126.00477,0.61911,887.47555,673.35396,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,238,675,15,62.166303,0.8654,74.54509,615.45491,"ccu"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.205249,0,238,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2020.50633,1000,"comp"]
["Maritime","comp","Compensation",646.057583,0,238,825,15,126.00477,0.61911,840.00067,47.4748799999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,238,925,15,475.659121,2.00321,51.86914,113.59962,"ccu"]
["Aviation","comp","Compensation",0.123879,0,238,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},990.50633,1272.5443,"normal"]
["CF","comp","Compensation",6270.907809,0,238,1100,15,898.391809,4.8184,1115,691.458239999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,238,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6632.287809,0,238,1175,15,898.391809,4.8184,1190,681.20427,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,240,75,15,62.166303,0.8654,74.54509,15.4549099999999,"ccu"]
["Cement","ccs","CCS",122.327172,0.05836,240,100,15,62.166303,0.8654,74.54509,40.45491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,225,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Maritime","comp","Compensation",290.06905,0,240,250,15,126.00477,0.61911,265.00021,630.42507,"normal"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.169876,0,240,325,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1572.74684,1000,"comp"]
["Cement","ccs","CCS",145.087572,0,240,375,15,62.166303,0.8654,95.81843,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",6875.509197,0,240,375,15,898.391809,4.8184,1240.47762,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.174134,0,240,375,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1626.64557,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,375,15,126.00477,0.61911,895.42528,407.72276,"comp"]
["Primary steel","h2","DRI-EAF with H2",836.680315,0,240,375,15,475.659121,2.00321,180.22134,0.692900000000008,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,400,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",2898.027809,0,240,400,15,898.391809,4.8184,415,795.02745,"normal"]
["Aviation","comp","Compensation",0.078431,0,240,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,1238.37975,"normal"]
["Maritime","comp","Compensation",382.935624,0,240,400,15,126.00477,0.61911,415.00033,480.42495,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,400,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,400,15,62.166303,0.8654,74.54509,340.45491,"ccu"]
["CF","comp","Compensation",2898.027809,0,240,400,15,898.391809,4.8184,415,795.02745,"ccu"]
["Aviation","comp","Compensation",0.078431,0,240,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},415.21519,1238.37975,"ccu"]
["Maritime","comp","Compensation",382.935624,0,240,400,15,126.00477,0.61911,415.00033,480.42495,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,400,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",146.546572,0,240,400,15,62.166303,0.8654,97.50436,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",6978.426697,0,240,400,15,898.391809,4.8184,1261.83689,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.176263,0,240,400,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1653.59494,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,400,15,126.00477,0.61911,895.42528,431.95106,"comp"]
["Primary steel","h2","DRI-EAF with H2",839.558815,0,240,400,15,475.659121,2.00321,181.65829,8.79701,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,425,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3018.487809,0,240,425,15,898.391809,4.8184,440,791.609459999999,"normal"]
["Aviation","comp","Compensation",0.080407,0,240,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,1240.31645,"normal"]
["Maritime","comp","Compensation",398.413386,0,240,425,15,126.00477,0.61911,440.00035,455.42493,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,425,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,425,15,62.166303,0.8654,74.54509,365.45491,"ccu"]
["CF","comp","Compensation",3018.487809,0,240,425,15,898.391809,4.8184,440,791.609459999999,"ccu"]
["Aviation","comp","Compensation",0.080407,0,240,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},440.22785,1240.31645,"ccu"]
["Maritime","comp","Compensation",398.413386,0,240,425,15,126.00477,0.61911,440.00035,455.42493,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,425,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",148.005572,0,240,425,15,62.166303,0.8654,99.19028,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7081.344197,0,240,425,15,898.391809,4.8184,1283.19616,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.178392,0,240,425,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1680.5443,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,425,15,126.00477,0.61911,895.42528,456.179369999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",842.437315,0,240,425,15,475.659121,2.00321,183.09523,16.90113,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,450,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3138.947809,0,240,450,15,898.391809,4.8184,465,788.19147,"normal"]
["Aviation","comp","Compensation",0.082383,0,240,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,1242.25316,"normal"]
["Maritime","comp","Compensation",413.891148,0,240,450,15,126.00477,0.61911,465.00037,430.42491,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,450,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,450,15,62.166303,0.8654,74.54509,390.45491,"ccu"]
["CF","comp","Compensation",3138.947809,0,240,450,15,898.391809,4.8184,465,788.19147,"ccu"]
["Aviation","comp","Compensation",0.082383,0,240,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},465.24051,1242.25316,"ccu"]
["Maritime","comp","Compensation",413.891148,0,240,450,15,126.00477,0.61911,465.00037,430.42491,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,450,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",149.464572,0,240,450,15,62.166303,0.8654,100.87621,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7184.261697,0,240,450,15,898.391809,4.8184,1304.55543,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.180521,0,240,450,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1707.49367,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,450,15,126.00477,0.61911,895.42528,480.407669999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",845.315815,0,240,450,15,475.659121,2.00321,184.53217,25.0052499999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,475,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3259.407809,0,240,475,15,898.391809,4.8184,490,784.77348,"normal"]
["Aviation","comp","Compensation",0.084359,0,240,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},490.25316,1244.18988,"normal"]
["Maritime","comp","Compensation",429.368911,0,240,475,15,126.00477,0.61911,490.00039,405.42489,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,475,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,475,15,62.166303,0.8654,74.54509,415.45491,"ccu"]
["CF","comp","Compensation",3259.407809,0,240,475,15,898.391809,4.8184,490,784.77348,"ccu"]
["Aviation","comp","Compensation",0.084359,0,240,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},490.25316,1244.18988,"ccu"]
["Maritime","comp","Compensation",429.368911,0,240,475,15,126.00477,0.61911,490.00039,405.42489,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,475,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",150.923572,0,240,475,15,62.166303,0.8654,102.56213,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7287.179197,0,240,475,15,898.391809,4.8184,1325.9147,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.18265,0,240,475,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1734.44304,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,475,15,126.00477,0.61911,895.42528,504.635969999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",848.194315,0,240,475,15,475.659121,2.00321,185.96912,33.10936,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,500,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3379.867809,0,240,500,15,898.391809,4.8184,515,781.35548,"normal"]
["Aviation","comp","Compensation",0.086335,0,240,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,1246.12658999999,"normal"]
["Maritime","comp","Compensation",444.846673,0,240,500,15,126.00477,0.61911,515.00041,380.42487,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,500,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,500,15,62.166303,0.8654,74.54509,440.45491,"ccu"]
["CF","comp","Compensation",3379.867809,0,240,500,15,898.391809,4.8184,515,781.35548,"ccu"]
["Aviation","comp","Compensation",0.086335,0,240,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},515.26582,1246.12658999999,"ccu"]
["Maritime","comp","Compensation",444.846673,0,240,500,15,126.00477,0.61911,515.00041,380.42487,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,500,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",152.382572,0,240,500,15,62.166303,0.8654,104.24806,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7390.096697,0,240,500,15,898.391809,4.8184,1347.27397,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.184779,0,240,500,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1761.39241,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,500,15,126.00477,0.61911,895.42528,528.864279999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",851.072815,0,240,500,15,475.659121,2.00321,187.40606,41.21348,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,525,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3500.327809,0,240,525,15,898.391809,4.8184,540,777.93749,"normal"]
["Aviation","comp","Compensation",0.088311,0,240,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,1248.06329,"normal"]
["Maritime","comp","Compensation",460.324435,0,240,525,15,126.00477,0.61911,540.00043,355.42485,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,525,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,525,15,62.166303,0.8654,74.54509,465.45491,"ccu"]
["CF","comp","Compensation",3500.327809,0,240,525,15,898.391809,4.8184,540,777.93749,"ccu"]
["Aviation","comp","Compensation",0.088311,0,240,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},540.27848,1248.06329,"ccu"]
["Maritime","comp","Compensation",460.324435,0,240,525,15,126.00477,0.61911,540.00043,355.42485,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,525,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",153.841572,0,240,525,15,62.166303,0.8654,105.93398,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7493.014197,0,240,525,15,898.391809,4.8184,1368.63324,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.186908,0,240,525,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1788.34177,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,525,15,126.00477,0.61911,895.42528,553.092579999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",853.951315,0,240,525,15,475.659121,2.00321,188.843,49.31761,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,550,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3620.787809,0,240,550,15,898.391809,4.8184,565,774.5195,"normal"]
["Aviation","comp","Compensation",0.090287,0,240,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,1250,"normal"]
["Maritime","comp","Compensation",475.802198,0,240,550,15,126.00477,0.61911,565.00045,330.42483,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,550,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,550,15,62.166303,0.8654,74.54509,490.45491,"ccu"]
["CF","comp","Compensation",3620.787809,0,240,550,15,898.391809,4.8184,565,774.5195,"ccu"]
["Aviation","comp","Compensation",0.090287,0,240,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},565.29114,1250,"ccu"]
["Maritime","comp","Compensation",475.802198,0,240,550,15,126.00477,0.61911,565.00045,330.42483,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,550,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",155.300572,0,240,550,15,62.166303,0.8654,107.61991,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7595.931697,0,240,550,15,898.391809,4.8184,1389.99251,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.189037,0,240,550,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1815.29114,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,550,15,126.00477,0.61911,895.42528,577.320879999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",856.829815,0,240,550,15,475.659121,2.00321,190.27995,57.4217199999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,575,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3741.247809,0,240,575,15,898.391809,4.8184,590,771.10151,"normal"]
["Aviation","comp","Compensation",0.092263,0,240,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,1251.93671,"normal"]
["Maritime","comp","Compensation",491.27996,0,240,575,15,126.00477,0.61911,590.00047,305.42481,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,575,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,575,15,62.166303,0.8654,74.54509,515.45491,"ccu"]
["CF","comp","Compensation",3741.247809,0,240,575,15,898.391809,4.8184,590,771.10151,"ccu"]
["Aviation","comp","Compensation",0.092263,0,240,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},590.3038,1251.93671,"ccu"]
["Maritime","comp","Compensation",491.27996,0,240,575,15,126.00477,0.61911,590.00047,305.42481,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,575,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",156.759572,0,240,575,15,62.166303,0.8654,109.30583,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7698.849197,0,240,575,15,898.391809,4.8184,1411.35177,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.191166,0,240,575,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1842.24051,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,575,15,126.00477,0.61911,895.42528,601.54919,"comp"]
["Primary steel","h2","DRI-EAF with H2",859.708315,0,240,575,15,475.659121,2.00321,191.71689,65.5258399999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,600,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3861.707809,0,240,600,15,898.391809,4.8184,615,767.68352,"normal"]
["Aviation","comp","Compensation",0.094239,0,240,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,1253.87341,"normal"]
["Maritime","comp","Compensation",506.757722,0,240,600,15,126.00477,0.61911,615.00049,280.42479,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,600,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,600,15,62.166303,0.8654,74.54509,540.45491,"ccu"]
["CF","comp","Compensation",3861.707809,0,240,600,15,898.391809,4.8184,615,767.68352,"ccu"]
["Aviation","comp","Compensation",0.094239,0,240,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},615.31646,1253.87341,"ccu"]
["Maritime","comp","Compensation",506.757722,0,240,600,15,126.00477,0.61911,615.00049,280.42479,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,600,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",158.218572,0,240,600,15,62.166303,0.8654,110.99176,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7801.766697,0,240,600,15,898.391809,4.8184,1432.71104,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.193295,0,240,600,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1869.18987,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,600,15,126.00477,0.61911,895.42528,625.77749,"comp"]
["Primary steel","h2","DRI-EAF with H2",862.586815,0,240,600,15,475.659121,2.00321,193.15384,73.62995,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,625,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",3982.167809,0,240,625,15,898.391809,4.8184,640,764.265529999999,"normal"]
["Aviation","comp","Compensation",0.096215,0,240,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,1255.82279,"normal"]
["Maritime","comp","Compensation",522.235484,0,240,625,15,126.00477,0.61911,640.00051,255.42477,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,625,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,625,15,62.166303,0.8654,74.54509,565.45491,"ccu"]
["CF","comp","Compensation",3982.167809,0,240,625,15,898.391809,4.8184,640,764.265529999999,"ccu"]
["Aviation","comp","Compensation",0.096215,0,240,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},640.32911,1255.82279,"ccu"]
["Maritime","comp","Compensation",522.235484,0,240,625,15,126.00477,0.61911,640.00051,255.42477,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,625,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",159.677572,0,240,625,15,62.166303,0.8654,112.67769,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",7904.684197,0,240,625,15,898.391809,4.8184,1454.07031,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.195425,0,240,625,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1896.1519,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,625,15,126.00477,0.61911,895.42528,650.0058,"comp"]
["Primary steel","h2","DRI-EAF with H2",865.465315,0,240,625,15,475.659121,2.00321,194.59078,81.73407,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,650,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4102.627809,0,240,650,15,898.391809,4.8184,665,760.84753,"normal"]
["Aviation","comp","Compensation",0.098191,0,240,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,1257.7595,"normal"]
["Maritime","comp","Compensation",537.713247,0,240,650,15,126.00477,0.61911,665.00053,230.42475,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,650,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,650,15,62.166303,0.8654,74.54509,590.45491,"ccu"]
["CF","comp","Compensation",4102.627809,0,240,650,15,898.391809,4.8184,665,760.84753,"ccu"]
["Aviation","comp","Compensation",0.098191,0,240,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},665.34177,1257.7595,"ccu"]
["Maritime","comp","Compensation",537.713247,0,240,650,15,126.00477,0.61911,665.00053,230.42475,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,650,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",161.136572,0,240,650,15,62.166303,0.8654,114.36361,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8007.601697,0,240,650,15,898.391809,4.8184,1475.42958,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.197554,0,240,650,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1923.10127,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,650,15,126.00477,0.61911,895.42528,674.2341,"comp"]
["Primary steel","h2","DRI-EAF with H2",868.343815,0,240,650,15,475.659121,2.00321,196.02772,89.83819,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,675,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4223.087809,0,240,675,15,898.391809,4.8184,690,757.42954,"normal"]
["Aviation","comp","Compensation",0.100167,0,240,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,1259.69619999999,"normal"]
["Maritime","comp","Compensation",553.191009,0,240,675,15,126.00477,0.61911,690.00055,205.42473,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,675,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,675,15,62.166303,0.8654,74.54509,615.45491,"ccu"]
["CF","comp","Compensation",4223.087809,0,240,675,15,898.391809,4.8184,690,757.42954,"ccu"]
["Aviation","comp","Compensation",0.100167,0,240,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},690.35443,1259.69619999999,"ccu"]
["Maritime","comp","Compensation",553.191009,0,240,675,15,126.00477,0.61911,690.00055,205.42473,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,675,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",162.595572,0,240,675,15,62.166303,0.8654,116.04954,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8110.519197,0,240,675,15,898.391809,4.8184,1496.78885,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.199683,0,240,675,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1950.05063,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,675,15,126.00477,0.61911,895.42528,698.4624,"comp"]
["Primary steel","h2","DRI-EAF with H2",871.222315,0,240,675,15,475.659121,2.00321,197.46467,97.9422999999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,700,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4343.547809,0,240,700,15,898.391809,4.8184,715,754.011549999999,"normal"]
["Aviation","comp","Compensation",0.102143,0,240,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,1261.63291,"normal"]
["Maritime","comp","Compensation",568.668771,0,240,700,15,126.00477,0.61911,715.00057,180.42471,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,700,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,700,15,62.166303,0.8654,74.54509,640.45491,"ccu"]
["CF","comp","Compensation",4343.547809,0,240,700,15,898.391809,4.8184,715,754.011549999999,"ccu"]
["Aviation","comp","Compensation",0.102143,0,240,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},715.36709,1261.63291,"ccu"]
["Maritime","comp","Compensation",568.668771,0,240,700,15,126.00477,0.61911,715.00057,180.42471,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,700,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",164.054572,0,240,700,15,62.166303,0.8654,117.73546,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8213.436697,0,240,700,15,898.391809,4.8184,1518.14812,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.201812,0,240,700,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1977,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,700,15,126.00477,0.61911,895.42528,722.69071,"comp"]
["Primary steel","h2","DRI-EAF with H2",874.100815,0,240,700,15,475.659121,2.00321,198.90161,106.046429999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,725,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4464.007809,0,240,725,15,898.391809,4.8184,740,750.59356,"normal"]
["Aviation","comp","Compensation",0.104119,0,240,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,1263.56962,"normal"]
["Maritime","comp","Compensation",584.146534,0,240,725,15,126.00477,0.61911,740.00059,155.42469,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,725,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,725,15,62.166303,0.8654,74.54509,665.45491,"ccu"]
["CF","comp","Compensation",4464.007809,0,240,725,15,898.391809,4.8184,740,750.59356,"ccu"]
["Aviation","comp","Compensation",0.104119,0,240,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},740.37975,1263.56962,"ccu"]
["Maritime","comp","Compensation",584.146534,0,240,725,15,126.00477,0.61911,740.00059,155.42469,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,725,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",165.513572,0,240,725,15,62.166303,0.8654,119.42139,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8316.354197,0,240,725,15,898.391809,4.8184,1539.50739,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.203941,0,240,725,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2003.94937,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,725,15,126.00477,0.61911,895.42528,746.91901,"comp"]
["Primary steel","h2","DRI-EAF with H2",876.979315,0,240,725,15,475.659121,2.00321,200.33855,114.15055,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,750,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4584.467809,0,240,750,15,898.391809,4.8184,765,747.17557,"normal"]
["Aviation","comp","Compensation",0.106095,0,240,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,1265.50632,"normal"]
["Maritime","comp","Compensation",599.624296,0,240,750,15,126.00477,0.61911,765.00061,130.42467,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,750,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,750,15,62.166303,0.8654,74.54509,690.45491,"ccu"]
["CF","comp","Compensation",4584.467809,0,240,750,15,898.391809,4.8184,765,747.17557,"ccu"]
["Aviation","comp","Compensation",0.106095,0,240,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},765.39241,1265.50632,"ccu"]
["Maritime","comp","Compensation",599.624296,0,240,750,15,126.00477,0.61911,765.00061,130.42467,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,750,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",166.972572,0,240,750,15,62.166303,0.8654,121.10731,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8419.271697,0,240,750,15,898.391809,4.8184,1560.86665,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.20607,0,240,750,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2030.89873,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,750,15,126.00477,0.61911,895.42528,771.14731,"comp"]
["Primary steel","h2","DRI-EAF with H2",879.857815,0,240,750,15,475.659121,2.00321,201.7755,122.25466,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,775,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4704.927809,0,240,775,15,898.391809,4.8184,790,731.42229,"normal"]
["Aviation","comp","Compensation",0.108071,0,240,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,1267.44304,"normal"]
["Maritime","comp","Compensation",615.102058,0,240,775,15,126.00477,0.61911,790.00063,105.42465,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,775,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,775,15,62.166303,0.8654,74.54509,715.45491,"ccu"]
["CF","comp","Compensation",4704.927809,0,240,775,15,898.391809,4.8184,790,743.75758,"ccu"]
["Aviation","comp","Compensation",0.108071,0,240,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},790.40506,1267.44304,"ccu"]
["Maritime","comp","Compensation",615.102058,0,240,775,15,126.00477,0.61911,790.00063,105.42465,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,775,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",168.431572,0,240,775,15,62.166303,0.8654,122.79324,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8522.189197,0,240,775,15,898.391809,4.8184,1582.22592,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.208199,0,240,775,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2057.8481,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,775,15,126.00477,0.61911,895.42528,795.375619999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",882.736315,0,240,775,15,475.659121,2.00321,203.21244,130.35878,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,800,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4825.387809,0,240,800,15,898.391809,4.8184,815,706.42229,"normal"]
["Aviation","comp","Compensation",0.110047,0,240,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,1269.37975,"normal"]
["Maritime","comp","Compensation",630.579821,0,240,800,15,126.00477,0.61911,815.00065,80.42463,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,800,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,800,15,62.166303,0.8654,74.54509,740.45491,"ccu"]
["CF","comp","Compensation",4825.387809,0,240,800,15,898.391809,4.8184,815,740.33959,"ccu"]
["Aviation","comp","Compensation",0.110047,0,240,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},815.41772,1269.37975,"ccu"]
["Maritime","comp","Compensation",630.579821,0,240,800,15,126.00477,0.61911,815.00065,80.42463,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,800,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",169.890572,0,240,800,15,62.166303,0.8654,124.47916,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8625.106697,0,240,800,15,898.391809,4.8184,1603.58519,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.210328,0,240,800,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2084.79747,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,800,15,126.00477,0.61911,895.42528,819.603919999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",885.614815,0,240,800,15,475.659121,2.00321,204.64938,138.4629,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,825,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",4945.847809,0,240,825,15,898.391809,4.8184,840,681.42229,"normal"]
["Aviation","comp","Compensation",0.112023,0,240,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,1271.31645999999,"normal"]
["Maritime","comp","Compensation",646.057583,0,240,825,15,126.00477,0.61911,840.00067,55.42461,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,825,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,825,15,62.166303,0.8654,74.54509,765.45491,"ccu"]
["CF","comp","Compensation",4945.847809,0,240,825,15,898.391809,4.8184,840,736.921589999999,"ccu"]
["Aviation","comp","Compensation",0.112023,0,240,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},840.43038,1271.31645999999,"ccu"]
["Maritime","comp","Compensation",646.057583,0,240,825,15,126.00477,0.61911,840.00067,55.42461,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,825,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",171.349572,0,240,825,15,62.166303,0.8654,126.16509,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8728.024197,0,240,825,15,898.391809,4.8184,1624.94446,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.212457,0,240,825,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2111.74684,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,825,15,126.00477,0.61911,895.42528,843.832219999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",888.493315,0,240,825,15,475.659121,2.00321,206.08633,146.56701,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,850,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5066.307809,0,240,850,15,898.391809,4.8184,865,656.42229,"normal"]
["Aviation","comp","Compensation",0.113999,0,240,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,1273.25315999999,"normal"]
["Maritime","comp","Compensation",661.535345,0,240,850,15,126.00477,0.61911,865.00069,30.42459,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,850,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,850,15,62.166303,0.8654,74.54509,790.45491,"ccu"]
["CF","comp","Compensation",5066.307809,0,240,850,15,898.391809,4.8184,865,733.5036,"ccu"]
["Aviation","comp","Compensation",0.113999,0,240,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},865.44304,1273.25315999999,"ccu"]
["Maritime","comp","Compensation",661.535345,0,240,850,15,126.00477,0.61911,865.00069,30.42459,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,850,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",172.808572,0,240,850,15,62.166303,0.8654,127.85102,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8830.941697,0,240,850,15,898.391809,4.8184,1646.30373,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.214586,0,240,850,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2138.6962,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,850,15,126.00477,0.61911,895.42528,868.060529999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",891.371815,0,240,850,15,475.659121,2.00321,207.52327,154.67114,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,875,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5186.767809,0,240,875,15,898.391809,4.8184,890,631.42229,"normal"]
["Aviation","comp","Compensation",0.115975,0,240,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,1275.18987,"normal"]
["Maritime","comp","Compensation",677.013107,0,240,875,15,126.00477,0.61911,890.00071,5.42457000000001,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,875,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,875,15,62.166303,0.8654,74.54509,815.45491,"ccu"]
["CF","comp","Compensation",5186.767809,0,240,875,15,898.391809,4.8184,890,730.08561,"ccu"]
["Aviation","comp","Compensation",0.115975,0,240,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},890.4557,1275.18987,"ccu"]
["Maritime","comp","Compensation",677.013107,0,240,875,15,126.00477,0.61911,890.00071,5.42457000000001,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,875,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",174.267572,0,240,875,15,62.166303,0.8654,129.53694,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",8933.859197,0,240,875,15,898.391809,4.8184,1667.663,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.216715,0,240,875,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2165.64557,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,875,15,126.00477,0.61911,895.42528,892.288829999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",894.250315,0,240,875,15,475.659121,2.00321,208.96022,162.77525,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,900,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5307.227809,0,240,900,15,898.391809,4.8184,915,606.42229,"normal"]
["Aviation","comp","Compensation",0.117951,0,240,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,1277.12658999999,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,900,15,126.00477,0.61911,895.42528,19.5754499999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,900,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,900,15,62.166303,0.8654,74.54509,840.45491,"ccu"]
["CF","comp","Compensation",5307.227809,0,240,900,15,898.391809,4.8184,915,726.667619999999,"ccu"]
["Aviation","comp","Compensation",0.117951,0,240,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},915.46835,1277.12658999999,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,900,15,126.00477,0.61911,895.42528,19.5754499999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,900,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",175.726572,0,240,900,15,62.166303,0.8654,131.22287,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9036.776697,0,240,900,15,898.391809,4.8184,1689.02227,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.218844,0,240,900,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2192.59494,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,900,15,126.00477,0.61911,895.42528,916.51713,"comp"]
["Primary steel","h2","DRI-EAF with H2",897.128815,0,240,900,15,475.659121,2.00321,210.39716,170.879369999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,925,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5427.687809,0,240,925,15,898.391809,4.8184,940,581.42229,"normal"]
["Aviation","comp","Compensation",0.119927,0,240,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},940.48101,1279.06329,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,925,15,126.00477,0.61911,895.42528,44.5754699999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,925,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,925,15,62.166303,0.8654,74.54509,865.45491,"ccu"]
["CF","comp","Compensation",5427.687809,0,240,925,15,898.391809,4.8184,940,723.24963,"ccu"]
["Aviation","comp","Compensation",0.119927,0,240,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},940.48101,1279.06329,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,925,15,126.00477,0.61911,895.42528,44.5754699999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,925,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",177.185572,0,240,925,15,62.166303,0.8654,132.90879,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9139.694197,0,240,925,15,898.391809,4.8184,1710.38153,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.220973,0,240,925,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2219.5443,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,925,15,126.00477,0.61911,895.42528,940.74544,"comp"]
["Primary steel","h2","DRI-EAF with H2",900.007315,0,240,925,15,475.659121,2.00321,211.8341,178.98349,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,950,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5548.147809,0,240,950,15,898.391809,4.8184,965,556.42229,"normal"]
["Aviation","comp","Compensation",0.121903,0,240,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},965.49367,1281.01266,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,950,15,126.00477,0.61911,895.42528,69.5754899999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,950,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,950,15,62.166303,0.8654,74.54509,890.45491,"ccu"]
["CF","comp","Compensation",5548.147809,0,240,950,15,898.391809,4.8184,965,719.83164,"ccu"]
["Aviation","comp","Compensation",0.121903,0,240,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},965.49367,1281.01266,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,950,15,126.00477,0.61911,895.42528,69.5754899999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,950,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",178.644572,0,240,950,15,62.166303,0.8654,134.59472,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9242.611697,0,240,950,15,898.391809,4.8184,1731.7408,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.223103,0,240,950,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2246.50633,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,950,15,126.00477,0.61911,895.42528,964.97374,"comp"]
["Primary steel","h2","DRI-EAF with H2",902.885815,0,240,950,15,475.659121,2.00321,213.27105,187.0876,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,975,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5668.607809,0,240,975,15,898.391809,4.8184,990,531.42229,"normal"]
["Aviation","comp","Compensation",0.123879,0,240,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},990.50633,1282.94936999999,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,975,15,126.00477,0.61911,895.42528,94.57551,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,975,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,975,15,62.166303,0.8654,74.54509,915.45491,"ccu"]
["CF","comp","Compensation",5668.607809,0,240,975,15,898.391809,4.8184,990,716.41364,"ccu"]
["Aviation","comp","Compensation",0.123879,0,240,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},990.50633,1282.94936999999,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,975,15,126.00477,0.61911,895.42528,94.57551,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,975,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",180.103572,0,240,975,15,62.166303,0.8654,136.28064,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9345.529197,0,240,975,15,898.391809,4.8184,1753.10007,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.225232,0,240,975,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2273.4557,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,975,15,126.00477,0.61911,895.42528,989.20204,"comp"]
["Primary steel","h2","DRI-EAF with H2",905.764315,0,240,975,15,475.659121,2.00321,214.70799,195.19172,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1000,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5789.067809,0,240,1000,15,898.391809,4.8184,1015,506.42229,"normal"]
["Aviation","comp","Compensation",0.125855,0,240,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,1284.88607,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1000,15,126.00477,0.61911,895.42528,119.575529999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1000,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1000,15,62.166303,0.8654,74.54509,940.45491,"ccu"]
["CF","comp","Compensation",5789.067809,0,240,1000,15,898.391809,4.8184,1015,712.99565,"ccu"]
["Aviation","comp","Compensation",0.125855,0,240,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1015.51899,1284.88607,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1000,15,126.00477,0.61911,895.42528,119.575529999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1000,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",181.562572,0,240,1000,15,62.166303,0.8654,137.96657,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9448.446697,0,240,1000,15,898.391809,4.8184,1774.45934,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.227361,0,240,1000,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2300.40506,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1000,15,126.00477,0.61911,895.42528,1013.43035,"comp"]
["Primary steel","h2","DRI-EAF with H2",908.642815,0,240,1000,15,475.659121,2.00321,216.14493,203.29585,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1025,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",5909.527809,0,240,1025,15,898.391809,4.8184,1040,481.42229,"normal"]
["Aviation","comp","Compensation",0.127831,0,240,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,1286.82278,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1025,15,126.00477,0.61911,895.42528,144.575549999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1025,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1025,15,62.166303,0.8654,74.54509,965.45491,"ccu"]
["CF","comp","Compensation",5909.527809,0,240,1025,15,898.391809,4.8184,1040,709.577659999999,"ccu"]
["Aviation","comp","Compensation",0.127831,0,240,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1040.53165,1286.82278,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1025,15,126.00477,0.61911,895.42528,144.575549999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1025,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",183.021572,0,240,1025,15,62.166303,0.8654,139.65249,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9551.364197,0,240,1025,15,898.391809,4.8184,1795.81861,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.22949,0,240,1025,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2327.35443,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1025,15,126.00477,0.61911,895.42528,1037.65864999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",911.521315,0,240,1025,15,475.659121,2.00321,217.58188,211.399959999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1050,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6029.987809,0,240,1050,15,898.391809,4.8184,1065,456.42229,"normal"]
["Aviation","comp","Compensation",0.129807,0,240,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,1288.7595,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1050,15,126.00477,0.61911,895.42528,169.575569999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1050,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1050,15,62.166303,0.8654,74.54509,990.45491,"ccu"]
["CF","comp","Compensation",6029.987809,0,240,1050,15,898.391809,4.8184,1065,706.15967,"ccu"]
["Aviation","comp","Compensation",0.129807,0,240,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1065.5443,1288.7595,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1050,15,126.00477,0.61911,895.42528,169.575569999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1050,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",184.480572,0,240,1050,15,62.166303,0.8654,141.33842,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9654.281697,0,240,1050,15,898.391809,4.8184,1817.17788,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.231619,0,240,1050,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2354.3038,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1050,15,126.00477,0.61911,895.42528,1061.88695999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",914.399815,0,240,1050,15,475.659121,2.00321,219.01882,219.50408,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1075,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6150.447809,0,240,1075,15,898.391809,4.8184,1090,431.42229,"normal"]
["Aviation","comp","Compensation",0.131783,0,240,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,1290.6962,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1075,15,126.00477,0.61911,895.42528,194.57559,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1075,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1075,15,62.166303,0.8654,74.54509,1015.45491,"ccu"]
["CF","comp","Compensation",6150.447809,0,240,1075,15,898.391809,4.8184,1090,702.74168,"ccu"]
["Aviation","comp","Compensation",0.131783,0,240,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1090.55696,1290.6962,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1075,15,126.00477,0.61911,895.42528,194.57559,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1075,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",185.939572,0,240,1075,15,62.166303,0.8654,143.02435,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9757.199197,0,240,1075,15,898.391809,4.8184,1838.53715,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.233748,0,240,1075,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2381.25316,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1075,15,126.00477,0.61911,895.42528,1086.11526,"comp"]
["Primary steel","h2","DRI-EAF with H2",917.278315,0,240,1075,15,475.659121,2.00321,220.45577,227.60819,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1100,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6270.907809,0,240,1100,15,898.391809,4.8184,1115,406.42229,"normal"]
["Aviation","comp","Compensation",0.133759,0,240,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,1292.63291,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1100,15,126.00477,0.61911,895.42528,219.575609999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1100,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1100,15,62.166303,0.8654,74.54509,1040.45491,"ccu"]
["CF","comp","Compensation",6270.907809,0,240,1100,15,898.391809,4.8184,1115,699.323689999999,"ccu"]
["Aviation","comp","Compensation",0.133759,0,240,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1115.56962,1292.63291,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1100,15,126.00477,0.61911,895.42528,219.575609999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1100,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",187.398572,0,240,1100,15,62.166303,0.8654,144.71027,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9860.116697,0,240,1100,15,898.391809,4.8184,1859.89642,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.235877,0,240,1100,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2408.20253,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1100,15,126.00477,0.61911,895.42528,1110.34355999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",920.156815,0,240,1100,15,475.659121,2.00321,221.89271,235.71231,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1125,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6391.367809,0,240,1125,15,898.391809,4.8184,1140,381.42229,"normal"]
["Aviation","comp","Compensation",0.135735,0,240,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1140.58228,1294.56961999999,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1125,15,126.00477,0.61911,895.42528,244.575619999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1125,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1125,15,62.166303,0.8654,74.54509,1065.45491,"ccu"]
["CF","comp","Compensation",6391.367809,0,240,1125,15,898.391809,4.8184,1140,695.90569,"ccu"]
["Aviation","comp","Compensation",0.135735,0,240,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1140.58228,1294.56961999999,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1125,15,126.00477,0.61911,895.42528,244.575619999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1125,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",188.857572,0,240,1125,15,62.166303,0.8654,146.3962,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",9963.034197,0,240,1125,15,898.391809,4.8184,1881.25568,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.238006,0,240,1125,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2435.1519,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1125,15,126.00477,0.61911,895.42528,1134.57186999999,"comp"]
["Primary steel","h2","DRI-EAF with H2",923.035315,0,240,1125,15,475.659121,2.00321,223.32965,243.81643,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1150,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6511.827809,0,240,1150,15,898.391809,4.8184,1165,356.42229,"normal"]
["Aviation","comp","Compensation",0.137711,0,240,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1165.59494,1296.50633,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1150,15,126.00477,0.61911,895.42528,269.575649999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1150,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1150,15,62.166303,0.8654,74.54509,1090.45491,"ccu"]
["CF","comp","Compensation",6511.827809,0,240,1150,15,898.391809,4.8184,1165,692.487699999999,"ccu"]
["Aviation","comp","Compensation",0.137711,0,240,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1165.59494,1296.50633,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1150,15,126.00477,0.61911,895.42528,269.575649999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1150,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",190.316572,0,240,1150,15,62.166303,0.8654,148.08212,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",10065.951697,0,240,1150,15,898.391809,4.8184,1902.61495,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.240135,0,240,1150,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2462.10127,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1150,15,126.00477,0.61911,895.42528,1158.80017,"comp"]
["Primary steel","h2","DRI-EAF with H2",925.913815,0,240,1150,15,475.659121,2.00321,224.7666,251.920549999999,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1175,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6632.287809,0,240,1175,15,898.391809,4.8184,1190,331.42229,"normal"]
["Aviation","comp","Compensation",0.139687,0,240,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,1298.44304,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1175,15,126.00477,0.61911,895.42528,294.575659999999,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1175,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1175,15,62.166303,0.8654,74.54509,1115.45491,"ccu"]
["CF","comp","Compensation",6632.287809,0,240,1175,15,898.391809,4.8184,1190,689.06971,"ccu"]
["Aviation","comp","Compensation",0.139687,0,240,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1190.60759,1298.44304,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1175,15,126.00477,0.61911,895.42528,294.575659999999,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1175,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",191.775572,0,240,1175,15,62.166303,0.8654,149.76805,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",10168.869197,0,240,1175,15,898.391809,4.8184,1923.97422,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.242264,0,240,1175,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2489.05063,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1175,15,126.00477,0.61911,895.42528,1183.02847,"comp"]
["Primary steel","h2","DRI-EAF with H2",928.792315,0,240,1175,15,475.659121,2.00321,226.20354,260.02467,"comp"]
["Cement","ccs","CCS",122.327172,0.05836,240,1200,15,62.166303,0.8654,74.54509,71.97033,"normal"]
["CF","comp","Compensation",6752.747809,0,240,1200,15,898.391809,4.8184,1215,306.42229,"normal"]
["Aviation","comp","Compensation",0.141663,0,240,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,1300.37975,"normal"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1200,15,126.00477,0.61911,895.42528,319.57568,"normal"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1200,15,475.659121,2.00321,51.86914,21.9150899999999,"normal"]
["Cement","ccs","CCS",122.327172,0.05836,240,1200,15,62.166303,0.8654,74.54509,1140.45491,"ccu"]
["CF","comp","Compensation",6752.747809,0,240,1200,15,898.391809,4.8184,1215,685.65172,"ccu"]
["Aviation","comp","Compensation",0.141663,0,240,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},1215.62025,1300.37975,"ccu"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1200,15,126.00477,0.61911,895.42528,319.57568,"ccu"]
["Primary steel","ccs","BF-BOF + CCS",539.909427,0.76451,240,1200,15,475.659121,2.00321,51.86914,115.559289999999,"ccu"]
["Cement","ccs","CCS",193.23457200000001,0,240,1200,15,62.166303,0.8654,151.45397,1000,"comp"]
["CF","efuel","MTO using non-fossil CO2",10271.786697,0,240,1200,15,898.391809,4.8184,1945.33349,1000,"comp"]
["Aviation","efuel","Syn-kerosene (non-fossil CO2)",0.244393,0,240,1200,15,0.045629,{"v":7.9e-05,"d":"7.90E-05"},2516,1000,"comp"]
["Maritime","h2","Low-emission ammonia",680.371517,0,240,1200,15,126.00477,0.61911,895.42528,1207.25678,"comp"]
["Primary steel","h2","DRI-EAF with H2",931.670815,0,240,1200,15,475.659121,2.00321,227.64048,268.12879,"comp"]

{"sheet":"Data_Fig4","index":3,"n_rows":11,"n_cols":11,"rows_kept":11}
["Sector","Technology","Technology type","LCOP","LCOP unit","CCU attribution","CO2 emissions","CO2 emission unit","H2 cost \n(EUR/MWh)","Non-fossil CO2 cost \n(EUR/tCO2)","Fuel-switching CO2 price \n(EUR/tCO2)"]
["Cement\n","Cement production with CaL CC + CO2 storage","CCS",{"v":122.327172,"d":"122.327"},"EUR/tclinker",0.5,{"v":0.05836,"d":"0.058"},"tCO2/tclinker",50,800,{"v":74.54509,"d":"74.545"}]
[null,"Cement production with CaL CC + CO2 usage","CCU",{"v":107.372172,"d":"107.372"},"EUR/tclinker",0.5,{"v":0.55686,"d":"0.557"},"tCO2/tclinker",50,800,{"v":146.51542,"d":"146.515"}]
[null,"Cement production with CaL CC + CO2 usage","CCU",{"v":107.372172,"d":"107.372"},"EUR/tclinker",0.6,{"v":0.45716,"d":"0.457"},"tCO2/tclinker",50,800,{"v":110.73356,"d":"110.734"}]
[null,"Cement production with CaL CC + CO2 usage","CCU",{"v":107.372172,"d":"107.372"},"EUR/tclinker",0.7,{"v":0.35746,"d":"0.357"},"tCO2/tclinker",50,800,{"v":88.99844,"d":"88.998"}]
[null,"Cement production with CaL CC + CO2 usage","CCU",{"v":107.372172,"d":"107.372"},"EUR/tclinker",0.8,{"v":0.25776,"d":"0.258"},"tCO2/tclinker",50,800,{"v":74.39581,"d":"74.396"}]
["Aviation\n","Aviation using fossil kerosene + CDR compensation","CDR Compensation",{"v":0.110047,"d":"0.110"},"EUR/PAX/km",0.5,{"$f":"0*1000","v":{"v":0,"d":"0.000"}},"kgCO2/PAX/km",50,800,{"v":815.41772,"d":"815.418"}]
[null,"Aviation using syn-kerosene produced using CCU CO2 from cement ","CCU",{"v":0.064167,"d":"0.064"},"EUR/PAX/km",0.5,{"$f":"0.000043*1000","v":{"v":0.043000000000000003,"d":"0.043"}},"kgCO2/PAX/km",50,800,{"v":514.9444,"d":"514.944"}]
[null,"Aviation using syn-kerosene produced using CCU CO2 from cement ","CCU",{"v":0.064167,"d":"0.064"},"EUR/PAX/km",0.6,{"$f":"0.000051*1000","v":0.051},"kgCO2/PAX/km",50,800,{"v":662.07143,"d":"662.071"}]
[null,"Aviation using syn-kerosene produced using CCU CO2 from cement ","CCU",{"v":0.064167,"d":"0.064"},"EUR/PAX/km",0.7,{"$f":"0.00006*1000","v":{"v":0.060000000000000005,"d":"0.060"}},"kgCO2/PAX/km",50,800,{"v":975.68421,"d":"975.684"}]
[null,"Aviation using syn-kerosene produced using CCU CO2 from cement ","CCU",{"v":0.064167,"d":"0.064"},"EUR/PAX/km",0.8,{"$f":"0.000068*1000","v":0.068},"kgCO2/PAX/km",50,800,{"v":1685.27273,"d":"1685.273"}]

{"sheet":"Data_Fig5","index":4,"n_rows":8,"n_cols":17,"rows_kept":8}
["Technology","Assumption","H2 cost\n(EUR/MWh)","CO2 transport and storage cost\n(EUR/tCO2)","LCOP \n(EUR/PAX/km)","Aircraft cost and other fees \n(EUR/PAX/km)","CO2: CDR \n(EUR/PAX/km)","CO2: Methanol synthesis (total)\n(EUR/PAX/km)","CO2: Methanol synthesis (losses due to MtJ)\n(EUR/PAX/km)","Fossil jet fuel\n(EUR/PAX/km)","CO2 transport and storage\n(EUR/PAX/km)","CAPEX: MtJ\n(EUR/PAX/km)","CAPEX: Methanol synthesis\n(EUR/PAX/km)","All OPEX: MtJ\n(EUR/PAX/km)","O&M: Methanol synthesis\n(EUR/PAX/km)","Electricity: Methanol synthesis\n(EUR/PAX/km)","H2 cost: synfuel synthesis (varied in the figure)\n(EUR/PAX/km)"]
["Aviation using \nfossil kerosene","-",50,15,{"v":0.04563,"d":"0.0456"},0.0328,"-","-","-",{"v":0.01283,"d":"0.0128"},"-","-","-","-","-","-","-"]
["Aviation using fossil kerosene \n+ CDR compensation","Base CO2 transport and storage assumption\n(15EUR/tCO2)",50,15,{"v":0.07053,"d":"0.0705"},0.0328,{"v":0.02371,"d":"0.0237"},"-","-",{"v":0.01283,"d":"0.0128"},{"v":0.00119,"d":"0.0012"},"-","-","-","-","-","-"]
[null,"High CO2 transport and storage cost (50EUR/tCO2)",50,50,{"$f":"SUM(F4:Q4)","v":{"v":0.07329,"d":"0.0733"}},0.0328,{"v":0.02371,"d":"0.0237"},"-","-",{"v":0.01283,"d":"0.0128"},{"v":0.00395,"d":"0.0040"},"-","-","-","-","-","-"]
[null,"Very high CO2 transport and storage\ncost (100EUR/tCO2)",50,100,{"$f":"SUM(F5:Q5)","v":{"v":0.07724,"d":"0.0772"}},0.0328,{"v":0.02371,"d":"0.0237"},"-","-",{"v":0.01283,"d":"0.0128"},0.0079,"-","-","-","-","-","-"]
["Aviation using \ne-kerosene","Low hydrogen cost (50EUR/MWh)",50,15,{"v":0.08972,"d":"0.0897"},0.0328,"-",{"v":0.02555,"d":"0.0256"},{"$f":"H6-G3","v":{"v":1.8400000000000014E-3,"d":"0.0018"}},"-","-",{"v":0.00345,"d":"0.0035"},{"v":0.003085,"d":"0.0031"},{"v":2.33E-3,"d":"0.0023"},{"v":0.00112,"d":"0.0011"},{"v":0.000845,"d":"0.0008"},0.0205]
[null,"Medium hydrogen cost (100EUR/MWh)",100,15,{"v":0.11025,"d":"0.1103"},0.0328,"-",{"v":0.02555,"d":"0.0256"},{"$f":"H7-G3","v":{"v":1.8400000000000014E-3,"d":"0.0018"}},"-","-",{"v":0.00345,"d":"0.0035"},{"v":0.003085,"d":"0.0031"},{"v":2.33E-3,"d":"0.0023"},{"v":0.00112,"d":"0.0011"},{"v":0.000845,"d":"0.0008"},{"v":0.041069,"d":"0.0411"}]
[null,"High hydrogen cost (150EUR/MWh)",150,15,0.1308,0.0328,"-",{"v":0.02555,"d":"0.0256"},{"$f":"H8-G5","v":{"v":1.8400000000000014E-3,"d":"0.0018"}},"-","-",{"v":0.00345,"d":"0.0035"},{"v":0.003085,"d":"0.0031"},{"v":2.33E-3,"d":"0.0023"},{"v":0.00112,"d":"0.0011"},{"v":0.000845,"d":"0.0008"},0.0616]

{"sheet":"Data_Fig6","index":5,"n_rows":7,"n_cols":13,"rows_kept":7}
["Technology type","Technology detail","LCOP \n(EUR/tHRC)","CO2 emissions \n(tCO2/tHRC)","H2 cost \n(EUR/MWh)","Non-fossil CO2 cost (capture)\n(EUR/tCO2)","CO2 transport and storage cost \n(EUR/tCO2)","CO2 capture, transport and storage cost \n(EUR/tCO2)","% of CO2 emissions abated","Fuel-switching CO2 price \n(EUR/tCO2)","Cost of additional CDR to reach climate neutrality \n(EUR/tHRC)","Climate-neutral LCOP \n(EUR/tHRC)","Climate-neutral fuel-switching CO2 price \n(EUR/tCO2)"]
["BF-BOF","Depreciated (greyfield) BF-BOF plant",{"v":360.7042,"d":"360.70"},{"v":2.00321,"d":"2.00"},{"v":100,"d":"100.00"},{"v":350,"d":"350.00"},{"v":15,"d":"15.00"},{"$f":"F2+G2","v":{"v":365,"d":"365.00"}},"-","-","-","-","-"]
["BF-BOF-CCS","Greenfield CCS: Relative to greyfield BF-BOF",539.91,0.76,{"v":100,"d":"100.00"},{"v":350,"d":"350.00"},{"v":15,"d":"15.00"},{"$f":"F3+G3","v":{"v":365,"d":"365.00"}},{"$f":"(1-(D3/D2))*100","v":{"v":62.060892267910006,"d":"62.06"}},144.67,{"$f":"D3*H3","v":{"v":277.4,"d":"277.40"}},{"$f":"C3+K3","v":817.31},{"$f":"(L3-C2)/D2","v":{"v":227.93706101706755,"d":"227.94"}}]
[null,"Retrofit CCS: Relative to greyfield BF-BOF",427.24,0.76,{"v":100,"d":"100.00"},{"v":350,"d":"350.00"},{"v":15,"d":"15.00"},{"$f":"F4+G4","v":{"v":365,"d":"365.00"}},{"$f":"(1-(D4/D2))*100","v":{"v":62.060892267910006,"d":"62.06"}},53.71,{"$f":"D4*H4","v":{"v":277.4,"d":"277.40"}},{"$f":"C4+K4","v":704.64},{"$f":"(L4-C2)/D2","v":{"v":171.69233380424416,"d":"171.69"}}]
["BF-BOF + CDR","Relative to greyfield BF-BOF",1091.88,{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":350,"d":"350.00"},{"v":15,"d":"15.00"},{"v":365,"d":"365.00"},{"$f":"(1-(D5/D2))*100","v":{"v":100,"d":"100.00"}},{"v":365,"d":"365.00"},{"$f":"D5*H5","v":{"v":0,"d":"0.00"}},{"$f":"C5+K5","v":1091.88},{"$f":"(L5-C2)/D2","v":{"v":365.0020716749617,"d":"365.00"}}]
["H2-DRI-EAF","Low H2 cost, relative to greyfield BF-BOF",532.78,0.12,{"v":100,"d":"100.00"},{"v":350,"d":"350.00"},{"v":15,"d":"15.00"},{"v":365,"d":"365.00"},{"$f":"(1-(D6/D2))*100","v":{"v":94.00961456861737,"d":"94.01"}},91.14,{"$f":"D6*H6","v":{"v":43.8,"d":"43.80"}},{"$f":"C6+K6","v":{"v":576.5799999999999,"d":"576.58"}},{"$f":"(L6-C2)/D2","v":{"v":107.7649372756725,"d":"107.76"}}]
[null,"High H2 cost, relative to greyfield BF-BOF",717.78,0.12,{"v":200,"d":"200.00"},{"v":350,"d":"350.00"},{"v":15,"d":"15.00"},{"v":365,"d":"365.00"},{"$f":"(1-(D7/D2))*100","v":{"v":94.00961456861737,"d":"94.01"}},189.12,{"$f":"D7*H7","v":{"v":43.8,"d":"43.80"}},{"$f":"C7+K7","v":{"v":761.5799999999999,"d":"761.58"}},{"$f":"(L7-C2)/D2","v":{"v":200.11671267615472,"d":"200.12"}}]

{"sheet":"Data_Fig6Breakevenpoints","index":6,"n_rows":5,"n_cols":3,"rows_kept":5}
["Break-even point type","Mitigation extent","H2 break-even cost (EUR/MWh)"]
["CCS retrofit to H2-DRI-EAF","incomplete",{"v":61.8,"d":"61.80"}]
[null,"complete",171.07]
["CCS greenfield to H2-DRI-EAF","incomplete",154.64]
[null,"complete",231.98]