 .gw file Watershed HRU:167 Subbasin:7 HRU:7 Luse:FRSD Soil: Tu3 Slope: 0-9999 24/06/2016 00:00:00 ArcSWAT 2012.10_0.14
      10000.0000    | SHALLST : Initial depth of water in the shallow aquifer [mm]
      10000.0000    | DEEPST : Initial depth of water in the deep aquifer [mm]
       35.798140    | GW_DELAY : Groundwater delay [days]
        0.775838    | ALPHA_BF : Baseflow alpha factor [days]
      293.436300    | GWQMN : Threshold depth of water in the shallow aquifer required for return flow to occur [mm]
        0.085486    | GW_REVAP : Groundwater "revap" coefficient
      500.000000    | REVAPMN: Threshold depth of water in the shallow aquifer for "revap" to occur [mm]
        0.040369    | RCHRG_DP : Deep aquifer percolation fraction
          1.0000    | GWHT : Initial groundwater height [m]
          0.0030    | GW_SPYLD : Specific yield of the shallow aquifer [m3/m3]
          0.0000    | SHALLST_N : Initial concentration of nitrate in shallow aquifer [mg N/l]
          0.0000    | GWSOLP : Concentration of soluble phosphorus in groundwater contribution to streamflow from subbasin [mg P/l]
          1.2500    | HLIFE_NGW : Half-life of nitrate in the shallow aquifer [days]
          0.0000    | LAT_ORGN : Organic N in the base flow [mg/L]
          0.0000    | LAT_ORGP : Organic P in the base flow [mg/L]
        0.061035    | ALPHA_BF_D : Baseflow alpha factor for deep aquifer [days]
