Each folder contains ADCIRC input files and outfiles for each mesh (with different MinEle) using in the Super Typhoon Haiyan simulations

Input files:
   *.13 - ADCIRC format nodal attributes file (fort.13)
   *.14 - ADCIRC format mesh file (fort.14)
   *_CS.15 - ADCIRC format fort.15 control file for the cold-start run
   *_HS.15 - ADCIRC format fort.15 control file for the hot-start run
   Haiyan.22 - ADCIRC format fort.22 wind control file for the best-track Holland vortex model (same for all simulations)
   fort.rotm - ADCIRC format coordinate rotation file (same for all simulations)  

   Input data not provided [large file size and freely available elsewhere]:
   *.24 - ADCIRC format self-attraction and loading [SAL] tide (fort.24). Users can generate with OceanMesh2D "Make_f24" function using SAL data available from: "ftp://ftp.legos.obs-mip.fr/pub/FES2012-project/data/LSA/FES2014/"
   fort.221.grb2 - CFSv2 mean sea level pressure data in GRIB2 format; merge Oct+Nov from: "ftp://nomads.ncdc.noaa.gov/modeldata/cfsv2_analysis_timeseries/2013/201310/prmsl.gdas.201310.grib2" & "ftp://nomads.ncdc.noaa.gov/modeldata/cfsv2_analysis_timeseries/2013/201311/prmsl.gdas.201311.grib2"
   fort.222.grb2 - CFSv2 10-m wind velocity data in GRIB2 format; merge Oct+Nov data from: "ftp://nomads.ncdc.noaa.gov/modeldata/cfsv2_analysis_timeseries/2013/201310/wnd10m.gdas.201310.grib2" & "ftp://nomads.ncdc.noaa.gov/modeldata/cfsv2_analysis_timeseries/2013/201311/wnd10m.gdas.201311.grib2"

Output files:
   *.61.nc - NetCDF format 15-min station elevations recorded during hot-start run (fort.61.nc)
   *.62.nc - NetCDF format 15-min station velocities recorded during hot-start run (fort.62.nc)
   *.63.nc - NetCDF format 3-hourly global elevations recorded during hot-start run (fort.63.nc)
   *_maxele.63.nc - NetCDF format maximum global elevations recorded during hot-start run (maxele.63.nc)