

[Soni, 3(6): June 2016]                                                                        	           ISSN 2348 – 8034
DOI-10.5281/zenodo.54858                                                                                                               Impact Factor- 4.022

 GLOBAL JOURNAL OF ENGINEERING SCIENCE AND RESEARCHES
POWER UPGRADING OF TRANSMISSION LINE BY COMBINING AC-DC TRANSMISSION
Kiran Soni*1, Dr. Dharmendra singh2 and Dr. sushil kumar3
*1M.Tech. Scholar, Dr. C.V. Raman University,Bilaspur
2Department of electrical & electronics engineering, Dr. C.V. Raman University,Bilaspur
3Principal PCEM,Raipur, Department of electrical & electronics engineering
ABSTRACT
Long extra high voltage (EHV) ac lines cannot be loaded to their thermal limits in order to keep sufficient margin against transient instability. With the scheme proposed in this paper it is possible to load these lines very close to their thermal limits. The conductors are allowed to carry usual ac along with dc superimposed on it.
[bookmark: _GoBack]The added dc power flow does not cause any transient instability. This paper gives the feasibility of converting a double circuit ac line into composite ac–dc power transmission line to get the advantages of parallel ac–dc transmission to improve stability and damping out oscillations. Simulation and experimental studies are carried out for the coordinated control as well as independent control of ac and dc power transmissions. No alterations of conductors, insulator strings, and towers of the original line are needed. Substantial gain in the load ability of the line is obtained. Master current controller senses ac current and regulates the dc current orders for converters online such that conductor current never exceeds its thermal limit.

Keywords: Flexible ac transmission system (FACTS) ,Extra high voltage (EHV)transmission, power system computer-aided design(PSCAD),Simultaneous ac-dc power transmission.
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Neglecting ac resistance drop in the
line and transformer, the de power Par and P of

each rectifier and inverter are given by
Pa=Vels (3.5]

Pa=Vals [3.6]

Reactive powers required by the converters

are
Qdr = Pyr tan O

Bl
Qui = Pgi tan 6;

B8l

cos, = [cosa+ cos(a+)]/2 B9
cos®, = [cosy+ cos(y +,))/2 [3.10]

where X; and X are commutation
angles of inverter and rectifier, respectively, and

total active and reactive powers at the two ends are
Pot P [3,11]

‘The net current "I in any conductor is offseted from
zero. In case of a fault in the transmission system,
gate signals to all the SCRs are blocked and that to
the bypass SCRs are released to protect rectifier and
inverter bridges. The current in any conductor is no
more offseted. Circuit breakers (CBs) are then
tripped at both ends to isolate the faulty line. CBs
connected at the two ends of transmission
interrupt current at natural current zeroes, and no
special de CB is required. Now, allowing the net
current through the conductor equal to its thermal

limit Iin.
Iy = [+ (1a/3)172

B.14]

Let 17, be per-phase rms voltage of original ac
line. Let also V. be the per-phase voltage of ac
component of composite ac—de line with dc voltage
¥, superimposed on . As insulators remain
unchanged, the peak voltage in both cases should be
cqualto

Vo =205
[3.15]

Electric field produced by any conductor possesses a
de component superimpose on it a sinusoidal

varying ac component. However, the instantaneous
electric field polarity changes its sign twice in a
eyeteit (Woyf Vo)< V12 i insured. Therefore,

hioher creenace distance remmirement for insnlator

a+V2V,
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Figure: 4.2 Equivalent Circuit

Transmission loss for each line is

P = (P +Py) — (B + )

[B3.13]

Ta being the rms ac current per conductor at any

point of the line, the total rms current per conductor
becomes

1=[12 + (1/3)*1*

Power loss for each line =Py~

discs used for HVDC lines are not required. Each
conductor is 10 be insulated for Vamas, but the linc-
to-ine voltage has no dc component and

Vitmee = V6V,  .Thercfore,  conductor-to-

conductor separation distance of each line is
determined only by rated ac voltage of the line.
Allowing maximum permissible voltage offset such
that the composite voltage wave just touches zero in
cach every cyeles





image8.png
‘The total power transfer through the double circuit
Tine before conversion is as follows

P ¥ 3Viasind1/X

where *X" is the transfer reactance per phase of the
single circuit line, and O is the power angle
between the voltages at the two ends. To keep.

sufficient stability margin, J_. is generally kept low

for long lines and seldom exceeds 30°. With the
increasing length of line, the load ability of the line
is decreased. An approximate value of O-: may be
computed from the loadability curve by knowing the
values of surge impedance loading (SIL) and
transfer reactance of the line.

P = 2.M.SIL

[3.18]
‘Where M is the mul

ing factor and its magnitude

decreases with the length of line. The value of M can
be obtained from the loadability curve.
‘The total power transfer through the composite line

Proal = Pac + Pye

A surge diverter connected between the zig-zag
neutral and the ground protects the converter bridge
against any over voltage.

4 Simulation:-
4.1 Simulink Model Using AC
‘Transmission:-

Figure: 4.1 Simulink model using
AC Transmission

4.2 Simulink Model Using AC -DC
Transmission:-
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‘The power angle 3. between the ac voltages at the
two ends of the composite line may be increased to a
high value due to fast controllability of de component
of power. For a constant value of total power, P._
‘may be modulated by fast control of the
current  controller of dc power converters.
Approximate value of ac current per phase per
cireuit of the double circuit line may be computed as
I, =V(sin8/2)/X

[3.20]

‘The rectifier de current order is adjusted

online as

L =3 15~ Iy

Preliminary ~qualitative ~analysis suggests ~that
commonly used_techniques in HVDC/AC system
may be adopted for the purpose of the design of
protective ~ scheme, filter, and  instrumentation
network to be used with the composite line for
simultaneous ac~dc power flow. In case of a fault in
the transmission system, gate signals to all the SCRs
are blocked and that to the bypass SCRs are released
to protect rectifier and inverter bridges. CBs are then
tripped at both ends to isolate the complete system.

Figure: 6.2 Simulink model using combined
AC - DC Transmission.

6 Results:-
6.1 AC Configuration only
The laudability of Moose (commercial name),
ACSR, twin bundle conductor, 400-kV, 50-Hz, 430-
K single circuit line has been computed.
The parameters of the line are
2=0.6054+j0.66172

Zka/phickt
Y=j6.67594* 105 /kmv/ph/ckt

Current carrying capacity of each sub conductor

9kA

o= 18 KAkt

SIL = S1IMWrckt.
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Using (17)20), the computed power at receiving
end and conductor current is

Plowl =11242 MW

Tphieka = 0.803 kKA.

5 Results:-

5.1Both AC-DC Configuratios

5.2 Simulated Results

6 Conclusion and Future Scope

6.1 Conclusion

The feasibility to convert ac transmission line to a
composite ac—dc line has been demonstrated. For the
particular system ~studied, there is substantial
increase (about 83.45%) in the loadability of the
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line. The line is loaded to its thermal limit with the.
superimposed de current. The de power flow does
not impose any stability problem. The advantage of
parallel ac—de transmission is obtained. De current
regulator may modulate ac power flow. There is no
need for any modification in the size of conductors,
insulator strings, and towers structure of the original
line. The optimum values of ac and de voliage
components of the converted composite line are 1/2
and 1/V2 times the ac voltage before conversion,

respectively.

6.2 Future Scope

In this paper, it is shown that by injecting DC power
in AC power transmission lines, we can improve the
transmission_capacity of the line by 2 to 4 times
without altering the physical equipment. This work
can be extended for analyzing the effect of faults on
this type of transmission. This work is done on
double circuit AC transmission lines but it can be
extended to other types of transmission methods.
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1 Introduction: - In recent years,
environmental, right-of-way, and cost concems have
delayed the construction of a new transmission line,
while demand of electric power has shown steady
but geographically uneven growth. The power is
often available at locations ot close to the growing
load centers but at remote locations. These locations
are largely determined by regulatory policies,
environmental  acceptability, and the cost of
available energy. The wheeling of this available
energy through existing long ac lines to load centers
has a certain upper limit due to stability
considerations. Thus, these lines are not loaded to
their thermal limit to keep sufficient margin against

The present situation demands the review of
traditional power transmission theory and practice,
on the basis of new concepts that allow full
wilization of existing transmission facilities without
decreasing system availability and security. The

flexible ac transmission system (FACTS) concepts,
based on applying state-of-the-art power electronic
technology to existing ac transmission system,
improve stability to achieve power transmission
close to its thermal limit.

The basic proof justifying the simultaneous ac—dc
power transmission is explained in an IEEE paper
“Simultaneous acdc power transmission,” by K. P.
Basu and B. H. Khan. In the above reference,
simultaneous ac—dc power transmission was first
proposed through a single circuit ac transmission
Tine. In these proposals Mono-polar dc transmission
with ground as return path was used. There were
certain limitations due to use of ground as return
path. Moreover, the instantaneous value of each
conductor voltage with respect to ground becomes
higher by the amount of the dc voltage, and more
discs are to be added in each insulator string to
withstand this  increased voltage. However, there
was no change in the conductor separation distance
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2 Problem Definition:-

The main object of my paper is to show that by
superimposing DC in AC transmission, the capacity
of the transmission line can be increased by nearly
70 % of that if only AC is transmitted. In our
existing transmission system, long extra high voltage
(EHV) ac lines cannot be loaded to their thermal
imits in order to keep sufficient margin against
transient instability. With the scheme proposed in
this paper, it is possible to load these lines very close
to their thermal limits. The conductors are allowed
to carry usual ac along with de superimposed on it.

3 Proposed System (Simultaneous AC-DC
Power Transmission):-

With the scheme proposed in this thesis, it is
possible to load the transmission lines very close to
their thermal limits. The conductors are allowed to
carry usual ac along with de superimposed on it. The
added de power flow does not cause any transient
instability. This thesis gives the feasibility of
converting a double circuit ac line into composite
ac~dc power transmission line to get the advantages
of parallel ac~dc transmission to_improve stability
and damping out oscillations. No- alterations  of
conductors, insulator strings, and towers of the
original line are needed. Substantial gain in the load
ability of the line is obtained. In this thesis, the
feasibility study of conversion of a single circuit ac
line to composite ac—dc line without altering the

transformer due to dc current. Two fluxes produced
by the e current (I / 3) flowing through each of a
‘winding in each limb of the core of a zig-zag

transformer are equal in magnitude and opposite in
direction. So the net dc flux at any instant of time
becomes zero in each limb of the core. Thus, the d
saturation of the core is avoided. A high value of
reactor X is used to reduce harmonics in dc current
In the absence of zero sequence and third harmonics
or its multiple harmonic voltages, under normal
operating conditions, the ac current flow through
each transmission line will be restricted between the
zigzag connected windings and the three
conductors of the transmission line. Even the
presence of these components of voltages may only
be able to produce negligible current through the
ground
high
of Xq.

Figure: 4.1 Basic scheme for composite ac—dc
transmission.

Assuming the usual constant current control of rectifier

and constant extinction angle control of inverter as

‘mentioned later, the equivalent circuit of the scheme
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original line conductors and tower structures has
been presented.

3.1 Introduction:-

Fig. 1 depicts the basic scheme for simultaneous ac—
de power flow through a double circuit ac
transmission line. The de power is obtained through
line commutated 12-pulse rectifier bridge used in
conventional HVDC and injected to the neutral point
of the zigzag connected secondary of sending end
transformer and is reconverted to ac again by the
conventional line commutated 12-pulse ~ bridge
inverter at the receiving end. The inverter bridge is
again connected to the neutral of zig-zag connected
‘winding of the receiving end transformer.

The double circuit ac transmission line carriers both
three-phase ac and dc power. Each conductor of
each line carries one third of the total dc current
along with ac current. Resistance being equal in all
the three phases of secondary winding of zig-zag
transformer as well as the three conductors of the
line, the de current is equally divided among all the
three phases.

The three conductors of the second line provide
retun path for the dc current. Zig-zag connected
winding is used at both ends to avoid saturation of

under normal steady-state operating condition is given
in Fig. 2. The dotted lines in the figure show the path
of ac return current only. The second transmission line
carries the return de current, and cach conductor of the
line carries (1a/ 3)

along with the ac current per phase and Voo and Vaio
are the maximum values of rectifier and inverter

side de voltages and are equal to 31/ Z times
converter ac input line-to-line voltage. R, L and C
are the line parameters per phase of each line. Rer
and Re; are commutating resistances, and, a, ¥ are
firing and extinction angles of rectifier and inverter,
respectively.

32 Proof with Equations:-

Neglecting the resistive drops in the line conductors
and transformer windings due to dc current,
expressions for ac voltage and current, and for
active and reactive powers in terms of A, B, C, and
D parameters of each line may be written as

Es=AEg + Blg

B
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